- Top
- Network Connection
- Using the cloud service
- Remote operation of the streaming

# Remote operation of the streaming

## Procedure for using

Perform the basic setting of the camera.

For details, refer to “Basic setting of the camera”.

Create an SD card with a profile set in following procedure using a computer.

- Login to the cloud service, and download the profile.

- Decompress the downloaded file.

- Save the decompressed PRIVATE folder in the root directory of the SD card.

Set the camera as follows to enable the profile.

- Select the [NETWORK] menu → [STREAMING] → [STREAMING PROTOCOL] → [RTMP(S)] or [SRT CLIENT].

- Insert an SD card, and load the profile into the camera with one of the following methods.

  (The card slot to load and save can be set with the [OTHERS] menu → [FILE] → [SLOT FOR LOAD/SAVE])

  - Select the [NETWORK] menu → [STREAMING] → [CONNECTION INFO.] → [MEMORY], and load the content of the SD card with the [NETWORK] menu → [STREAMING] → [LOAD (SD CARD)].

  - Select the [NETWORK] menu → [STREAMING] → [CONNECTION INFO.] → [SD CARD].

- Confirm that the [NETWORK] menu → [STREAMING] → [DATA TYPE] → [CLOUD] is displayed.

Perform various operation for streaming in the cloud service.

## Streaming from the cloud service

- For details, refer to the cloud service documents.

- When the profile for the cloud service different from the contents upload function is set, the profile setting for the contents upload will be prioritized.

- It is necessary to set the camera to be able to use the streaming function. For details, refer to “Settings for the streaming function”.

- The items that can be specified from the cloud service are items set in the destination setting (Setting of the destination). Set other items in the menu of the camera.

- This function cannot be used if anything other than [RTMP(S)] or [SRT CLIENT] is selected in the streaming protocol.

- Remote operation of the streaming is not possible when the thumbnail screen is displayed on the camera.

- Once the operation to start streaming or setting of the destination URL is performed from the cloud service, the destination URL is recorded inside the camera. Streaming to the same destination can be performed with the operation from the camera after that. (Setting for each protocol and starting the streaming)

- The recorded streaming information can be confirmed in the [NETWORK] menu → [INFORMATION] → [STATUS]. (Except [PASSPHRASE])

- The recorded destination URL information is also cleared when the destination information is cleared.

  For details on clearing the destination information, refer to “Clearing the destination information”.

Top of the page