- Top
- Network Connection
- Streaming function
- Setting for each protocol and starting the streaming

# Setting for each protocol and starting the streaming

## RTMP(S)

Select the [NETWORK] menu → [STREAMING] → [STREAMING PROTOCOL] → [RTMP(S)].

Set the destination.

For details of setting the streaming destination, refer to “Setting of the destination”.

Select the [NETWORK] menu → [STREAMING] → [START] → [ON].

If the camera is connected to the transmission destination through a network, the camera starts the transmission of streaming video.

- To stop the transmission of the streaming image, select the [NETWORK] menu → [STREAMING] → [START] → [OFF].

NOTE

- The H.265 format cannot be selected in the 4K streaming.

- [START] menu cannot be selected when the streaming cannot be started due to reasons such as the network is not connected, etc.

- Starting/stopping of the streaming from the camera can be assigned to the USER button. (Assigning function to the USER buttons)

  Streaming cannot be started by pressing the USER button or touching the USER button icon when the menu or the thumbnail screen is displayed.

- IPv6 cannot be used for RTMP(S).

- For settings such as URL, refer to the manual for each streaming service.

- Streaming may not be possible depending on the operating condition of the streaming service.

- Setting of [RECEIVER URL] is not possible when [DATA TYPE] is set to [CLOUD]. Set this after performing the operation for [CLEAR (MEMORY)] once.

## RTSP

Start the streaming with an operation of the application software or device at the receiving side (referred to as “receiving side” hereinafter).

Select the [NETWORK] menu → [STREAMING] → [STREAMING PROTOCOL] → [RTSP].

Set the standby port with the [NETWORK] menu → [STREAMING] → [RTSP SETTING] → [PORT] on the camera if required.

Specify the IP address and the path of the camera as following on the receiving side, and start streaming.

rtsp://(IP address):(Port number)/stream

NOTE

- Stop the streaming with the operation in the receiving side.

- For details about the operations to start streaming from the application software, refer to the manual for the receiving side.

- Streaming cannot be started while the thumbnail screen is displayed.

#### Streaming with multicast

One streaming can be distributed to multiple receivers via supported router, etc., when the multicast function is used.

Select the [NETWORK] menu → [STREAMING] → [RTSP SETTING] → [MULTICAST] → [ENABLE].

Select the [NETWORK] menu → [STREAMING], and specify [MULTICAST ADDRESS] and [MULTICAST PORT].

- Set [MULTICAST ADDRESS] within following range.

  IPv4: 224.0.1.0 to 239.255.255.254

  IPv6: Multicast address starting with FF

- Set [MULTICAST PORT] within the range of 1024 to 50000.

Specify the address of the camera and start streaming with the application software.

NOTE

- Depending on the specification of the device receiving streaming and the connected router, quality of the video image may not be preserved. When streaming by multicast, contact the administrator of the network being used and prepare appropriate communication environment.

- Disable the LAN card not to be used when receiving the multicast image to be displayed on a computer with multiple LAN cards installed.

- Range of streaming can be adjusted with the [NETWORK] menu → [STREAMING] → [RTSP SETTING] → [TTL/HOP LIMIT]. For details, contact the network administrator.

## SRT client

Select the [NETWORK] menu → [STREAMING] → [STREAMING PROTOCOL] → [SRT CLIENT].

Set the destination.

For details of setting the streaming destination, refer to “Setting of the destination”.

Select the [NETWORK] menu → [STREAMING] → [START] → [ON].

If the camera is connected to the transmission destination through a network, the camera starts the transmission of streaming video.

- To stop the transmission of the streaming image, select the [NETWORK] menu → [STREAMING] → [START] → [OFF].

NOTE

- Streaming in 23.98 Hz is not possible with SRT.

- [START] menu cannot be selected when the streaming cannot be started due to reasons such as the network is not connected, etc.

- Starting/stopping of the streaming from the camera can be assigned to the USER button. (Assigning function to the USER buttons)

- Streaming cannot be started by pressing the USER button or touching the USER button icon when the menu or the thumbnail screen is displayed.

- For settings such as URL, refer to the manual for each streaming service.

- Streaming may not be possible depending on the operating condition of the streaming service.

- Range of streaming can be adjusted with the [NETWORK] menu → [STREAMING] → [SRT SETTING] → [TTL/HOP LIMIT]. For details, contact the network administrator.

- Depending on the environment, the delay time can be adjusted with the [NETWORK] menu → [STREAMING] → [SRT SETTING] → [LATENCY]. For details, contact the network administrator.

- Settings of [DEST URL], [STREAM ID], [ENCRYPTION], and [PASSPHRASE] are not possible when [DATA TYPE] is set to [CLOUD]. Set this after performing the operation for [CLEAR (MEMORY)] once.

## SRT listener

Start the streaming with an operation of the application software or device at the receiving side (referred to as “receiving side” hereinafter).

Select the [NETWORK] menu → [STREAMING] → [STREAMING PROTOCOL] → [SRT LISTENER].

Set following items with the [NETWORK] menu → [STREAMING] → [SRT SETTING] on the camera.

- Set the standby port with [PORT].

- If the streaming data is to be encrypted, select the encryption method in [ENCRYPTION], and enter the passphrase in [PASSPHRASE].

Specify the IP address and the stream ID of the camera as following on the receiving side, and start streaming.

srt://(IP address):(Port number)

- The stream ID is fixed to following value in the SRT listener mode.

  #!::m=publish,r=PanasonicStream

NOTE

- Streaming in 23.98 Hz is not possible with SRT.

- Stop the streaming with the operation in the receiving side.

- For details about the operations to start streaming from the application software, refer to the manual for each application software.

- Range of streaming can be adjusted with the [NETWORK] menu → [STREAMING] → [SRT SETTING] → [TTL/HOP LIMIT]. For details, contact the network administrator.

- Depending on the environment, the delay time can be adjusted with the [NETWORK] menu → [STREAMING] → [SRT SETTING] → [LATENCY]. For details, contact the network administrator.

- Streaming cannot be started while the thumbnail screen is displayed.

Top of the page