- Top
- Network Connection
- Using the cloud service
- Contents upload

# Contents upload

## Procedure for using

Perform the network settings with the camera. (Network settings)

Create an SD card with a profile set in following procedure using a computer.

- Login to the cloud service, and download the profile.

- Decompress the downloaded file.

- Save the decompressed PRIVATE folder in the root directory of the SD card.

Set the camera as follows to enable the profile.

- Select the [NETWORK] menu → [UPLOAD] → [ENABLE/DISABLE] → [ENABLE].

- Insert an SD card, and load the profile into the camera with one of the following methods.

  (The card slot to load and save can be set with the [OTHERS] menu → [FILE] → [SLOT FOR LOAD/SAVE])

  - Select the [NETWORK] menu → [UPLOAD] → [CONNECTION INFO.] → [MEMORY], and load the content of the SD card with the [NETWORK] menu → [UPLOAD] → [LOAD (SD CARD)].

  - Select the [NETWORK] menu → [UPLOAD] → [CONNECTION INFO.] → [SD CARD].

- Confirm that the [NETWORK] menu → [UPLOAD] → [DATA TYPE] → [CLOUD] is displayed.

Perform the setting and operation necessary for uploading with the cloud service.

## Uploading of the contents with the cloud service

- To use the contents upload function, linking to a cloud service is necessary.

- For details, refer to the cloud service documents.

- The camera supports FTP/SFTP protocol. Set it on the cloud service depending on the server to be used.

- The recording data in AVCHD is not supported for uploading.

- Setting only the clips with shot marks added (Shot mark recording function) as upload target is possible by the operation in the cloud service for the P2 recording data.

- Operation to only upload the proxy data (Recording the proxy data) can be set by the operation in the cloud service for the P2 recording data. When only the proxy data is uploaded and then upload the main material recording data by selecting them in the cloud service, set to the [RECORDING] menu → [REC META DATA] → [CARD SERIAL] → [ON] before recording. Also, use the SD cards that do not have duplicated card serial number.

- Operations such as deleting the clip or formatting the memory card while uploading a clip may result in failure of the operation or incomplete upload.

- Connection may not be possible depending on the encryption algorithm setting of the server when SFTP is used.

- The upload operation may be paused when the SD card access load is high due to the recording operation, etc.

Top of the page