- Top
- Overview
- What you can do with this camera
- Linking to external devices

# Linking to external devices

## Connecting to monitor

A monitor can be connected to output images.

HDMI cable

Monitor

BNC cable (<SDI OUT> terminal)

Video/audio cable* (<AV OUT> terminal)

Use a commercial video/audio cable (4-pole mini plug).

Check the wire specifications of the 4-pole mini plug.

Audio (Left audio: White)

Video (Yellow)

Ground

Audio (Right audio: Red)

- Use the double shielded cable supporting 4K/60P as the HDMI cable (optional). It is also recommended to use the Panasonic 4K/60P compatible HDMI cable.

- For the BNC cable (optional) connected to the <SDI OUT> terminal, prepare a double-shielded cable equivalent to 5C-FB.

## Card reader mode

Data (files) for performing nonlinear editing on a computer are transferred.

- The camera supports USB 3.1 (GEN1).

Memory card*1

USB type C cable*2

Computer

Memory cards are optionally available. They are not supplied with the camera.

A USB type C cable is not supplied with the camera.

Use a commercial USB-type C cable. Use of a cable no longer than 1.5 m is recommended.

The camera does not offer a bus-powered function.

Data from a computer cannot be written to the memory card inserted into the camera.

## Connecting to the remote camera controller (AW-RP150G)

Connects the remote camera controller AW-RP150G (optional) via LAN cable to control some functions remotely.

LAN cable

AW-RP150G

Top of the page