- Top
- Operation
- Menu settings
- [NETWORK] menu

# [NETWORK] menu

Sets the setting regarding the network function.

## [DEVICE SEL]

Select the device that connects external equipment (computer, etc.) to the camera.

The camera may restart when the setting is changed.

[LAN] | Connects via a wired LAN.
[WLAN] | Connects via a wireless LAN.
[USB TETHERING] | Connects to iPhone/iPad or Android devices using USB tethering.
[OFF] | Does not connect.

(Factory setting: [OFF])

## [NETWORK FUNC]

Selects the network function of the camera.

[STREAMING] | Enables the streaming function.
[STREAMING(4K)] | Enables the 4K streaming function.
[NDI|HX] | Enables the NDI|HX function.
[OFF] | Does not use the network function.

(Factory setting: [OFF])

NOTE

- Recording and thumbnail display are not possible when [STREAMING(4K)] or [NDI|HX] is selected.

## [IP REMOTE]

Perform settings for the IP remote. (Remote operation by the remote camera controller or CX ROP app)

### [ENABLE/DISABLE]

Sets whether to enable the IP remote function.

[ENABLE] | Enables the IP remote function.
[ENABLE(HOLD)] | Enables the IP remote function. Connection will be preserved even if the remote controller switches cameras.
[DISABLE] | Disables the IP remote function.

(Factory setting: [DISABLE])

NOTE

- Set to [ENABLE(HOLD)] when using the protocol for a remote camera.

- Port 80 is used for the protocol for a remote camera.

- The whole menu will close immediately after setting this to [DISABLE] while connected to a remote controller.

### [CX ROP PORT]

Specifies the standby port number to connect to CX ROP.

(Factory setting: [49152])

### [REMOTE CONTROL PORT]

Specifies the standby port number to connect to a remote controller.

(Factory setting: [49154])

### [USER ACCOUNT]

Registers a new user account to use for authentication in the network function of the camera. (Maximum of ten accounts)

The character limit of the user account name and password is as follows.

- User account name: Maximum of 31 characters

- Password: Between 8 to 15 characters

### [ACCOUNT LIST]

Displays a list of registered users.

In addition, select the user and press the <SET> button to display the confirmation screen to delete a registered user.

## [UPLOAD]

Sets the upload function that will transfer the clip recorded on the camera to a server device on the network by linking with a cloud service.

### [ENABLE/DISABLE]

Enables/disables the upload function from the camera to the server device.

[ENABLE] | Enables the upload function.
[DISABLE] | Disables the upload function.

(Factory setting: [DISABLE])

### [CONNECTION INFO.]

Select where the connection information for upload is to be acquired from.

[MEMORY] | Uses the information saved in the camera memory. It is necessary to load the connection information from the file in the SD card with [LOAD (SD CARD)] in [UPLOAD] and save in the camera memory in advance.
[SD CARD] | Uses the information from the file in the SD card.

(Factory setting: [MEMORY])

### [DATA TYPE]

Displays the type of the connection information data. (Cannot be changed)

[--] | There is no connection information.
[CLOUD] | This is a connection information for the cloud service to upload.

(Factory setting: [--])

### [LOAD (SD CARD)]

The connection information file is loaded from the SD card and saved in the camera memory when [CONNECTION INFO.] is set to [MEMORY].

### [CLEAR (MEMORY)]

Clears the connection information for upload saved in the camera memory.

## [STREAMING]

Performs the settings for the streaming function.

### [STREAMING PROTOCOL]

Specifies the streaming protocol.

[RTMP(S)] | Streams in RTMP or RTMPS.
[RTSP] | Streams in RTSP.
[SRT CLIENT] | Streams in client mode of SRT.
[SRT LISTENER] | Streams in listener mode of SRT.

(Factory setting: [RTSP])

### [STREAMING FORMAT]

Specifies the streaming format.

The item that can be selected varies depending on the condition. For details, refer to “Settings when using the streaming function” or “Settings when using the 4K streaming function”.

### [CONNECTION INFO.]

Selects the internal memory of the camera or the memory card as the reference location for the transfer destination when starting a stream with the operation of the camera.

The items that can be set are as follows.

- [MEMORY], [SD CARD]

(Factory setting: [MEMORY])

### [DATA TYPE]

Displays the type of the setting data. (Cannot be changed)

[GENERAL] | General streaming settings
[CLOUD] | Cloud service setting

### [RTMP(S) RECEIVER URL]

Enter the destination URL in following format.

- rtmp://(server URL):(port number)/(path)/(stream key)

- rtmps://(server URL):(port number)/(path)/(stream key)

### [RTSP SETTING]

[PORT] | Sets the port number to wait for the RTSP command. Factory setting: [554]
[MULTICAST] | Enables/disables the multicast function. Factory setting: [DISABLE]
[MULTICAST ADDRESS] | Sets the address when using the streaming with the multicast. Factory setting: [239.192.0.20]
[MULTICAST PORT] | Sets the port number when using the streaming with the multicast. Factory setting: [37004]
[TTL/HOP LIMIT] | Sets the TTL/HOP limit value for the multicast. (1-254) Factory setting: [16]

### [SRT SETTING]

[DEST URL] | Specifies the destination URL for the client mode.
[STREAM ID] | Sets the stream ID for the client mode.
[PORT] | Specifies the standby port for the listener mode. Factory setting: [2020]
[TTL/HOP LIMIT] | Sets the TTL/HOP limit value. (1-255) Factory setting: [254]
[LATENCY] | Sets the time (ms) from when the packet is sent and to be played back at the receiving side. Factory setting: [120]
[ENCRYPTION] | Sets the encryption of the IP image to be streamed. [OFF]: IP image is streamed without encryption. [AES128]: It is encrypted with AES 128 bit. [AES192]: It is encrypted with AES 192 bit. [AES256]: It is encrypted with AES 256 bit. Factory setting: [OFF] NOTE [--] is displayed when [DATA TYPE] is set to [CLOUD].
[PASSPHRASE] | Sets the phrase to decrypt the encrypted IP image.

### [LOAD (SD CARD)]

Loads the settings file from the memory card and reflects in the menu when [CONNECTION INFO.] is set to [MEMORY].

The items that can be selected are as follows.

- [YES], [NO]

### [SAVE (SD CARD)]

Encrypts and saves the information of the destination URL to the memory card.

The items that can be selected are as follows.

- [YES], [NO]

### [CLEAR (MEMORY)]

Clears the contents of the streaming setting set in the menu item.

The setting information of the streaming destination that was received from the cloud service is also cleared.

The items that can be selected are as follows.

- [YES], [NO]

### [START]

Starts streaming.

The items that can be set are as follows.

- [ON], [OFF]

(Factory setting: [OFF])

## [NDI|HX]

Performs settings related to NDI|HX.

### [ACTIVATION]

Displays whether the NDI|HX function is enabled. (Cannot be changed)

[--] | Not active.
[NDI|HX] | Active.

### [STREAMING FORMAT]

Specifies the streaming format.

The items that can be set are as follows.

- When [FILE FORMAT] is set to [P2] or [MOV], and [REC FORMAT] is set to 1080/50p

  - [1920×1080-50fps 24M], [1920×1080-50fps 16M], [1920×1080-50fps 10M], [1920×1080-50fps 8M], [1280×720-50fps 14M], [1280×720-50fps 10M], [1280×720-50fps 6M]

    (Factory setting: [1920×1080-50fps 10M])

- When [FILE FORMAT] is set to [P2] or [MOV], and [REC FORMAT] is set to 1080/59.94p

  - [1920×1080-60fps 24M], [1920×1080-60fps 16M], [1920×1080-60fps 10M], [1920×1080-60fps 8M], [1280×720-60fps 14M], [1280×720-60fps 10M], [1280×720-60fps 6M]

    (Factory setting: [1920×1080-60fps 10M])

- When [FILE FORMAT] is set to [P2] or [MOV], and [REC FORMAT] is set to 1080/50i or 1080/25p

  - [1920×1080-25fps 14M], [1920×1080-25fps 10M], [1920×1080-25fps 6M], [1280×720-25fps 8M], [1280×720-25fps 4M], [1280×720-25fps 2M]

    (Factory setting: [1920×1080-25fps 10M])

- When [FILE FORMAT] is set to [P2] or [MOV], and [REC FORMAT] is set to 1080/59.94i or 1080/29.97p

  - [1920×1080-30fps 14M], [1920×1080-30fps 10M], [1920×1080-30fps 6M], [1280×720-30fps 8M], [1280×720-30fps 4M], [1280×720-30fps 2M]

    (Factory setting: [1920×1080-30fps 10M])

- When [FILE FORMAT] is set to [P2], and [REC FORMAT] is set to 720/50p

  - [1280×720-50fps 14M], [1280×720-50fps 10M], [1280×720-50fps 6M]

    (Factory setting: [1280×720-50fps 10M])

- When [FILE FORMAT] is set to [P2], and [REC FORMAT] is set to 720/59.94p

  - [1280×720-60fps 14M], [1280×720-60fps 10M], [1280×720-60fps 6M]

    (Factory setting: [1280×720-60fps 10M])

NOTE

- Cannot be set when [FILE FORMAT] is set to [AVCHD] or [REC FORMAT] is set to UHD or 1080/23.98p.

### [MULTICAST]

Enables/disables the multicast function.

(Factory setting: [DISABLE])

### [MULTICAST ADDRESS]

Sets the address when using the streaming with the multicast.

(Factory setting: [239.192.0.20])

### [MULTICAST PORT]

Sets the port number when using the streaming with the multicast.

(Factory setting: [37004])

### [TTL/HOP LIMIT]

Sets the TTL/HOP limit value for the multicast. (1-254)

(Factory setting: [16])

### [CLEAR ACTIVATION]

Clears the activation license information that is saved.

The items that can be selected are as follows.

- [YES], [NO]

## [LAN PROPERTY]

Performs settings related to the wired LAN.

### [MAC ADDRESS]

Displays the MAC address for the wired LAN of the camera. (Cannot be changed)

### [IPv4 SETTING]

[DHCP] | Sets whether to use the automatic acquisition through DHCP or to use the DHCP server function of the camera. [OFF]: Does not use DHCP. [CLIENT]: Acquires automatically with DHCP. The address from 192.168.0.10 through 192.168.0.255 is automatically assigned when the IP address cannot be acquired automatically within one minute. [SERVER]: Enables the DHCP server function of the camera. Factory setting: [OFF]
[IP ADDRESS] | Sets the IP address. Factory setting: [192.168.0.1] NOTE Cannot be set when [LAN PROPERTY] → [IPv4 SETTING] → [DHCP] → [CLIENT] is selected.
[SUBNET MASK] | Sets the subnet mask. Factory setting: [255.255.255.0] NOTE Cannot be set when [LAN PROPERTY] → [IPv4 SETTING] → [DHCP] → [CLIENT] is selected.
[DEFAULT GATEWAY] | Sets the default gateway. Factory setting: [192.168.0.254] NOTE Cannot be set when [LAN PROPERTY] → [IPv4 SETTING] → [DHCP] → [CLIENT] is selected.
[PRIMARY DNS] | Sets the primary DNS server. Factory setting: [0.0.0.0]
[SECONDARY DNS] | Sets the secondary DNS server. Factory setting: [0.0.0.0]

### [IPv6 SETTING]

[ENABLE/DISABLE] | Sets whether to use IPv6. [ENABLE]: Uses IPv6. [DISABLE]: Does not use IPv6. Factory setting: [DISABLE]
[DHCP] | Sets whether to use automatic acquisition via DHCP. [OFF]: Does not use DHCP. [CLIENT]: Performs automatic acquisition through DHCP. Factory setting: [OFF]
[IP ADDRESS] | Sets the IP address. Factory setting: [::]
[PREFIX LENGTH] | Sets the prefix length of the subnet. Factory setting: [64]
[DEFAULT GATEWAY] | Sets the default gateway. Factory setting: [::]
[PRIMARY DNS] | Sets the primary DNS server. Factory setting: [::]
[SECONDARY DNS] | Sets the secondary DNS server. Factory setting: [::]

## [WLAN PROPERTY]

Performs settings related to the wireless LAN.

### [MAC ADDRESS]

Displays the wireless LAN MAC address of the camera. (Cannot be changed)

### [TYPE]

Sets the connection method to the wireless LAN.

[DIRECT] | It can connect directly without using a wireless access point to a device equipped with wireless LAN such as a tablet terminal.
[INFRA(SELECT)] | Connects to the wireless access point. The access point is selected from the list.
[INFRA(MANUAL)] | Connects to the wireless access point. Wireless access point is entered manually.

(Factory setting: [DIRECT])

### [SSID]

Enters or displays the network name of the camera (SSID). (32 characters or less)

(Factory setting: [AG-CX350E])

### [BAND]

Switches between two communication methods ([2.4GHz] or [5GHz]) when the [NETWORK] menu → [WLAN PROPERTY] → [TYPE] → [DIRECT] is selected.

The items that can be set are as follows.

- [2.4GHz], [5GHz]

(Factory setting: [2.4GHz])

### [CHANNEL(2.4GHz)]

Sets the channel to be used when connected to the wireless LAN with following items set.

- The [NETWORK] menu → [WLAN PROPERTY] → [TYPE] → [DIRECT]

- The [NETWORK] menu → [WLAN PROPERTY] → [BAND] → [2.4GHz]

The items that can be set are as follows.

- [AUTO], [CH1], [CH6], [CH11]

(Factory setting: [AUTO])

### [CHANNEL(5GHz)]

Sets the channel to be used when connected to the wireless LAN with following items set.

- The [NETWORK] menu → [WLAN PROPERTY] → [TYPE] → [DIRECT]

- The [NETWORK] menu → [WLAN PROPERTY] → [BAND] → [5GHz]

The items that can be set are as follows.

- [AUTO], [CH36], [CH40], [CH44], [CH48], [CH100], [CH104], [CH108], [CH112], [CH116], [CH132], [CH136], [CH140], [CH149], [CH153], [CH157], [CH161], [CH165]

(Factory setting: [AUTO])

NOTE

- Some items may not be able to select depending on the used wireless module.

### [ENCRYPTION]

Sets the encryption method when the [NETWORK] menu → [WLAN PROPERTY] → [TYPE] → [INFRA(SELECT)]/[INFRA(MANUAL)] is selected.

The items that can be set are as follows.

- [WPA-TKIP], [WPA-AES], [WPA2-TKIP], [WPA2-AES], [NONE]

(Factory setting: [WPA2-AES])

NOTE

- The setting is fixed to [WPA2-AES] when the [NETWORK] menu → [WLAN PROPERTY] → [TYPE] → [DIRECT] is set.

### [ENCRYPT KEY]

Sets the encryption key. Set the key using a string of 8 to 63 characters or a hexadecimal number with 64 digits.

(Factory setting: [01234567890123456789abcdef])

### [IPv4 SETTING]

[DHCP] | Sets whether to use the automatic acquisition through DHCP or to use the DHCP server function of the camera. [OFF]: Does not use DHCP. [CLIENT]: Performs automatic acquisition through DHCP if connecting by setting [WLAN PROPERTY] → [TYPE] → [INFRA(SELECT)]/[INFRA(MANUAL)]. [SERVER]: Enables the DHCP server function of the camera when connecting by setting [WLAN PROPERTY] → [TYPE] → [DIRECT]. Factory setting: [OFF]
[IP ADDRESS] | Sets the IP address. Factory setting: [192.168.0.1] NOTE Cannot be set when [WLAN PROPERTY] → [IPv4 SETTING] → [DHCP] → [CLIENT] is selected.
[SUBNET MASK] | Sets the subnet mask. Factory setting: [255.255.255.0] NOTE Cannot be set when [WLAN PROPERTY] → [IPv4 SETTING] → [DHCP] → [CLIENT] is selected.
[DEFAULT GATEWAY] | Sets the default gateway. Factory setting: [192.168.0.254] NOTE If you do not use default gateway, set to [0.0.0.0]. Cannot be set when [WLAN PROPERTY] → [IPv4 SETTING] → [DHCP] → [CLIENT] is selected. Disables the setting for the default gateway when [WLAN PROPERTY] → [TYPE] → [DIRECT] is selected.
[PRIMARY DNS] | Sets the primary DNS server. Factory setting: [0.0.0.0] NOTE Disables the setting for the primary DNS server when [WLAN PROPERTY] → [TYPE] → [DIRECT] is selected.
[SECONDARY DNS] | Sets the secondary DNS server. Factory setting: [0.0.0.0] NOTE Disables the setting for the secondary DNS server when [WLAN PROPERTY] → [TYPE] → [DIRECT] is selected.

## [INFORMATION]

### [STATUS]

Displays the status of the network function.

## [UTILITY]

Performs the various operations related to the network function.

### [NETWORK INITIALIZE]

Restores the network setting status to the factory settings.

### [NET CHECKER]

Checks network connection status.

### [EASY IP SETTING]

Sets the time to accept EASY IP Setup Software.

The items that can be set are as follows.

- [DISABLE], [20 MIN.], [UNLIMITED]

(Factory setting: [DISABLE])

NOTE

- This is fixed to [UNLIMITED] when [USB TETHERING] is selected in [DEVICE SEL].

- This is fixed to [UNLIMITED] when [NDI|HX] is selected in [NETWORK FUNC].

### [EASY IP CAMERA TITLE]

Configure the individual device names to display in EASY IP Setup Software. (15 characters or less)

The camera title set here is also displayed as the individual device name in the NDI|HX compatible switcher and the CX ROP app.

(Factory setting: [AG-CX350])

Top of the page