- Top
- Notes
- Recording function that cannot be used simultaneously

# Recording function that cannot be used simultaneously

Depending on the recording function that is set, there are recording functions that cannot be used simultaneously.

- Meaning of the symbols used in the table are as follows.

  - ✓: Can be used simultaneously.

  - —: Cannot be used simultaneously.

| Recording function that is set
--- | ---
Recording function to additionally set | Pre-recording*1*2 | Relay recording | Simultaneous recording | Interval recording*3*4*6*7*9
Pre-recording*1*2 |  | ✓ | ✓ | —
Relay recording | ✓ |  | — | —
Simultaneous recording | ✓ | — |  | ✓
Interval recording*3*4*6*7*9 | — | — | ✓ |
Background recording*1*3*8*9*10 | — | — | — | —
VFR/Super slow recording*3*4*5*10 | — | — | — | —
Proxy recording*11*12*13 | ✓ | ✓ | — | —

| Recording function that is set
--- | ---
Recording function to additionally set | Background recording*1*3*8*9*10 | VFR/Super slow recording*3*4*5*10 | Proxy recording*11*12*13
Pre-recording*1*2 | — | — | ✓
Relay recording | — | — | ✓
Simultaneous recording | — | — | —
Interval recording*3*4*6*7*9 | — | — | —
Background recording*1*3*8*9*10 |  | — | —
VFR/Super slow recording*3*4*5*10 | — |  | —
Proxy recording*11*12*13 | — | — |

Time code is fixed to free run.

The pre-recording is canceled once when three hours has passed without starting the recording.

Cannot set simultaneously in the following cases.

- When recording in AVCHD format

Time code is fixed to recording run.

This cannot be set when the frequency of the [SYSTEM] menu → [REC FORMAT] is set to 50.00i/59.94i.

The time code is fixed to [NDF].

The [VIDEO OUT/LCD/VF] menu → [SDI OUT] → [SDI REC REMOTE] and the [VIDEO OUT/LCD/VF] menu → [HDMI OUT] → [HDMI REC REMOTE] will not operate.

This will not operate when anything other than 1080p/1080i is selected in the [SYSTEM] menu → [REC FORMAT].

Cannot set simultaneously when recording format is set to AVC-Intra 200/AVC-Intra 100/AVC-Intra 50.

Cannot set simultaneously in the following cases.

- When recording in P2 format

Cannot be set when the file format is MOV or AVCHD.

Cannot be set when the recording format is AVC-G12.

Cannot be simultaneously used with recording of the time stamp and the streaming on network.

Top of the page