- Top
- Output and Screen Display
- Screen status display
- Checking and displaying shooting status

# Checking and displaying shooting status

The screen to check the setting and status of the camera can be displayed.

Press the <DISP/MODE CHK> button while the camera image screen is displayed to hide most of the items.

Press the <DISP/MODE CHK> button for one second or more while the camera image screen is displayed to display the STATUS screen of the mode check and check the shooting status.

For details about each item that can be displayed in the mode check, refer to “Mode check display”.

The following table indicates each item to display/hide in each screen.

- “✓” indicates displaying and “—” indicates hiding.

- You can select to display or hide each item in the [VIDEO OUT/LCD/VF] menu → [INDICATOR].

No | Item | Camera image screen | When the <DISP/MODE CHK> button is pressed | STATUS | Playback screen
--- | --- | --- | --- | --- | ---
1 | Time code | ✓ | ✓ | ✓ | ✓
2 | Frame rate | ✓ | — | ✓ | —
3 | <AUTO/MANUAL> switch | ✓ | — | ✓ | —
4 | Message display area for stop of cooling fan | ✓ | ✓ | ✓ | ✓
5 | Tally lamp command status via the network | ✓ | — | ✓ | —
6 | Recording status (card slot 1) | ✓ | ✓*1 | ✓ | —
7 | Remaining recording capacity and status of the memory card (card slot 1) | ✓ | —*2 | ✓ | —
8 | Bonding Device Status | ✓ | — | ✓ | —
9 | External equipment recording operation control status (<SDI OUT>/<HDMI> terminal) | ✓ | — | ✓ | —
10 | Recording status (card slot 2) | ✓ | ✓*1 | ✓ | —
11 | Remaining recording capacity and status of the memory card (card slot 2) | ✓ | —*2 | ✓ | —
12 | Special recording function | ✓ | — | ✓ | —
13 | Two-slot function | ✓ | — | ✓ | —
14 | Flash band compensation function | ✓ | — | ✓ | —
15 | Streaming status | ✓ | — | ✓ | —
16 | High dynamic range recording function/dynamic range stretcher function/V-Log recording function | ✓ | — | ✓ | —
17 | Connection status of the wired LAN, wireless LAN, and USB tethering | ✓ | — | ✓ | —
18 | Power status | ✓ | —*2 | ✓ | ✓
19 | Audio level meter | ✓ | — | ✓ | ✓
20 | Luminance of Y GET | ✓ | ✓ | ✓ | —
21 | Gain | ✓ | — | ✓ | —
22 | ND filter | ✓ | — | ✓ | —
23 | Date and time information | ✓ | — | ✓ | —
24 | Shutter speed | ✓ | — | ✓ | —
25 | Auto iris control status | ✓ | — | ✓ | —
26 | High-sensitivity mode | ✓ | — | ✓ | —
27 | Iris | ✓ | — | ✓ | —
28 | Zoom | ✓ | — | ✓ | —
29 | System resolution/system frequency | ✓ | — | ✓ | —
30 | Recording format | ✓ | — | ✓ | —
31 | Clip name | ✓ | — | ✓ | ✓*3
32 | Recommended ND filter | ✓ | ✓ | ✓ | —
33 | Message display area | ✓ | ✓ | ✓ | ✓
34 | Level gauge | ✓ | ✓ | ✓ | —
35 | Main face frame (orange)/face detection frame (white) | ✓ | ✓ | ✓ | —
36 | Tracking frame (green) | ✓ | ✓ | ✓ | —
37 | Error display of auto white balance | — | — | ✓ | —
38 | Error display of auto black balance | — | — | ✓ | —
39 | Remote control status in an IP connection | — | — | ✓ | —
40 | Multi manual function | ✓ | —*4 | ✓ | —
41 | Color temperature | ✓ | — | ✓ | —
42 | Optical image stabilizer function | ✓ | — | ✓ | —
43 | Scene file name | ✓ | — | ✓ | —
44 | Upload status display | ✓ | — | ✓ | —
45 | Area mode function/auto focus area width adjustment function/face detection/tracking AE&AF function | ✓ | — | ✓ | —
46 | Waveform monitor | ✓ | ✓ | — | —
47 | IR recording | ✓ | — | ✓ | —
48 | Digital zoom | ✓ | — | ✓ | —
49 | Focus | ✓ | — | ✓ | —
50 | Audio monitor volume adjustment | ✓ | ✓ | ✓ | ✓

This is not displayed in the status where is not displayed.

Displays when the remaining recording capacity of the memory card or remaining battery level gets low.

The display position differs in the playback screen. Refer to Screen display during playback.

Displays when the multidial, </> button, <> button, or <SET> button is pressed. The display is cleared approximately three seconds after the operation.

Top of the page