- Top
- Network Connection
- Streaming function
- Entering the setting using the setting tool

# Entering the setting using the setting tool

## Installing software

Download and expand the P2 Network Setting software for Windows from the following website.

https://pro-av.panasonic.net/

## Creating the SD card for setting using the P2 Network Setting software

The SD card created with this software can be used to load into the camera menu or as the reference destination when the [NETWORK] menu → [STREAMING] → [CONNECTION INFO.] → [SD CARD] is selected.

## RTMP(S) setting procedure

Fig. 1

Fig. 2

Start the P2 Network Setting software. (Fig. 1)

Select the Streaming tab → RTMP tab.

Enter the destination URL in STREAM DESTINATION URL.

Click Export and select the destination in the drive selection dialog (Fig. 2), and then click OK.

- This cannot be saved to anything other than a removable drive.

## SRT client setting procedure

Fig. 1

Fig. 2

Start the P2 Network Setting software. (Fig. 1)

Select the Streaming tab → SRT tab.

Enter the destination URL in STREAM DEST. URL.

Enter the stream ID in STREAM ID.

To encrypt, select Encryption and enter the PASS PHRASE.

Click Export and select the destination in the drive selection dialog (Fig. 2), and then click OK.

- This cannot be saved to anything other than a removable drive.

NOTE

- When setting the SRT client, use the P2 Network Setting software Ver.3.00 or later.

Top of the page