- Top
- Network Connection
- Network settings
- USB tethering setting

# USB tethering setting

These are the settings when using USB tethering.

Select the [NETWORK] menu → [DEVICE SEL] → [USB TETHERING].

Enable USB tethering (Internet sharing) in the setting screen for network on the USB tethering device connected to the camera.

Allow access of the connected device if an alert to confirm permission is displayed on the USB tethering device. Connection will not be complete until permission is given.

Close the menu or return to the level of the [NETWORK] menu.

Check the network connection.

Once connected, is displayed on the screen of the camera.

NOTE

- The startup time after turning on the power may be longer due to starting of the network.

- When changing the settings of [DEVICE SEL], the changes will not be reflected until the camera is restarted. Also, the setting screen termination may take some time due to the restart of the network service after the setting is changed.

- For details of the network status, confirm by selecting the [NETWORK] menu → [INFORMATION] → [STATUS].

- IP address, DNS, and other setting cannot be set manually when connecting to the network by USB tethering.

- The icon to show that the connection is complete indicates that communication between this camera and the USB tethering device has been established. When the USB tethering device cannot connect to the Internet, the camera cannot connect to the Internet even if the icon that indicates connection is complete is displayed on the camera’s screen.

- When a USB tethering device is connected to the camera using a USB cable, the USB tethering device will be charged. If a battery is used to supply power to the camera, continuous recordable time will be shortened.

Top of the page