- Top
- Network Connection
- Streaming function

# Streaming function

You can perform streaming of audio and video currently shot with the camera over a network (wired LAN, wireless LAN, and USB tethering).

Streaming can be performed using the camera, an application software of a device connected via a network, or a server that is capable of receiving streaming video sent from the camera.

There are two ways to start streaming: streaming from an application software and streaming from the camera. This section describes the camera's network connection method for each method.

NOTE

- The streaming function cannot be simultaneously used with the recording function of the proxy data.

- Streaming stops when performing operations such as displaying the thumbnail screen or playing back clips on the camera.

- Streaming may stop when the date/time is set while streaming.

- If there is a setting that disables VFR and other streaming functions in the scene file, streaming will end due to the scene file changing.

- Take caution as streaming image may unintentionally be released depending on the system environment to stream on and setting of the service and system used.

Basic setting of the camera
Setting for each protocol and starting the streaming
Management of setting information
Entering the setting using the setting tool
Top of the page