- Top
- Specification
- Specifications
- Digital audio

# Digital audio

Recording audio signal | P2: 48 kHz/24 bits, 4ch (excluding AVC-LongG12) 48 kHz/16 bits, 4ch (AVC-Intra 100/AVC-Intra 50/AVC-LongG12) 24 bits/16 bits of AVC-Intra 100/AVC-Intra 50 can be selected by menu Proxy: 48 kHz/16-bit, 2ch MOV: 48 kHz/24-bit, 4ch AVCHD: 48 kHz/16-bit, 2ch
Audio recording format | P2: LPCM Proxy: AAC MOV: LPCM AVCHD: Dolby AudioTM
Headroom | 12 dB/18 dB/20 dB switchable menu

Top of the page