- Top
- Preparation
- Assigning function to the USER buttons
- Functions assigned to USER buttons

# Functions assigned to USER buttons

Item | Description
--- | ---
[INHIBIT] | Disables assignment of functions.
[AWB] | Assigns the automatic white balance function.
[DRS] | Assigns the dynamic range stretcher function.
[FBC] | Enables/disables the flash band compensation function.
[ONE PUSH AF] | Assigns the one-push auto focus function. The same is performed when the <PUSH AUTO> button is pressed.
[S.GAIN] | Assigns the function that increases the gain to 24 dB or more.
[AREA] | Assigns the area function.
[AF AREA] | Assigns the area auto focus function.
[FACE DETECT] | Enables/disables the face detection AE&AF function.
[ATW] | Enables/disables the auto tracking white balance functions.
[ATW LOCK] | Fixes the value of the white balance. Press the USER button again or touch the USER button icon to resume the operation of the auto tracking white balance. Enable when the auto tracking white balance is operating.
[SPOTLIGHT] | Enables/disables the auto iris control function for the spot light.
[BACKLIGHT] | Enables/disables the auto iris control function for the backlight compensation.
[A.IRIS LEVEL] | Enables/disables the auto iris level function.
[IRIS] | Assigns the function that switches the auto iris and manual iris.
[Y GET] | Assigns the function that displays the luminance level of the frame area displayed near the center.
[FOCUS MACRO] | Switches the focus macro setting.
[O.I.S.] | Enables/disables the optical image stabilizer function.
[O.I.S. MODE] | Switches the operation mode of the optical image stabilizer function. Toggles [NORMAL], [PAN/TILT], and [STABLE] in order each time the USER button is pressed or the USER button icon is touched.
[i.ZOOM] | Assigns the zoom function to minimize image distortion.
[D.ZOOM] | Enables/disables the digital zoom. Zooms in on the field angle by 2x, 5x, and 10x vertically and horizontally each time the USER button is pressed or the USER button icon is touched.
[IR REC] | Enables/disables the IR recording.
[FAST ZOOM] | Speeds up the zoom speed when the zoom lever is pushed in all the way.
[ADAPTIVE MATRIX] | Enables/disables the function to control the linear matrix in accordance with the shooting condition.
[BARS] | Toggles whether to turn the color bars on or off. The color bar is interlocked with the test tone (1 kHz).
[PRE REC] | Enables/disables the pre-recording.
[VFR] | Enables/disables the variable frame rate recording function.
[SUPER SLOW] | Enables/disables the super slow recording function.
[REC CHECK] | Automatically plays back the last approximately three seconds of the previously shot clip.
[BACKGR PAUSE] | Assigns the function that stops the background recording of card slot 2. Press and hold the USER button to which [BACKGR PAUSE] is assigned for approximately five seconds or touch and hold the USER button icon for approximately five seconds and release to stop background recording.
[DEL LAST CLIP] | Deletes the clip last shot.
[SLOT SEL] | Selects the card slot with the memory card for recording inserted. Or, switches the card slot for the clip to display in the thumbnail screen.
[AUDIO CH1 LEVEL] | Switches the recording level adjustment method for audio channel 1 between automatic and manual.
[AUDIO CH2 LEVEL] | Switches the recording level adjustment method for audio channel 2 between automatic and manual.
[EXPAND] | Enables/disables the enlarged display function (focus assist function).
[PEAKING] | Enables/disables the peaking display (focus assist function).
[WFM] | Switches the display of the waveform monitor. The waveform display is selected in the [VIDEO OUT/LCD/VF] menu → [EI ASSIST] → [WFM MODE].
[ZEBRA] | Displays/hides zebra patterns.
[LEVEL GAUGE] | Displays/hides the level gauge.
[LEVEL GAUGE SET] | Sets the current horizontal and vertical direction as the reference value of the level gauge.
[LCD/VF HDR] | Toggles output images from the LCD monitor and view finder between the high dynamic range and standard dynamic range.
[LCD/VF V-Log] | Toggles output images from the LCD monitor and view finder between V-Log and V-709.
[VF ON/OFF] | Forces images to be displayed in the viewfinder.
[LCD/VF DETAIL] | Adjusts the intensity for the contour of the video in the viewfinder or LCD monitor to make it easier to focus.
[AUDIO MON SEL] | Switches the audio channel 1/2 and the audio channel 3/4 for the output audio (headphone terminal, built-in speaker, <AV OUT> terminal) while the USER button is pressed or the USER button icon is touched. Also, the display of the audio level meter is switched between the audio channel 1/2 and the audio channel 3/4.
[AUDIO OUT] | Switches the audio channel and the format to output from the <AV OUT> terminal, the headphone terminal, and the built-in speaker. When the [AUDIO] menu → [OUTPUT SETTINGS] → [AUDIO OUT] is set to [CH1]/[CH2]/[CH1/2 STEREO]/[CH1/2 MIX], toggles [CH1], [CH2], [CH1/2 STEREO], and [CH1/2 MIX] in order each time the USER button is pressed or the USER button icon is touched. When the [AUDIO] menu → [OUTPUT SETTINGS] → [AUDIO OUT] is set to [CH3]/[CH4]/[CH3/4 STEREO]/[CH3/4 MIX], toggles [CH3], [CH4], [CH3/4 STEREO], and [CH3/4 MIX] in order each time the USER button is pressed or the USER button icon is touched.
[MENU] | Switches display/hide of the menu.
[LOAD SETUP FILE] | Selects the setup file saved on the memory card to load on the camera.
[LCD BACKLIGHT] | Switches the brightness of the LCD monitor. Toggles [0], [1], [2], and [−1] in order each time the USER button is pressed or the USER button icon is touched.
[CARD READER MODE] | Enables/disables the card reader mode function (USB mass storage function). Release the connection to enable the card reader mode when connected to a network via a wireless LAN. (The camera returns to the original setting when the card reader mode is disabled.)
[STREAMING START] | Starts/stops streaming from the camera. Streaming starts only during RTMP streaming.
[SHOT MARK] | Assigns the shot mark function.

NOTE

- Following functions will be disabled when the camera is set to < > (standby) and then turned on again.

  [FBC], [S.GAIN], [AREA], [AF AREA], [ATW LOCK], [SPOTLIGHT], [BACKLIGHT], [Y GET], [D.ZOOM], [FAST ZOOM], [BARS], [EXPAND], [PEAKING], [WFM], [VF ON/OFF], [AUDIO MON SEL], [CARD READER MODE], [STREAMING START]

Top of the page