- Top
- Description of Parts
- Camera
- Left side

# Left side

1. Eye cup

2. Eyepiece

   Do not leave the eyepiece pointed toward the sun. Doing so might damage the devices inside.

3. <USB2.0 HOST> terminal

   Can connect to wireless LAN when the wireless module (optional) compatible to camera is mounted.

   When connecting the camera to iPhone/iPad or Android device using USB cable, connection to the network is possible using USB tethering.

4. REC button (on the grip)

   Starts or stops the recording.

   Used for direct shooting in thumbnail mode.

5. Power switch

   Switches between power on/standby.

   To turn on, set the power switch to < > (ON). To set to standby, set the power switch to < > (standby).

6. Microphone cable clamp

   Fixes the external microphone cable.

7. Microphone holder mounting section

   Mounts the supplied microphone holder with microphone holder screws.

8. Tripod holes

   Attaches the tripod. (bottom)

   - Mounting hole size

     - 1/4-20 UNC (screw length 5.5 mm or shorter)

     - 3/8-16 UNC (screw length 5.5 mm or shorter)

9. Accessory mounting holes

   Attaches accessories.

   The weight of the accessory should be no more than 2 kg including the mounting fixture.

   - Mounting hole size

     - Mounting screw size: M3

     - Mounting hole depth: 6 mm

     - Mounting hole pitch: 25 mm

Top of the page