- Top
- Specification
- Specifications
- Memory card recorder

# Memory card recorder

Recording media | Card slot × 2 SDHC memory card SDXC memory card : UHS-I/UHS-II, UHS Speed Class 3 compatible, video Speed Class V90 compatible microP2 card (A series/B series) It is possible to record to SDXC memory cards in P2 format. Card that the operation is confirmed by Panasonic is recommended.
Recording slot | microP2/SDXC UHS-II card slot × 2
Number of recording pixels | 3840×2160 (UHD), 1920×1080 (FHD), 1280×720 (HD), 720×576 (SD), 720×480 (SD) (AVC-Intra 50: 1440×1080, 960×720)
Recording file format | P2 (P2 MXF compatible), MOV (HEVC), MOV (AVC), AVCHD Proxy: MOV (AVC)
System frequency | 59.94 Hz/50.00 Hz
Recording format | P2 AVC-Intra 422, AVC-LongG50, AVC-LongG25, AVC-LongG12 AVC-Intra 200, AVC-Intra 100, AVC-Intra 50 Proxy: 4:2:0 (8-bit) AVC-Proxy G6 MOV: 4:2:0 (10-bit) HEVC LongGOP 200M/HEVC LongGOP 150M/HEVC LongGOP 100M MOV: 4:2:0 (8-bit) 420LongGOP 150M/420LongGOP 100M MOV: 4:2:2 (10-bit) 422LongGOP 150M/422LongGOP 100M/422LongGOP 50M 422ALL-I 400M/422ALL-I 200M/422ALL-I 100M AVCHD: PS/PH/HA/PM/SA
Recording video signal | 3840×2160/59.94p, 50p, 29.97p, 25p, 23.98p 1920×1080/59.94p, 50p, 29.97p, 25p, 23.98p, 59.94i, 50i 1280×720/59.94p, 50p 1440×1080/59.94i, 50i (AVC-Intra 50) 960×720/59.94p, 50p (AVC-Intra 50) 720×480/59.94i, 720×576/50i
Recording and playback time | When using a 64 GB microP2 card 1080-59.94p, 50p/AVC-Intra 422, 1080-59.94i, 50i/AVC-Intra 200 Approx. 32 minutes 1080-59.94i, 50i/AVC-Intra 100 Approx. 1 hour 4 minutes 1080-59.94i, 50i/AVC-LongG50 Approx. 2 hours 8 minutes 1080-59.94i, 50i/AVC-LongG25 Approx. 4 hours 16 minutes When using a 64 GB SDXC memory card 3840×2160/420LongGOP 150M/59.94p, 50p Approx. 55 minutes 1920×1080/420LongGOP 100M/59.94p, 50p Approx. 1 hour 20 minutes 1920×1080/420LongGOP 50M/29.97p, 25p, 23.98p Approx. 2 hours 40 minutes
Two-slot function | Simultaneous recording, relay recording, background recording
Special recording | Pre-recording, interval recording, time stamp recording, proxy recording

Top of the page