- Top
- Network Connection
- Streaming function
- Management of setting information

# Management of setting information

## Setting of the destination

Information regarding the destination can be set or referenced.

### Setting the destination with the camera menu

#### For RTMP(S)

Select the [NETWORK] menu → [STREAMING] → [CONNECTION INFO.] → [MEMORY].

Enter the destination URL in the [NETWORK] menu → [STREAMING] → [RTMP(S) RECEIVER URL].

- Enter the destination URL in following format.

  - rtmp://(server URL):(port number)/(path)/(stream key)

  - rtmps://(server URL):(port number)/(path)/(stream key)

NOTE

- In general, a parameter for the stream key is required for URL, but the stream key may be contained as a part of the path depending on the service. For details, refer to the manual for each streaming service.

- When using RTMPS, only the streaming format equal to or less than 25 Mbps can be selected.

#### For SRT client

Select the [NETWORK] menu → [STREAMING] → [CONNECTION INFO.] → [MEMORY].

Set following items with the [NETWORK] menu → [STREAMING] → [SRT SETTING].

- Enter the destination URL in [DEST URL] in following format.

  srt://(server URL):(Port number)/(Path)

- Enter the stream ID in [STREAM ID].

- If the streaming data is to be encrypted, select the encryption method in [ENCRYPTION], and enter the passphrase in [PASSPHRASE].

NOTE

- In general, a parameter for the stream ID is required for URL, but the stream ID may be contained as a part of the path depending on the service. For details, refer to the manual for each streaming service.

- When the SRT encryption is enabled, only the streaming format equal to or less than 25 Mbps can be selected.

- When the passphrase is blank, communication is performed without encryption even if [ENCRYPTION] is set to anything other than [OFF].

### Referencing destination from the memory card

Insert the memory card with the destination information saved.

- The card slot to perform loading and saving can be set in the [OTHERS] menu → [FILE] → [SLOT FOR LOAD/SAVE].

Select the [NETWORK] menu → [STREAMING] → [CONNECTION INFO.] → [SD CARD].

NOTE

- If the setting information in the memory card is not information for the selected protocol or the cloud, it will be treated as no setting.

## Saving the destination information on the memory card

Insert a memory card formatted with the camera.

- The card slot to perform loading and saving can be set in the [OTHERS] menu → [FILE] → [SLOT FOR LOAD/SAVE].

Select the [NETWORK] menu → [STREAMING] → [SAVE (SD CARD)].

Select [YES] when the confirmation message is displayed.

NOTE

- Only items saved are the ones that are used in the destination setting.

- The name of the file in the memory card to save the destination information cannot be changed.

- The file with the destination information saved on the memory card is encrypted.

- Only the selected protocol settings are saved if the protocol is RTMP(S) or SRT client.

- Save is not possible when [DATA TYPE] is set to [CLOUD].

- Save is not possible when the starting character string of the [RECEIVER URL] or the [DEST URL] (“rtmp://”, etc.) is not set correctly.

## Loading destination information from the memory card

Insert the memory card with the destination information saved.

- The card slot to perform loading and saving can be set in the [OTHERS] menu → [FILE] → [SLOT FOR LOAD/SAVE].

Select the [NETWORK] menu → [STREAMING] → [LOAD (SD CARD)].

Select [YES] when the confirmation message is displayed.

NOTE

- The name of the file to load destination information saved on the memory card cannot be selected.

- The setting information that can be loaded (referenced) by the camera is as follows.

  - Information saved with the camera

  - Setting file created with the P2 Network Setting software (Entering the setting using the setting tool)

  - Profile downloaded from the cloud service (Using the cloud service)

## Clearing the destination information

Select the [NETWORK] menu → [STREAMING] → [CLEAR (MEMORY)].

- The setting information for the cloud service is also cleared.

- The destination URL information set in the cloud service is also cleared. (Using the cloud service)

## Stopping streaming of video

Stop the streaming in following procedure if the streaming was started with the operation of the camera.

Select the [NETWORK] menu → [STREAMING] → [START] → [OFF].

- If a start/stop of streaming is assigned to a USER button, streaming can also be stopped with the USER button.

Top of the page