- Top
- Network Connection
- Streaming function
- Starting streaming with an operation on the camera

# Starting streaming with an operation on the camera

Select the [NETWORK] menu → [STREAMING] → [START TRIGGER] → [CAMERA].

Set the destination.

For details of setting the destination, refer to “Setting the destination for streaming in the menu of the camera” or “Referring to the memory card for the destination of streaming”.

Select the [NETWORK] menu → [STREAMING] → [START] → [ON].

If the camera is connected to the transmission destination through a network, the camera starts the transmission of streaming video.

NOTE

- [START] menu cannot be selected when the streaming cannot be started due to reasons such as the network is not connected, etc.

- Starting/stopping of the streaming from the camera can be assigned to the USER button. (Assigning function to the USER buttons)

  Streaming cannot be started by pressing the USER button or touching the USER button icon when the menu or the thumbnail screen is displayed.

- Only RTMP and RTMPS are available when starting streaming with an operation from the camera. In such case, IPv6 cannot be used.

- For settings such as URL, refer to the manual for each streaming service.

- Streaming may not be possible depending on the operating condition of the streaming service.

- Streaming stops when performing operations such as displaying the thumbnail screen or playing back clips on the camera.

- Streaming may stop when the date/time is set while streaming.

## Setting the destination for streaming in the menu of the camera

Select the [NETWORK] menu → [STREAMING] → [CONNECTION INFO.] → [MEMORY].

Enter the destination URL in the [NETWORK] menu → [STREAMING] → [RECEIVER URL].

- Enter the destination URL in following format.

  - rtmp://(server URL):(port number)/(path)/(stream key)

  - rtmps://(server URL):(port number)/(path)/(stream key)

NOTE

- In general, a parameter for the stream key is required with RTMP, but the stream key may be contained as a part of the path depending on the service. For details, refer to the manual for each streaming service.

- Setting of [RECEIVER URL] is not possible when [DATA TYPE] is set to [P2CAST]. Set this after performing the operation for [CLEAR (MEMORY)] once.

## Referring to the memory card for the destination of streaming

Insert the memory card with the destination information saved into card slot 1.

Select the [NETWORK] menu → [STREAMING] → [CONNECTION INFO.] → [SD CARD].

## Management of destination information

Destination information can be saved and loaded between the menu of the camera and the memory card.

#### Saving the destination information on the memory card

Insert a memory card formatted with the camera into card slot 1.

Select the [NETWORK] menu → [STREAMING] → [SAVE (SD CARD)].

Select [YES] when the confirmation message is displayed.

NOTE

- The name of the file in the memory card to save the destination information cannot be changed.

- The file with the destination information saved on the memory card is encrypted.

- Save is not possible when [DATA TYPE] is set to [P2CAST].

- Save is not possible when the starting character string of the [RECEIVER URL] (“rtmp://”, etc.) is not set correctly.

#### Loading destination information from the memory card

Insert the memory card with the destination information saved into card slot 1.

Select the [NETWORK] menu → [STREAMING] → [LOAD (SD CARD)].

Select [YES] when the confirmation message is displayed.

NOTE

- The name of the file to load destination information saved on the memory card cannot be selected.

- The setting information that can be loaded (referenced) by the camera is as follows.

  - Information saved with the camera

  - Setting file created with the P2 Network Setting software (Entering the setting using the setting tool)

  - Profile downloaded with P2 Cast (Using P2 Cast)

## Clearing the destination information

Select the [NETWORK] menu → [STREAMING] → [CLEAR (MEMORY)].

- The setting information for P2 Cast is also cleared.

- The destination URL information set in P2 Cast is also cleared. (Using P2 Cast)

- The setting related to multicast is not cleared.

## Stopping streaming of video

Select the [NETWORK] menu → [STREAMING] → [START] → [OFF].

Top of the page