- Top
- Specification
- Specifications
- Audio input/output

# Audio input/output

Built-in microphone | Supports stereo microphone
<AUDIO INPUT 1>/<AUDIO INPUT 2> terminal | XLR×2, 3-pin Input high impedance, <LINE>/<MIC>/<+48V> (switch selection) <LINE>: 4 dBu/0 dBu (menu selection) <MIC>: −40 dBu/−50 dBu/−60 dBu (menu selection)
<SDI OUT> terminal | LPCM 4ch
<HDMI> terminal | LPCM 2ch/4ch (selected by menu)
<AV OUT> terminal | 3.5 mm diameter mini jack Output level: 600 Ω, 316 mV
Headphone terminal | 3.5 mm diameter stereo mini jack × 1
Speaker | 20 mm diameter, round ×1

Top of the page