- Top
- Operation
- Menu settings
- [SCENE FILE] menu

# [SCENE FILE] menu

Sets the detailed image quality adjustment of the camera video.

This menu cannot be set when the thumbnail screen is displayed.

For the factory settings, refer to “Factory setting value of the scene file”.

## [FILE SELECT]

Selects the scene file (1 to 6).

The items that can be set are as follows.

- [F1:], [F2:FLUO.], [F3:SPARK], [F4:B.STR], [F5:CINE], [F6:HLG]

## [NAME EDIT]

Edits the name of the scene file selected in the scene file menu. (Maximum eight characters)

## [LOAD/SAVE/INITIALIZE]

Loads/saves/initializes the setting values of the scene file assigned to the current scene file number (any one from 1 to 6).

[LOAD] | Selects and loads the scene file saved in the internal memory of the camera.
[SAVE] | Saves the current setting value as a scene file in the internal memory of the camera by specifying the title and the file number.
[INITIALIZE] | Initializes the selected scene files (1 to 6) to the factory settings.

## [VFR]

Sets permission/prohibition of the variable frame rate (VFR).

The items that can be set are as follows.

- [ON], [OFF]

## [FRAME RATE]

Switches the shooting interval and exposure time when [VFR] is [ON].

The items that can be set are as follows.

- When the [SYSTEM] menu → [FREQUENCY] → [59.94Hz] is set

  - [60fps], [54fps], [48fps], [44fps], [40fps], [36fps], [34fps], [32fps], [30fps], [28fps], [27fps], [26fps], [25fps], [24fps], [22fps], [21fps], [20fps], [18fps], [15fps], [12fps], [9fps], [6fps], [4fps], [2fps], [1fps]

- When the [SYSTEM] menu → [FREQUENCY] → [50.00Hz] is set

  - [50fps], [48fps], [45fps], [42fps], [37fps], [34fps], [32fps], [30fps], [28fps], [27fps], [26fps], [25fps], [24fps], [23fps], [22fps], [21fps], [20fps], [18fps], [15fps], [12fps], [9fps], [6fps], [4fps], [2fps], [1fps]

## [SYNC SCAN TYPE]

Switches the synchro scan display settings.

[sec] | Displays in time.
[deg] | Displays in the shutter aperture angle.

## [SYNC SCAN]

Displays the speed of the synchro scan shutter that is used when shooting video for television etc.

The items that can be set are as follows.

- When [SYNC SCAN TYPE] is set to [sec] and the [SYSTEM] menu → [FREQUENCY] → [59.94Hz] is set

  - 59.94i/59.94p mode: [1/60.0] … [1/7200]

  - 29.97p mode: [1/30.0]…[1/7200]

  - 23.98p mode: [1/24.0]…[1/7200]

- When [SYNC SCAN TYPE] is set to [sec] and the [SYSTEM] menu → [FREQUENCY] → [50.00Hz] is set

  - 50i/50p mode: [1/50.0]…[1/7200]

  - 25p mode: [1/25.0]…[1/7200]

- When [SYNC SCAN TYPE] is set to [deg]

  - [3.0d]…[360.0d]

## [MASTER DTL]

Sets the level of the detail effect of the whole part.

The items that can be set are as follows.

- [−31]…[31]

NOTE

- This cannot be set when the [SYSTEM] menu → [COLOR SETTING] is set to [V-Log].

## [DTL CORING]

Sets the level of signal (including noise) that does not activate the detail effect.

The items that can be set are as follows.

- [0]…[60]

NOTE

- This cannot be set when the [SYSTEM] menu → [COLOR SETTING] is set to [V-Log].

## [DETAIL SETTING]

This cannot be set when the [SYSTEM] menu → [COLOR SETTING] is set to [V-Log].

### [DETAIL]

Sets [ON]/[OFF] of the detail function.

The items that can be set are as follows.

- [ON], [OFF]

### [V.DTL LEVEL]

Sets the intensity of the detail level in the vertical direction.

The items that can be set are as follows.

- [−7]…[7]

### [DTL FREQ.]

Sets the thickness of the detail.

The items that can be set are as follows.

- [−7]…[7]

### [LEVEL DEPEND.]

When the detail of luminosity signal is emphasized, details in the darker areas are compressed.

Details of bright areas are compressed more when the value set for [LEVEL DEPEND.] is larger.

The items that can be set are as follows.

- [−7]…[7]

### [KNEE APE LVL]

Sets the detail level of high luminosity areas (high-brightness areas).

The items that can be set are as follows.

- [0]…[5]

### [DTL GAIN(+)]

Sets the detail level of the plus direction (to make brighter).

The items that can be set are as follows.

- [−31]…[31]

### [DTL GAIN(−)]

Sets the detail level of the minus direction (to make darker).

The items that can be set are as follows.

- [−31]…[31]

## [SKIN TONE DTL A]

Selects the skin tone table that will display the skin tone detail.

Create the skin tone table with [DETECT TABLE]. You can shoot smoother skin tones by displaying the skin tone detail.

You can use only [SKIN TONE DTL A] or use a combination of [SKIN TONE DTL A] and [SKIN TONE DTL B] or a combination of [SKIN TONE DTL A] and [SKIN TONE DTL C].

The items that can be set are as follows.

- [ON], [OFF]

NOTE

- The setting is fixed to [OFF] when the [SYSTEM] menu → [COLOR SETTING] is set to [V-Log].

## [SKIN TONE DTL B]

Selects the skin tone table that will display the skin tone detail.

Create the skin tone table with [DETECT TABLE]. You can shoot smoother skin tones by displaying the skin tone detail.

You can use only [SKIN TONE DTL B] or use a combination of [SKIN TONE DTL B] and [SKIN TONE DTL A] or a combination of [SKIN TONE DTL B] and [SKIN TONE DTL C].

The items that can be set are as follows.

- [ON], [OFF]

NOTE

- The setting is fixed to [OFF] when the [SYSTEM] menu → [COLOR SETTING] is set to [V-Log].

## [SKIN TONE DTL C]

Selects the skin tone table that will display the skin tone detail.

Create the skin tone table with [DETECT TABLE]. You can shoot smoother skin tones by displaying the skin tone detail.

You can use only [SKIN TONE DTL C] or use a combination of [SKIN TONE DTL C] and [SKIN TONE DTL A] or a combination of [SKIN TONE DTL C] and [SKIN TONE DTL B].

The items that can be set are as follows.

- [ON], [OFF]

NOTE

- The setting is fixed to [OFF] when the [SYSTEM] menu → [COLOR SETTING] is set to [V-Log].

## [SKIN TONE ZEBRA]

Set to display a zebra pattern in the skin tone area displayed in the viewfinder screen.

The zebra pattern is displayed when this item is set to [ON] and [SKIN TONE DTL A]/[SKIN TONE DTL B]/[SKIN TONE DTL C] is activated.

The zebra pattern displays the area selected in [SKIN TONE DTL SETTING].

The items that can be set are as follows.

- [ON], [OFF]

NOTE

- The setting is fixed to [OFF] when the [SYSTEM] menu → [COLOR SETTING] is set to [V-Log].

## [SKIN TONE DTL SETTING]

This cannot be set when the [SYSTEM] menu → [COLOR SETTING] is set to [V-Log].

### [DETECT TABLE]

Selects the skin tone table of the subject that displays the skin tone detail.

The items that can be set are as follows.

- [A], [B], [C]

### [SKIN DTL EFFECT]

Sets the effective level of the skin tone detail.

The items that can be set are as follows.

- [0]…[31]

### [I CENTER]

Sets the center position of the upper I axis (setting the area that applies the skin tone).

The items that can be set are as follows.

- [0]…[255]

### [I WIDTH]

Sets the width of the area that displays the skin tone of the upper I axis that focus on [I CENTER].

The items that can be set are as follows.

- [1]…[3]

### [Q WIDTH]

Sets the width of the area that displays the skin tone of the upper Q axis that focus on [I CENTER].

The items that can be set are as follows.

- [1]…[3]

### [Q PHASE]

Sets the phase of the area that applies the skin tone related to the Q axis.

The items that can be set are as follows.

- [−128]…[127]

## [RB GAIN CONTROL SETTING]

### [R GAIN AWB PRE]

Sets the Rch gain when the <WHITE BAL> switch is at the <PRST> position.

The items that can be set are as follows.

- [−200]…[200]

### [B GAIN AWB PRE]

Sets the Bch gain when the <WHITE BAL> switch is at the <PRST> position.

The items that can be set are as follows.

- [−200]…[200]

### [R GAIN AWB A]

Sets the Rch gain when the <WHITE BAL> switch is at the <A> position.

The items that can be set are as follows.

- [−200]…[200]

### [B GAIN AWB A]

Sets the Bch gain when the <WHITE BAL> switch is at the <A> position.

The items that can be set are as follows.

- [−200]…[200]

### [R GAIN AWB B]

Sets the Rch gain when the <WHITE BAL> switch is at the <B> position.

The items that can be set are as follows.

- [−200]…[200]

### [B GAIN AWB B]

Sets the Bch gain when the <WHITE BAL> switch is at the <B> position.

The items that can be set are as follows.

- [−200]…[200]

### [AWB A GAIN OFFSET]

Sets the Rch gain and Bch gain when the <WHITE BAL> switch is at the <A> position and automatic white balance is performed.

[ON] | Keeps the values set in [R GAIN AWB A] and [B GAIN AWB A].
[OFF] | Sets the value of Rch gain and Bch gain to [0].

### [AWB B GAIN OFFSET]

Sets the Rch gain and Bch gain when the <WHITE BAL> switch is at the <B> position and automatic white balance is performed.

[ON] | Keeps the values set in [R GAIN AWB B] and [B GAIN AWB B].
[OFF] | Sets the value of Rch gain and Bch gain to [0].

## [COLOR TEMP Ach SETTING]

### [COLOR TEMP]

Displays the color temperature when the <WHITE BAL> switch is at the <A> position and automatic white balance is working, or when it is preset.

Also, in automatic white balance operation, the color temperature can be changed by changing the output balance of Rch and Bch.

The items that can be set are as follows.

- [2000K]…[15000K]

### [R GAIN]

Displays the output of Rch when the <WHITE BAL> switch is at the <A> position and automatic white balance is working, or when it is preset.

In the automatic white balance operation, the color can also be changed on the Rch axis by changing the output of Rch.

The items that can be set are as follows.

- [−400]…[400]

### [B GAIN]

Displays the output of Bch when the <WHITE BAL> switch is at the <A> position and automatic white balance is working, or when it is preset.

In automatic white balance operation, the color can also be changed on the Bch axis by changing the output of Bch.

The items that can be set are as follows.

- [−400]…[400]

### [G AXIS]

Displays the output of G axis when the <WHITE BAL> switch is at the <A> position and automatic white balance is working, or when it is preset.

In the automatic white balance operation, the color can also be changed on the G axis by changing the output of Rch and Bch.

The items that can be set are as follows.

- [−400]…[400]

## [COLOR TEMP Bch SETTING]

### [COLOR TEMP]

Displays the color temperature when the <WHITE BAL> switch is at the <B> position and automatic white balance is working, or when it is preset.

Also, in automatic white balance operation, the color temperature can be changed by changing the output balance of Rch and Bch.

The items that can be set are as follows.

- [2000K]…[15000K]

### [R GAIN]

Displays the output of Rch when the <WHITE BAL> switch is at the <B> position and automatic white balance is working, or when it is preset.

In automatic white balance operation, the color can also be changed on the Rch axis by changing the output of Rch.

The items that can be set are as follows.

- [−400]…[400]

### [B GAIN]

Displays the output of Bch when the <WHITE BAL> switch is at the <B> position and automatic white balance is working, or when it is preset.

In automatic white balance operation, the color can also be changed on the Bch axis by changing the output of Bch.

The items that can be set are as follows.

- [−400]…[400]

### [G AXIS]

Displays the output of G axis when the <WHITE BAL> switch is at the <B> position and automatic white balance is working, or when it is preset.

In the automatic white balance operation, the color can also be changed on the G axis by changing the output of Rch and Bch.

The items that can be set are as follows.

- [−400]…[400]

## [CHROMA LEVEL]

Sets the chroma level of PR and PB signals.

The items that can be set are as follows.

- [−99%]…[99%], [OFF]

NOTE

- This cannot be set when the [SYSTEM] menu → [COLOR SETTING] is set to [V-Log].

## [CHROMA PHASE]

Finely adjusts the chroma phase of the PR signal and PB signal.

The items that can be set are as follows.

- [−31]…[31]

NOTE

- This cannot be set when the [SYSTEM] menu → [COLOR SETTING] is set to [V-Log].

## [MATRIX]

This cannot be set when the [SYSTEM] menu → [COLOR SETTING] is set to [V-Log].

### [MATRIX TYPE]

Selects the matrix table to display the color for shooting.

[NORMAL1] | Displays the color suitable for shooting outdoors or under a halogen lamp.
[NORMAL2] | Displays more vivid color than [NORMAL1].
[FLUO.] | Displays the color suitable for shooting indoors under fluorescent light.
[CINELIKE] | Displays the color suitable for shooting cinematic video.

### [ADAPTIVE MATRIX]

Enables/disables the function to control the linear matrix in accordance with the shooting condition.

If [ADAPTIVE MATRIX] is assigned to the USER button, pressing the USER button switches [ON]/[OFF].

The items that can be set are as follows.

- [ON], [OFF]

## [MATRIX SETTING]

This cannot be set when the [SYSTEM] menu → [COLOR SETTING] is set to [V-Log].

### [R-G]

Adjusts the linear matrix. (Red - Green)

The items that can be set are as follows.

- [−63]…[63]

### [R-B]

Adjusts the linear matrix. (Red - Blue)

The items that can be set are as follows.

- [−63]…[63]

### [G-R]

Adjusts the linear matrix. (Green - Red)

The items that can be set are as follows.

- [−63]…[63]

### [G-B]

Adjusts the linear matrix. (Green - Blue)

The items that can be set are as follows.

- [−63]…[63]

### [B-R]

Adjusts the linear matrix. (Blue - Red)

The items that can be set are as follows.

- [−63]…[63]

### [B-G]

Adjusts the linear matrix. (Blue - Green)

The items that can be set are as follows.

- [−63]…[63]

## [COLOR CORRECTION]

This cannot be set when the [SYSTEM] menu → [COLOR SETTING] is set to [V-Log].

### [R] ([SAT])

Corrects red color saturation.

The items that can be set are as follows.

- [−63]…[63]

### [R] ([PHASE])

Corrects the red hue.

The items that can be set are as follows.

- [−63]…[63]

### [R-R-Mg] ([SAT])

Corrects the color saturation between red and “colors between red and magenta”.

The items that can be set are as follows.

- [−63]…[63]

### [R-R-Mg] ([PHASE])

Corrects the hue between red and “colors between red and magenta”.

The items that can be set are as follows.

- [−63]…[63]

### [R-Mg] ([SAT])

Corrects the color saturation between red and magenta.

The items that can be set are as follows.

- [−63]…[63]

### [R-Mg] ([PHASE])

Corrects the hue between red and magenta.

The items that can be set are as follows.

- [−63]…[63]

### [Mg] ([SAT])

Corrects magenta color saturation.

The items that can be set are as follows.

- [−63]…[63]

### [Mg] ([PHASE])

Corrects the magenta hue.

The items that can be set are as follows.

- [−63]…[63]

### [Mg-B] ([SAT])

Corrects the color saturation between magenta and blue.

The items that can be set are as follows.

- [−63]…[63]

### [Mg-B] ([PHASE])

Corrects the hue between magenta and blue.

The items that can be set are as follows.

- [−63]…[63]

### [B] ([SAT])

Corrects blue color saturation.

The items that can be set are as follows.

- [−63]…[63]

### [B] ([PHASE])

Corrects the blue hue.

The items that can be set are as follows.

- [−63]…[63]

### [B-Cy] ([SAT])

Corrects the color saturation between blue and cyan.

The items that can be set are as follows.

- [−63]…[63]

### [B-Cy] ([PHASE])

Corrects the hue between blue and cyan.

The items that can be set are as follows.

- [−63]…[63]

### [Cy] ([SAT])

Corrects cyan color saturation.

The items that can be set are as follows.

- [−63]…[63]

### [Cy] ([PHASE])

Corrects the cyan hue.

The items that can be set are as follows.

- [−63]…[63]

### [Cy-G] ([SAT])

Corrects the color saturation between cyan and green.

The items that can be set are as follows.

- [−63]…[63]

### [Cy-G] ([PHASE])

Corrects the hue between cyan and green.

The items that can be set are as follows.

- [−63]…[63]

### [G] ([SAT])

Corrects green color saturation.

The items that can be set are as follows.

- [−63]…[63]

### [G] ([PHASE])

Corrects the green hue.

The items that can be set are as follows.

- [−63]…[63]

### [G-Yl] ([SAT])

Corrects the color saturation between green and yellow.

The items that can be set are as follows.

- [−63]…[63]

### [G-Yl] ([PHASE])

Corrects the hue between green and yellow.

The items that can be set are as follows.

- [−63]…[63]

### [G-Yl-Yl] ([SAT])

Corrects the color saturation between “colors between green and yellow” and yellow.

The items that can be set are as follows.

- [−63]…[63]

### [G-Yl-Yl] ([PHASE])

Corrects the hue between “colors between green and yellow” and yellow.

The items that can be set are as follows.

- [−63]…[63]

### [Yl] ([SAT])

Corrects yellow color saturation.

The items that can be set are as follows.

- [−63]…[63]

### [Yl] ([PHASE])

Corrects the yellow hue.

The items that can be set are as follows.

- [−63]…[63]

### [Yl-Yl-R] ([SAT])

Corrects the color saturation between yellow and “colors between yellow and red”.

The items that can be set are as follows.

- [−63]…[63]

### [Yl-Yl-R] ([PHASE])

Corrects the hue between yellow and “colors between yellow and red”.

The items that can be set are as follows.

- [−63]…[63]

### [Yl-R] ([SAT])

Corrects the color saturation between yellow and red.

The items that can be set are as follows.

- [−63]…[63]

### [Yl-R] ([PHASE])

Corrects the hue between yellow and red.

The items that can be set are as follows.

- [−63]…[63]

### [Yl-R-R] ([SAT])

Corrects the color saturation between “colors between yellow and red” and red.

The items that can be set are as follows.

- [−63]…[63]

### [Yl-R-R] ([PHASE])

Corrects the hue between “colors between yellow and red” and red.

The items that can be set are as follows.

- [−63]…[63]

## [MASTER PED]

Sets the master pedestal.

The items that can be set are as follows.

- [−200]…[200]

NOTE

- This cannot be set when the [SYSTEM] menu → [COLOR SETTING] is set to [V-Log].

## [RGB BLACK CONTROL SETTING]

This cannot be set when the [SYSTEM] menu → [COLOR SETTING] is set to [V-Log].

### [R PED]

Sets the Rch pedestal level.

The items that can be set are as follows.

- [−100]…[100]

### [G PED]

Sets the Gch pedestal level.

The items that can be set are as follows.

- [−100]…[100]

### [B PED]

Sets the Bch pedestal level.

The items that can be set are as follows.

- [−100]…[100]

### [PEDESTAL OFFSET]

Sets the Rch, Gch, and Bch pedestal levels after adjusting the automatic black balance.

[ON] | Keeps each of the values set in [R PED], [G PED], and [B PED].
[OFF] | Sets the pedestal level of Rch, Gch, and Bch to [0].

## [GAMMA MODE SEL]

Selects the gamma mode.

[HD] | Sets the gamma characteristics for HD (High Definition).
[SD] | Increases gain in darker areas more than HD gamma.
[FILMLIKE1] | Sets the characteristics that reproduce more highlight areas compared to HD gamma.
[FILMLIKE2] | Sets the characteristics that reproduce more highlight areas compared to [FILMLIKE1].
[FILMLIKE3] | Sets the characteristics that reproduce more highlight areas compared to [FILMLIKE2].
[FILM-REC] | Sets the cine gamma characteristics for film.
[VIDEO-REC] | Sets the cine gamma characteristics for video.
[HLG] | Sets the hybrid log gamma (HLG) characteristics.

NOTE

- This cannot be set when the [SYSTEM] menu → [COLOR SETTING] is set to [V-Log].

## [GAMMA SETTING]

This cannot be set when the [SYSTEM] menu → [COLOR SETTING] is set to [V-Log].

### [MASTER GAMMA]

Sets the master gamma in 0.01 steps.

The items that can be set are as follows.

- [0.30]…[0.75]

### [F-REC DYNAMIC LVL]

When [FILM-REC] is selected in [GAMMA MODE SEL], dynamic range is set.

No settings are changed if an item other than [FILM-REC] is selected.

The items that can be set are as follows.

- [200%] … [600%] (100% step)

### [F-REC BLACK STR LVL]

When [FILM-REC] is selected in [GAMMA MODE SEL], black stretch is set.

No settings are changed if an item other than [FILM-REC] is selected.

The items that can be set are as follows.

- [0%]…[30%]

### [V-REC KNEE SLOPE]

When [VIDEO-REC] is selected in [GAMMA MODE SEL], knee slope is set.

No settings are changed if an item other than [VIDEO-REC] is selected.

The items that can be set are as follows.

- [150%] … [500%] (50% step)

### [V-REC KNEE POINT]

When [VIDEO-REC] is selected in [GAMMA MODE SEL], knee point is set.

No settings are changed if an item other than [VIDEO-REC] is selected.

The items that can be set are as follows.

- [30%]…[107%]

### [BLACK GAMMA]

Sets the gamma curves of dark areas.

[−8]…[−1] | Compresses the dark area.
[0] | Standard state
[1]…[8] | Expands dark areas.

### [B.GAMMA RANGE]

Sets the maximum level of compression/expansion.

[1] | Around 20%
[2] | Around 30%
[3] | Around 40%

## [KNEE SETTING]

This cannot be set when the [SYSTEM] menu → [COLOR SETTING] is set to [V-Log].

### [KNEE MODE]

Sets the knee operation mode.

The items that can be set are as follows.

- [AUTO], [MANUAL], [OFF]

### [A.KNEE RESPONSE]

Sets the auto knee response speed. The smaller the setting value, the faster the response speed is.

The items that can be set are as follows.

- [1]…[8]

### [KNEE POINT]

Sets the knee point position in 0.5% steps.

The items that can be set are as follows.

- [70.0%]…[107.0%]

### [KNEE SLOPE]

Sets the knee inclination.

The items that can be set are as follows.

- [0]…[99]

### [HLG KNEE SW]

Enables/disables the operation of knee for HLG.

The items that can be set are as follows.

- [ON], [OFF]

### [HLG KNEE POINT]

Sets the position of the knee point for HLG.

The items that can be set are as follows.

- [55]…[100]

### [HLG KNEE SLOPE]

Sets the inclination of knee for HLG.

The items that can be set are as follows.

- [0]…[100]

## [WHITE CLIP SETTING]

This cannot be set when the [SYSTEM] menu → [COLOR SETTING] is set to [V-Log].

### [WHITE CLIP]

Turns the white clip function [ON]/[OFF]. The setting value of [WHITE CLIP LEVEL] is enabled when the function is [ON].

The items that can be set are as follows.

- [ON], [OFF]

### [WHITE CLIP LEVEL]

Sets the white clip level.

The items that can be set are as follows.

- [90%]…[109%]

## [DRS]

Enables/disables the dynamic range stretcher function.

If functions are assigned to the USER buttons, [ON]/[OFF] can be switched using the USER button operations.

The items that can be set are as follows.

- [ON], [OFF]

NOTE

- The setting is fixed to [OFF] when the [SYSTEM] menu → [COLOR SETTING] is set to [V-Log].

## [DRS EFFECT DEPTH]

Sets the compression level of the high luminosity areas of the dynamic range stretcher function.

By compressing the video signal levels of the high luminosity areas that are blown out in normal shooting, the dynamic range can be expanded.

The items that can be set are as follows.

- [1]…[3]

NOTE

- This cannot be set when the [SYSTEM] menu → [COLOR SETTING] is set to [V-Log].

## [DNR]

Changes the noise reduction setting and adjusts the noise reduction effect.

The items that can be set are as follows.

- [OFF], [1], [2]

## [A.IRIS LEVEL]

Enables/disables the auto iris level function.

If functions are assigned to the USER buttons, [ON]/[OFF] can be switched using the USER button operations.

The items that can be set are as follows.

- [ON], [OFF]

## [A.IRIS LEVEL EFFECT]

Adjusts the brightness in the auto iris mode.

Increase the value to brighten, and decrease the value to darken the convergence of auto iris.

The items that can be set are as follows.

- [−50]…[50]

Top of the page