- Top
- Shooting
- Variable frame rate (VFR) recording function/super slow recording function

# Variable frame rate (VFR) recording function/super slow recording function

It is possible to acquire smooth slow motion or quick motion vide by shooting with a different frame rate from the frame rate to play back.

Variable frame rate (VFR)
Super slow

NOTE

- Audio cannot be recorded with the variable frame rate recording and super slow recording. However, audio is also recorded if the frame rate same as the recording frame frequency of [REC FORMAT] is set when using variable frame rate recording.

- The screen may be disrupted or become dark when the frame rate setting is changed.

- The frame rate cannot be changed while recording.

- The [RECORDING] menu → [TC/UB] → [FREE/REC RUN] is fixed to [REC RUN].

- The recording is paused when ten hours has past from the time the recording was started. The recording is automatically resumed after few seconds.

  When performing high-speed shooting, the recording time will be shorter than 10 hours depending on the ratio of the frame rate of the recording format and the variable frame rate. The recording will stop in 5 hours when the recording frame frequency of [REC FORMAT] is set to 23.98p and the [SCENE FILE] menu → [FRAME RATE] is set to [48fps].

- For recording limitations of variable frame rate recording or super slow recording, refer to “Recording function that cannot be used simultaneously”.

- It may take time to stop recording even if recording is stopped right after recording is started.

  When the recording frame frequency of [REC FORMAT] is set to 59.94p and the [SCENE FILE] menu → [FRAME RATE] is set to [1fps], recording is continued for a maximum of one minute until the length of the clip after shooting becomes one second.

Top of the page