- Top
- Shooting
- Convenient shooting functions
- Level gauge

# Level gauge

A level gauge that indicates the horizontal and vertical inclinations of the camera can be displayed on the LCD monitor.

The line of the level gauge is displayed in orange while the camera is inclined. The line of the level gauge will change from orange to light blue, and then to white when the inclination of the camera is corrected. It will indicate up to approximately 30° in horizontal direction, and 30° in vertical direction.

Select the [VIDEO OUT/LCD/VF] menu → [LEVEL GAUGE] → [LEVEL GAUGE] → [ON].

NOTE

- The display of level gauge cannot be recorded.

- The level gauge is not displayed when the enlarged display function of the focus assist function is enabled, or when displaying the color bars.

- The level gauge may not display correctly while moving the camera.

- The level gauge may not display correctly when shooting with the camera inclined excessively upward or downward.

- Press the USER button to which [LEVEL GAUGE] is assigned or touch USER button icon to display or hide the level gauge.

- Press the USER button to which [LEVEL GAUGE SET] is assigned or touch the USER button icon to set the current horizontal and vertical directions as the reference value of the level gauge. Restore the set value in the [VIDEO OUT/LCD/VF] menu → [LEVEL GAUGE] → [LEVEL GAUGE RESET].

Top of the page