- Top
- Shooting
- Variable frame rate (VFR) recording function/super slow recording function
- Variable frame rate (VFR)

# Variable frame rate (VFR)

Allows the high-speed shooting from 1fps to maximum of 60fps.

In the [SYSTEM] menu → [FREQUENCY]/[FILE FORMAT]/[REC FORMAT], select the resolution and codec for recording video and the frequency for the reference frame rate.

- For the combinations that can be set, refer to “Selecting the resolution, codec, and frame rate for recording video”.

  The range of the frame rate that can perform high-speed shooting differs depending on the setting.

Select the [SCENE FILE] menu → [VFR] → [ON].

- This can also be set even with the USER button. Refer to “Functions assigned to USER buttons”.

Set the frame rate in accordance with the shooting condition in the [SCENE FILE] menu → [FRAME RATE].

- This can also be set with the multi manual function. Refer to “Multi manual function”.

Press the REC button.

Variable frame rate recording is started.

Top of the page