- Top
- Shooting
- Adjustable settings when shooting
- Area mode function

# Area mode function

Touch the subject to apply various effects tailored to the subject that is touched.

- Area auto focus function

  Adjusts the focus automatically tailored to the subject that is touched.

- Area auto iris level function

  Adjusts the iris automatically tailored to the subject that is touched.

- Area brightness display

  Displays the luminance level of the subject that is touched.

## Operation function settings

Sets the operation to be assigned to the area mode function from the [CAMERA] menu.

Select the desired function in the [CAMERA] menu → [SW MODE] → [AREA MODE].

- [INHIBIT]: Does not assign a function.

- [FOCUS]: Sets the area focus function

- [IRIS]: Area iris function

- [Y GET]: Area brightness display

- [FOCUS/IRIS]: Simultaneous operation of the area focus function and area iris function

- [FOCUS/Y GET]: Simultaneous operation of the area focus function and area brightness display

## Operation of area mode function

The function set in the [CAMERA] menu → [SW MODE] → [AREA MODE] can be used by performing the following operation when shooting or while in shooting standby.

Press the USER button to which the function set in the [CAMERA] menu → [SW MODE] → [AREA MODE] is assigned or touch the USER button icon.

- The area frame is displayed, and the is displayed on the right side of the screen.

- When the area brightness display is activated, the brightness display in the center does not operate.

Touch the shooting screen.

- The area frame is displayed in the area that is touched to apply the effects set in the menu.

Press the USER button or the USER button icon again.

- The area frame disappears and the camera exits the area mode function.

NOTE

- The area mode function is cancelled when the power is turned off or when the thumbnail screen is displayed.

Top of the page