- Top
- Output and Screen Display
- Output format
- Format that can be output from the <SDI OUT> terminal

# Format that can be output from the <SDI OUT> terminal

The format that can be output from the <SDI OUT> terminal differs with following combination of the settings.

- [SYSTEM] menu → [FREQUENCY]

- [SYSTEM] menu → [REC FORMAT]

- [VIDEO OUT/LCD/VF] menu → [SDI OUT] → [OUT FORMAT]

Item | Output Format [OUT FORMAT]
--- | ---
[FREQUENCY] | [REC FORMAT]
Resolution | Frequency
[59.94Hz] | 3840×2160 | 59.94p | 1920×1080 59.94p 1920×1080 59.94i (Factory setting)
|  | 29.97p | 1920×1080 29.97PsF
|  | 23.98p | 1920×1080 23.98PsF
| 1920×1080 | 59.94p | 1920×1080 59.94p 1920×1080 59.94i (Factory setting) 720×480 59.94i
|  | 59.94i | 1920×1080 59.94i (Factory setting) 720×480 59.94i
|  | 29.97p | 1920×1080 29.97p (Factory setting) 720×480 59.94i
|  | 23.98p | 1920×1080 23.98p (Factory setting) 720×480 59.94i
| 1280×720 | 59.94p | 1280×720 59.94p (Factory setting) 720×480 59.94i
| 720×480 | 59.94i | 720×480 59.94i
[50.00Hz] | 3840×2160 | 50.00p | 1920×1080 50.00p 1920×1080 50.00i (Factory setting)
|  | 25.00p | 1920×1080 25.00PsF
| 1920×1080 | 50.00p | 1920×1080 50.00p 1920×1080 50.00i (Factory setting) 720×576 50.00i
|  | 50.00i | 1920×1080 50.00i (Factory setting) 720×576 50.00i
|  | 25.00p | 1920×1080 25.00PsF (Factory setting) 720×576 50.00i
| 1280×720 | 50.00p | 1280×720 50.00p (Factory setting) 720×576 50.00i
| 720×576 | 50.00i | 720×576 50.00i

NOTE

- The 3840×2160 output is not supported.

- [OUT FORMAT] restores the factory settings when the settings of [FREQUENCY] and [REC FORMAT] change and the current setting values of [OUT FORMAT] cannot be acquired.

- The output format when playing back from the thumbnail screen is as follows.

  - It will be the value set in [OUT FORMAT] when the recording resolution of the playback clip is the same as [REC FORMAT].

  - It will be factory setting of [OUT FORMAT] when the recording resolution of the playback clip is different from [REC FORMAT].

Top of the page