- Top
- Shooting
- Multi manual function
- Setting the variable value for the white balance

# Setting the variable value for the white balance

Turn the multidial to display the [ WB].

Press the multidial.

The white balance display is highlighted in orange.

Turn the multidial to select the color temperature.

Press the multidial.

The setting changes to the value displayed and exits.

Press the <EXIT> button to exit without changing the setting.

NOTE

- [ WB] is only displayed when the following conditions are satisfied.

  - The <WHITE BAL> switch is in the <PRST> position

  - The [CAMERA] menu → [SW MODE] → [W.BAL PRESET] is set to [VAR]

  - The auto tracking white balance function is disabled

  - IR recording is disabled

Top of the page