- Top
- Network Connection
- Streaming function
- Starting streaming with an operation from the application software

# Starting streaming with an operation from the application software

Select the [NETWORK] menu → [STREAMING] → [START TRIGGER] → [RECEIVER].

Specify the IP address and the path of the camera with the application software as follows, and start streaming.

rtsp://(IP address)/stream

NOTE

- Perform an operation from the application software to stop streaming.

- Only RTSP is available when starting streaming with an operation from application software.

- For details about the operations to start streaming from the application software, please see the manual for each application software.

- Streaming stops when performing operations such as displaying the thumbnail screen or playing back clips on the camera.

- Streaming may stop when the date/time is set while streaming.

## Streaming with multicast

One streaming can be distributed to multiple receivers via supported router, etc., when the multicast function is used.

Select the [NETWORK] menu → [STREAMING] → [START TRIGGER] → [RECEIVER(MULTICAST)].

Select the [NETWORK] menu → [STREAMING], and specify [MULTICAST ADDRESS] and [MULTICAST PORT].

- Set [MULTICAST ADDRESS] within following range.

  IPv4: 224.0.1.0 to 239.255.255.254

  IPv6: Multicast address starting with FF

- Set [MULTICAST PORT] within the range of 1024 to 50000.

Specify the address of the camera and start streaming with the application software.

NOTE

- Multicast cannot start streaming with the operation on the camera.

- Disable the LAN card not to be used when receiving the multicast image to be displayed on a computer with multiple LAN cards installed.

Top of the page