- Top
- Operation
- Handling setting data
- Setup file

# Setup file

The menu that is specified can be saved to the camera memory or the memory card in card slot 1, or loaded to the camera from the memory card.

## Saving the setup file

The setup file can be overwritten to a file on the camera memory or memory card in card slot 1, or saved as a new file.

### Saving the setup file as a new file to the memory card

Specify a file name to save the current setting values of the camera to the memory card in card slot 1 as a new file.

Select the [OTHERS] menu → [FILE] → [SETUP FILE(SD CARD)] → [SAVE AS].

The file name entry screen and the keyboard are displayed.

Enter the text to set with the keyboard.

Select [Enter].

A confirmation screen is displayed.

Select [SET].

The file is saved.

- An error message may be displayed. For details about the error message, refer to “Cases indicated by error messages”.

### Saving the setup file by overwriting a file on the memory card

Overwrites the file selected in the list of the setup files saved on the memory card with the current setting values of the camera.

Select the [OTHERS] menu → [FILE] → [SETUP FILE(SD CARD)] → [SAVE].

The list of setup files saved on the memory card in card slot 1 is displayed.

Select the file to overwrite from the list of setup files.

The file name entry screen and the keyboard are displayed. Leave it as is when overwriting.

Select [Enter].

A confirmation screen is displayed.

Select [SET].

The file is saved.

### Saving the setup file to the camera memory

Saves the current setting value of the camera into the camera memory.

Select the [OTHERS] menu → [FILE] → [SETUP FILE(MEMORY)] → [SAVE].

## Loading the setup file

### Loading setup files from the memory card

Loads the setup file saved on the memory card in card slot 1.

Select the [OTHERS] menu → [FILE] → [SETUP FILE(SD CARD)] → [LOAD].

The list of setup files stored in the specified folder of the memory card in card slot 1 is displayed.

Select the file name for the file to load.

Select [SET].

Loading of the file is started. The camera is restarted after loading.

- An error message may be displayed. For details about the error message, refer to “Cases indicated by error messages”.

- The file saved by a camera with different firmware version may not be able to load.

### Loading setup files from the camera memory

Loads the setup file saved on the camera memory.

Select the [OTHERS] menu → [FILE] → [SETUP FILE(MEMORY)] → [LOAD].

Loading of the file is started. The camera is restarted after loading.

Top of the page