- Top
- Specification
- Specifications
- Other input/output

# Other input/output

<TC IN/OUT> terminal | BNC×1 Used as input/output terminal, input/output switch by menu Input: 1.0 V – 4.0 V [p-p], 10 kΩ Output: 2.0 V±0.5 V [p-p], low impedance
<REMOTE> terminal | 2.5 mm diameter super mini jack × 1 Remote control terminal of serial communication Analogue remote control used for previous Panasonic models cannot be used.
<USB2.0 HOST> terminal | Type A connector, 4-pin (5 V, 0.5 A), for attaching the wireless module (optional)
<USB3.0 DEVICE> terminal | USB 3.1 GEN1 type C connector, with USB mass storage function, without USB bus-powered function
<LAN> terminal | RJ-45: 1000BASE-T/100BASE-TX/10BASE-T
<DC IN 12V> terminal | DC12 V, EIAJ type 4

Top of the page