- Top
- Operation
- Menu settings
- [OTHERS] menu

# [OTHERS] menu

Configures the settings for writing/loading/initializing user files to the internal memory and other settings of the camera.

## [FILE]

Saves and loads the setting data.

For the saving and loading target, refer to “Target items for scene file/setup file/initialization”.

For details about saving and loading, refer to “Handling setting data”.

### [SCENE FILE(SD CARD)]

Loads or saves scene files on a memory card.

[LOAD] | Selects and loads the scene file saved on the memory card into the camera. Can select if all of the scene files ([F1:] to [F6:]) are loaded, or individually loaded.
[SAVE] | The setting values of the current scene file ([F1:] to [F6:]) are overwritten to the file selected from the list of scene files saved in the memory card.
[SAVE AS] | The setting values of the current scene file ([F1:] to [F6:]) is saved to the memory card as a new scene file by entering the file name.

### [SETUP FILE(SD CARD)]

Loads or saves setup files on a memory card.

[LOAD] | Selects the setup file saved on the memory card to load on the camera.
[SAVE] | Overwrites the file selected in the list of the setup files saved on the memory card with the current setting values of the camera.
[SAVE AS] | Enter a file name to save the current setting values in the camera as a new setup file in the memory card.

### [SETUP FILE(MEMORY)]

Loads/saves/initializes setup files in the internal memory of the camera.

[LOAD] | Loads setup data saved on the memory.
[SAVE] | Saves the setup data to the memory.
[INITIALIZE] | Restores the factory settings from the current settings for the menus in the setup data.

### [SLOT FOR LOAD/SAVE]

Sets the card slot to load and save the scene file, setup file, and streaming setting file.

The items that can be set are as follows.

- [SLOT1], [SLOT2]

(Factory setting: [SLOT1])

## [COLOR BARS]

### [COLOR BARS TYPE]

Sets the color bar to be used.

[SMPTE] | Uses the color bars in SMPTE standard.
[FULL] | Uses the full color bars.

(Factory setting: [SMPTE])

NOTE

- A smear may occur depending on the output resolution.

### [TEST TONE]

Sets whether the audio test signal (tone signal with specification level 1 kHz) is output when the video is switched to the color bar.

The standard level varies depending on the setting of the [AUDIO] menu → [REC CH SETTINGS] → [HEAD ROOM].

The items that can be set are as follows.

- [ON], [OFF]

(Factory setting: [ON])

## [LED]

### [TALLY LED]

Sets whether the tally lamp is to illuminate or not.

[FRONT] | The front tally lamp will illuminate.
[REAR] | The rear tally lamp will illuminate.
[BOTH] | Both the front and rear tally lamps will illuminate.
[OFF] | The tally lamp will not illuminate.

(Factory setting: [BOTH])

### [ACCESS LED]

Sets whether the card access lamp is to illuminate or not.

The items that can be set are as follows.

- [ON], [OFF]

(Factory setting: [ON])

## [CLOCK]

### [CLOCK SETTING]

Sets the calendar (date of the built-in clock) and time.

Year | [2018]…[2037]
Month | [JAN]…[DEC] ([1]…[12])
Day | [1]…[31] ([28], [29], [30])
Hour | [0]…[23]
Minute | [0]…[59]

### [TIME ZONE]

Sets the time zone. It will switch to the time with the time difference added when the time zone setting is changed.

The items that can be set are as follows.

- [−12:00]…[+12:30] (30 minutes steps), [+12:45], [+13:00]

(Factory setting: [+0:00])

### [DATE FORMAT]

Sets the display order of the year, month, and date of the calendar (date of the built-in clock). This is reflected to the date display of the clip information.

The items that can be set are as follows.

- [Y-M-D], [M-D-Y], [D-M-Y]

(Factory setting: [Y-M-D] (when [AREA SETTINGS] is set to [AREA 1] or [AREA 2]), [M-D-Y] (when [AREA SETTINGS] is set to [AREA 3]), [D-M-Y] (when [AREA SETTINGS] is set to [AREA 4]))

## [USB DEVICE]

### [CARD READER MODE]

Switches the camera to the card reader mode. A computer or other device can be connected via USB to use as a card reader of the memory card.

The LCD monitor turns off after approximately five to ten seconds when using the battery.

The screen will return to the card reader mode screen when the <> button, <> button, <> button, or </> button is pressed, or the multidial is turned up or down.

The card reader mode is ended and the screen will display the camera image screen when the <SET> button is pressed or the multidial is pressed.

The items that can be selected are as follows.

- [YES], [NO]

### [SERVICE MODE]

Switches the camera to the service mode.

You can also check software information (licenses) on a computer and other equipment. Confirm “LICENSE.TXT” for the external drive recognized by a computer.

The LCD monitor turns off after approximately five to ten seconds when using the battery.

The screen will return to the service mode screen when the <> button, <> button, <> button, or </> button is pressed, or the multidial is turned up or down.

The service mode is ended and the screen will display the camera image screen when the <SET> button is pressed or the multidial is pressed.

The items that can be selected are as follows.

- [YES], [NO]

## [INFORMATION]

Displays the information of the camera.

### [VERSION]

Displays the information of the camera.

[MODEL] | Displays the product name of the camera.
[SERIAL NO.] | Displays the serial number of the camera.
[NETWORK ID(MAC ADDRESS)] | Displays the MAC address for the <LAN> terminal of the camera.
[VERSION] | Displays the firmware version of the camera.

### [OPERATION TIME]

[TOTAL OPERATION] | Displays the total operation time.

### [UPDATE]

Updates the firmware.

Insert the memory card where the update file is saved into card slot 1.

The items that can be selected are as follows.

- [YES], [NO]

## [LANGUAGE]

Sets the display language.

This is not displayed when the [OPTION] menu → [AREA SETTINGS] → [AREA 2] is set.

- When [AREA SETTINGS] is set to [AREA 1]

  [] | Japanese
  [English] | English

(Factory setting: [])

- When [AREA SETTINGS] is set to [AREA 3]/[AREA 4]

  [English] | English
  [Español] | Spanish
  [Français] | French

(Factory setting: [English])

## [MENU INITIALIZE]

Returns the setting value of the menu to the factory setting. The camera is restarted after executing.

The items that can be selected are as follows.

- [YES], [NO]

Top of the page