- Top
- Shooting
- Audio input
- When using an audio device or an external microphone

# When using an audio device or an external microphone

Connect an audio device or an external microphone to the <AUDIO INPUT 1>/<AUDIO INPUT 2> terminal.

Switch the connected audio input with the <INPUT1>/<INPUT2> switch.

Connected device | Menu settings (you can set each channel individually)
--- | ---
<INPUT1>/<INPUT2> | [INPUT1 MIC LEVEL]/[INPUT2 MIC LEVEL]*1 | [INPUT1 LINE LEVEL]/[INPUT2 LINE LEVEL]*2
Audio device | <LINE> | Disabled | [4dB], [0dB]
External microphone | <MIC> | [−40dB], [−50dB], [−60dB] | Disabled
External microphone (with power supply) | <+48V> | [−40dB], [−50dB], [−60dB] | Disabled

Factory setting: [−50dB]

Factory setting: [0dB]

NOTE

- When using a super-directional microphone AG-MC200G (optional), set [INPUT1 MIC LEVEL]/[INPUT2 MIC LEVEL] to [−50dB].

Top of the page