- Top
- Shooting
- Image quality adjustment
- Color correction function

# Color correction function

This function sets color saturation and phase. These settings affect each of the 16 phases of the video individually. It can be set to individual color hue.

(Axis to operate)

#### General settings

Use the camera with the factory settings.

#### Advanced settings

[R] ([PHASE])/[R-R-Mg] ([PHASE])/[R-Mg] ([PHASE])/[Mg] ([PHASE])/[Mg-B] ([PHASE])/[B] ([PHASE])/[B-Cy] ([PHASE])/[Cy] ([PHASE])/[Cy-G] ([PHASE])/[G] ([PHASE])/[G-Yl] ([PHASE])/[G-Yl-Yl] ([PHASE])/[Yl] ([PHASE])/[Yl-Yl-R] ([PHASE])/[Yl-R] ([PHASE])/[Yl-R-R] ([PHASE]): Changes the phases. + rotates clockwise and − rotates counter-clockwise.

[R] ([SAT])/[R-R-Mg] ([SAT])/[R-Mg] ([SAT])/[Mg] ([SAT])/[Mg-B] ([SAT])/[B] ([SAT])/[B-Cy] ([SAT])/[Cy] ([SAT])/[Cy-G] ([SAT])/[G] ([SAT])/[G-Yl] ([SAT])/[G-Yl-Yl] ([SAT])/[Yl] ([SAT])/[Yl-Yl-R] ([SAT])/[Yl-R] ([SAT])/[Yl-R-R] ([SAT]): Changes the saturation.

NOTE

- Color correction function cannot be set when the [SYSTEM] menu → [COLOR SETTING] is set to [V-Log].

Top of the page