- Top
- Shooting
- Convenient shooting functions
- Zebra patterns display

# Zebra patterns display

The camera can display two types of zebra patterns to the output image from the LCD monitor.

Select the [VIDEO OUT/LCD/VF] menu → [EI ASSIST] → [ZEBRA] → [ON].

- Select [MOMENT]. The zebra pattern is displayed for approximately five seconds when the the USER button to which [ZEBRA] is assigned is pressed or the USER button icon is touched.

- Factory setting: [OFF]

## Setting the detection level

Set each item in the [VIDEO OUT/LCD/VF] menu → [EI ASSIST].

Item | Description of settings
--- | ---
[ZEBRA1 DETECT] | Sets the detection level of zebra pattern 1. [0%]…[109%] (Factory setting: [80%])
[ZEBRA2 DETECT] | Sets the detection level of zebra pattern 2. [0%]…[109%] (Factory setting: [100%])
[ZEBRA2] | Enables/disables zebra pattern 2 and selects [SPOT]. [ON], [SPOT], [OFF] (Factory setting: [OFF])

#### Display area of the zebra pattern

The display area of the zebra pattern varies depending on the [VIDEO OUT/LCD/VF] menu → [EI ASSIST] setting.

When [SPOT] is selected in [ZEBRA2], the area corresponding to the [ZEBRA1 DETECT] setting value to the [ZEBRA2 DETECT] setting value is displayed in zebra pattern.

[ZEBRA2]

[ON]

[OFF]

[SPOT]

[109%]

[ZEBRA2 DETECT]

[ZEBRA1 DETECT]

[0%]

NOTE

- The zebra pattern cannot be recorded.

- The zebra pattern is not displayed while displaying the color bars.

- The zebra pattern is not displayed when the [SCENE FILE] menu → [GAMMA MODE SEL] → [HLG] is selected.

- The zebra pattern is not displayed when the [SYSTEM] menu → [COLOR SETTING] → [V-Log] is selected.

Top of the page