- Top
- Preparation
- Preparing the memory card
- Memory cards supported by the camera

# Memory cards supported by the camera

The following SD cards and microP2 cards can be used with the camera. (As of April 2020)

Type of the SD card | Recording capacity
--- | ---
SDHC memory card | 4 GB - 32 GB
SDXC memory card | 48 GB - 256 GB

Type of the microP2 card | Recording capacity
--- | ---
microP2 card A series | 32 GB, 64 GB
microP2 card B series | 64 GB

- Operation is not guaranteed for any memory cards other than the above.

- Panasonic memory cards are recommended.

- The following memory cards cannot be used because they do not comply with the SD standards.

  - A memory card with 4 GB or more without the SDHC logo

  - A memory card with 48 GB or more without the SDXC logo

- The camera does not support the CPS (Content Protection System) function of the microP2 card, so a microP2 card formatted with encryption with CPS password cannot be sued. When formatted with the camera, it can be used as a microP2 card that is not encrypted.

## Speed Class during shooting

The memory card to use differs depending on the recording mode and the recording format.

Use memory cards compatible with the Speed Class, UHS Speed Class, or Video Speed Class.

The recording may stop suddenly when a memory card not compatible with the required Speed Class is used.

- Speed Class, UHS Speed Class, and Video Speed Class are the speed specification regarding continuous writing. Check the display on the label and other information on the memory card.

#### When the recording mode is P2

microP2 cards can be used.

Recording bit rate or recording function | Speed Class | Example of card display
--- | --- | ---
All | microP2 card A series, microP2 card B series |

NOTE

- It is possible to record to SDXC memory cards in P2 format but is only for emergency recording and is not supported.

#### When the recording mode is MOV

SDXC memory cards and 64 GB microP2 cards can be used.

SDHC memory cards and 32 GB microP2 cards cannot be used.

Recording bit rate or recording function | Speed Class | Example of card display
--- | --- | ---
400 Mbps | Video Speed Class V60 or higher Or the microP2 card B series |
FHD VFR (23.98p)/SUPER SLOW ALL-I (Variable frame rate recording/super slow recording)
200 Mbps | Video Speed Class V30 or higher, UHS Speed Class 3 or higher Or the microP2 card A series, microP2 card B series |
150 Mbps
100 Mbps
FHD VFR/SUPER SLOW LongGOP (Variable frame rate recording/super slow recording)
FHD VFR (59.94p/50.00p/29.97p/25.00p) ALL-I (Variable frame rate recording)
50 Mbps | Video Speed Class V10 or higher, UHS Speed Class 1 or higher, Speed Class 10 or higher Or the microP2 card A series, microP2 card B series |

#### When the recording mode is AVCHD

SDHC memory cards, SDXC memory cards and microP2 cards can be used.

Recording bit rate or recording function | Speed Class | Example of card display
--- | --- | ---
All | Speed Class 4 or higher Or the microP2 card A series, microP2 card B series |

Top of the page