- Top
- Operation
- Menu settings
- [CAMERA] menu

# [CAMERA] menu

Sets the basic camera function.

This menu cannot be set when the thumbnail screen is displayed.

## [SW MODE]

### [LOW GAIN]

Sets the gain value to be assigned to the <L> position of the <GAIN> switch. (The negative value of gain can be set only when [SYSTEM] menu → [SHOOTING MODE] → [HIGH SENS.] is set.)

The items that can be set are as follows.

- When the [CAMERA] menu → [SW MODE] → [GAIN/ISO MODE] → [dB] is set

  - [−3dB]…[18dB]

  (Factory setting: [0dB])

- When the [CAMERA] menu → [SW MODE] → [GAIN/ISO MODE] → [ISO] is set

  - [ISO 400], [ISO 500], [ISO 640], [ISO 800], [ISO 1000], [ISO 1250], [ISO 1600], [ISO 2000], [ISO 2500], [ISO 3200], [ISO 4000], [ISO 5000], [ISO 6400], [ISO 8000], [ISO 10000], [ISO 12800]

  (Factory setting: [ISO 800])

### [MID GAIN]

Sets the gain value to be assigned to the <M> position of the <GAIN> switch.

The items that can be set are as follows.

- When the [CAMERA] menu → [SW MODE] → [GAIN/ISO MODE] → [dB] is set

  - [−3dB]…[18dB]

  (Factory setting: [6dB])

- When the [CAMERA] menu → [SW MODE] → [GAIN/ISO MODE] → [ISO] is set

  - [ISO 400], [ISO 500], [ISO 640], [ISO 800], [ISO 1000], [ISO 1250], [ISO 1600], [ISO 2000], [ISO 2500], [ISO 3200], [ISO 4000], [ISO 5000], [ISO 6400], [ISO 8000], [ISO 10000], [ISO 12800]

  (Factory setting: [ISO 1600])

### [HIGH GAIN]

Sets the gain value to be assigned to the <H> position of the <GAIN> switch.

The items that can be set are as follows.

- When the [CAMERA] menu → [SW MODE] → [GAIN/ISO MODE] → [dB] is set

  - [−3dB]…[18dB]

  (Factory setting: [12dB])

- When the [CAMERA] menu → [SW MODE] → [GAIN/ISO MODE] → [ISO] is set

  - [ISO 400], [ISO 500], [ISO 640], [ISO 800], [ISO 1000], [ISO 1250], [ISO 1600], [ISO 2000], [ISO 2500], [ISO 3200], [ISO 4000], [ISO 5000], [ISO 6400], [ISO 8000], [ISO 10000], [ISO 12800]

  (Factory setting: [ISO 3200])

### [SUPER GAIN]

Sets the super gain to be assigned to the USER button.

Toggles [24dB], [30dB], [36dB], and the normal gain in order each time the USER button is pressed or the USER button icon is touched when set to [ALL].

The items that can be set are as follows.

- [24dB], [30dB], [36dB], [ALL]

(Factory setting: [36dB])

NOTE

- This cannot be set when the [CAMERA] menu → [SW MODE] → [GAIN/ISO MODE] is set to [ISO].

### [GAIN/ISO MODE]

Switches the unit for gain value.

The items that can be set are as follows.

- [dB], [ISO]

(Factory setting: [dB])

NOTE

- The setting is fixed to [dB] when the [SYSTEM] menu → [COLOR SETTING] is set to [NORMAL].

### [O.I.S.]

Enables/disables the optical image stabilizer function.

If [O.I.S.] is assigned to the USER button, pressing the USER button switches [ON]/[OFF].

For details about optical image stabilizer, refer to “Optical image stabilizer function”.

[ON] | Enables the optical image stabilizer function.
[OFF] | Disables the optical image stabilizer function.

(Factory setting: [ON])

### [HYBRID O.I.S.]

Enables/disables the hybrid optical image stabilizer function.

For details about optical image stabilizer, refer to “Optical image stabilizer function”.

[ON] | Enables the hybrid optical image stabilizer function.
[OFF] | Disables the hybrid optical image stabilizer function.

(Factory setting: [ON])

### [O.I.S. MODE]

Switches the operation mode of the optical image stabilizer function.

Toggles [NORMAL], [PAN/TILT], and [STABLE] in order each time the USER button to which [O.I.S. MODE] is assigned is pressed or the USER button icon is touched.

[NORMAL] | Specifies the standard setting for a good balance of correction for large and small camera shake.
[PAN/TILT] | Specifies a setting appropriate for shooting that uses a lot of panning and tilting of the camera.
[STABLE] | Specifies a setting appropriate for fixing a composition to shoot a subject.

(Factory setting: [NORMAL])

### [ATW]

Assigns the auto tracking white balance function to the <WHITE BAL> switch.

The items that can be set are as follows.

- [Ach], [Bch], [PRE], [OFF]

(Factory setting: [OFF])

### [ATW SPEED]

Sets the control speed of the auto tracking white balance function.

The items that can be set are as follows.

- [FAST], [NORMAL], [SLOW]

(Factory setting: [NORMAL])

### [ATW TARGET R]

Finely adjusts the Rch output for convergence with the auto tracking white balance operation.

The items that can be set are as follows.

- [−10]…[10]

(Factory setting: [0])

### [ATW TARGET B]

Finely adjusts the Bch output for convergence with the auto tracking white balance operation.

The items that can be set are as follows.

- [−10]…[10]

(Factory setting: [0])

### [W.BAL PRESET]

Sets the color temperature to be assigned to the <PRST> position of the <WHITE BAL> switch.

The items that can be set are as follows.

- [3200K], [5600K], [VAR]

(Factory setting: [3200K])

### [W.BAL VAR]

Sets the value of [VAR] in [W.BAL PRESET].

The setting can also be operated by the multidial button.

Enabled when [W.BAL PRESET] is set to [VAR] and the <WHITE BAL> switch is at <PRST>.

The items that can be set are as follows.

- [2000K]…[15000K]

(Factory setting: [3200K])

### [H.ZOOM SPEED]

Sets the zoom speed of the handle zoom.

The items that can be set are as follows.

- [1]…[99]

(Factory setting: [50])

### [i.ZOOM]

Keeps the image quality while performing digital zoom.

[ON] | Enables the i.ZOOM function.
[OFF] | Disables the i.ZOOM function.

(Factory setting: [OFF])

### [MF ASSIST]

Sets whether to adjust the last focus automatically when in the manual focus mode.

If the image is largely out of focus, the focus may not be adjusted properly.

[ON] | Adjusts the last focus automatically.
[OFF] | Does not adjust the focus automatically.

(Factory setting: [OFF])

### [MACRO]

Enables/disables the focus macro function.

If functions are assigned to the USER buttons, [ON]/[OFF] can be switched using the USER button operations.

[ON] | Enables the focus macro function.
[OFF] | Disables the focus macro function.

(Factory setting: [OFF])

### [AF AREA WIDTH]

Adjusts the width of the area enable for the auto focus to match the size of the subject.

The items that can be set are as follows.

- [ON], [OFF]

(Factory setting: [OFF])

### [A.IRIS SPEED]

Sets the control speed of the auto iris level function.

The items that can be set are as follows.

- [FAST], [NORMAL], [SLOW]

(Factory setting: [NORMAL])

### [A.IRIS WINDOW]

Selects the auto iris detection window.

[NORMAL1] | Window that is around center of the screen.
[NORMAL2] | Window that is around bottom of the screen.
[CENTER] | Window that is a spot around center of the screen.

(Factory setting: [NORMAL1])

### [AREA MODE]

Assign the function that is performed within the area selected by touching the LCD monitor or pressing the <> button, <> button, <> button, or </> button while shooting.

[INHIBIT] | Disables assignment of functions.
[FOCUS] | Assigns the auto focus function.
[IRIS] | Assigns the auto iris function.
[Y GET] | Assigns the brightness display function.
[FOCUS/IRIS] | Assigns the simultaneous operation of the [FOCUS] and [IRIS].
[FOCUS/Y GET] | Assigns the simultaneous operation of the [FOCUS] and [Y GET].

(Factory setting: [INHIBIT])

### [IR REC]

Enables/disables the IR recording.

The items that can be set are as follows.

- [ON], [OFF]

(Factory setting: [OFF])

NOTE

- The setting is fixed to [OFF] when the [SYSTEM] menu → [COLOR SETTING] is set to [V-Log].

## [AUTO SW]

### [A.IRIS]

Enables/disables the auto iris control.

[ON] | Performs the auto iris control operation when in auto mode. The <IRIS> button does not work.
[OFF] | Does not perform the auto iris control operation when in auto mode. This activates the iris control selected with the <IRIS> button.

(Factory setting: [ON])

### [AGC]

Sets the auto gain control operations when [ON] is selected in [A.IRIS].

[ON] | Performs the operation of the [AGC] function that automatically adjusts camera gain when in auto mode.
[OFF] | Does not perform the operation of the [AGC] function that automatically adjusts camera gain when in auto mode.

(Factory setting: [ON])

NOTE

- The setting is fixed to [OFF] when the [CAMERA] menu → [SW MODE] → [GAIN/ISO MODE] is set to [ISO].

### [AGC LIMIT]

Sets the maximum gain value during [AGC] operation.

The items that can be set are as follows.

- [3dB], [6dB], [12dB], [18dB]

(Factory setting: [6dB])

NOTE

- This cannot be set when the [CAMERA] menu → [SW MODE] → [GAIN/ISO MODE] is set to [ISO].

### [AGC POINT]

Sets the F value to switch control from auto iris to [AGC] during [AGC] operation.

The items that can be set are as follows.

- [F4.0], [F5.6]

(Factory setting: [F4.0])

NOTE

- This cannot be set when the [CAMERA] menu → [SW MODE] → [GAIN/ISO MODE] is set to [ISO].

### [A.SHUTTER]

Sets the auto shutter control operations when [ON] is selected in [A.IRIS].

[ON] | Performs the operation of the auto shutter when in auto mode.
[OFF] | Does not perform the operation of the auto shutter when in auto mode.

(Factory setting: [ON])

### [A.SHUTTER LIMIT]

Sets the maximum shutter value during [A.SHUTTER] operation.

The items that can be set are as follows.

- [1/100], [1/120], [1/250]

(Factory setting: [1/250])

### [A.SHUTTER POINT]

Sets the F value to switch control from auto iris to [A.SHUTTER] during [A.SHUTTER] operation.

The items that can be set are as follows.

- [F8.0], [F9.6]

(Factory setting: [F8.0])

### [ATW]

Sets the operations of the auto tracking white balance function.

[ON] | Activates the auto tracking white balance function when in auto mode. The [ATW] function cannot be switched between enabled and disabled with the <WHITE BAL> switch or the USER buttons. However, if [ATW LOCK] is assigned to the USER button, the white balance value can be fixed with the USER button.
[OFF] | Does not perform the [ATW] function operation in auto mode. Performs the operation of the white balance function selected with the <WHITE BAL> switch.

(Factory setting: [ON])

### [AF]

Sets the operation of the auto focus.

[ON] | Performs the operation of the auto focus when in auto mode. The <FOCUS> switch does not work.
[OFF] | Does not perform the operation of the auto focus when in auto mode. Performs the operation of the focus selected with the <FOCUS> switch.

(Factory setting: [ON])

## [USER SW]

Sets the function to assign to the <USER 1> to <USER 7> buttons or the [USER8] to [USER12] button icons.

For details, refer to “Assigning function to the USER buttons”.

Following functions can be assigned to [USER1] to [USER12].

- [INHIBIT], [AWB], [DRS], [FBC], [ONE PUSH AF], [S.GAIN], [AREA], [AF AREA], [ATW], [ATW LOCK], [SPOTLIGHT], [BACKLIGHT], [A.IRIS LEVEL], [IRIS], [Y GET], [FOCUS MACRO], [O.I.S.], [O.I.S. MODE], [i.ZOOM], [D.ZOOM], [IR REC], [FAST ZOOM], [ADAPTIVE MATRIX], [PRE REC], [VFR], [SUPER SLOW], [REC CHECK], [BACKGR PAUSE], [DEL LAST CLIP], [SLOT SEL], [AUDIO CH1 LEVEL], [AUDIO CH2 LEVEL], [EXPAND], [PEAKING], [WFM], [ZEBRA], [LEVEL GAUGE], [LEVEL GAUGE SET], [LCD/VF HDR], [LCD/VF V-Log], [VF ON/OFF], [LCD/VF DETAIL], [AUDIO MON SEL], [AUDIO OUT], [MENU], [LOAD SETUP FILE], [LCD BACKLIGHT], [CARD READER MODE], [STREAMING START]

[USER1] | Sets the function to assign to the <USER 1> button. (Factory setting: [O.I.S.])
[USER2] | Sets the function to assign to the <USER 2> button. (Factory setting: [ZEBRA])
[USER3] | Sets the function to assign to the <USER 3> button. (Factory setting: [WFM])
[USER4] | Sets the function to assign to the <USER 4> button. (Factory setting: [A.IRIS LEVEL])
[USER5] | Sets the function to assign to the <USER 5> button. (Factory setting: [SLOT SEL])
[USER6] | Sets the function to assign to the <USER 6> button. (Factory setting: [IRIS])
[USER7] | Sets the function to assign to the <USER 7> button. (Factory setting: [AWB])
[USER8] | Sets the function to assign to the [USER8] button icon. (Factory setting: [IR REC])
[USER9] | Sets the function to assign to the [USER9] button icon. (Factory setting: [FOCUS MACRO])
[USER10] | Sets the function to assign to the [USER10] button icon. (Factory setting: [AREA])
[USER11] | Sets the function to assign to the [USER11] button icon. (Factory setting: [ATW LOCK])
[USER12] | Sets the function to assign to the [USER12] button icon. (Factory setting: [MENU])

Top of the page