- Top
- Shooting
- Multi manual function
- Adjusting the area size/area position of the area mode function

# Adjusting the area size/area position of the area mode function

Turn the multidial to display the [ AREA].

Press the multidial.

Turn the multidial to change the size of the area frame.

Press the <> button, <> button, <> button, or </> button to change the position of the area frame.

Press the multidial.

The setting is changed to the displayed size/position and exits.

The setting is changed and exits also by pressing the <EXIT> button.

NOTE

- [ AREA] is displayed when the area mode function is enabled.

Top of the page