- Top
- Shooting
- Image quality adjustment
- RB gain control function

# RB gain control function

This function makes settings to add or reduce the intensity of red and blue colors according to the position of the <WHITE BAL> switch.

The function works when the switch is at the <PRST> position or when automatic white balance is active. It does not work when auto tracking white balance is activated.

#### General settings

Use the camera with the factory settings.

#### Advanced settings

Set with the [SCENE FILE] menu → [RB GAIN CONTROL SETTING].

- When the <WHITE BAL> switch is at the <PRST> position

  [R GAIN AWB PRE]: Sets to add or reduce the intensity of the red color.

  [B GAIN AWB PRE]: Sets to add or reduce the intensity of the blue color.

- When the <WHITE BAL> switch is at the <A> position

  [R GAIN AWB A]: Sets to add or reduce the intensity of the red color.

  [B GAIN AWB A]: Sets to add or reduce the intensity of the blue color.

- When the <WHITE BAL> switch is at the <B> position

  [R GAIN AWB B]: Sets to add or reduce the intensity of the red color.

  [B GAIN AWB B]: Sets to add or reduce intensity of the blue color.

- When performing automatic white balance by setting the <WHITE BAL> switch to the <A> position

  [AWB A GAIN OFFSET]: Sets whether to keep or reset the values set for [R GAIN AWB A] and [B GAIN AWB A].

- When performing automatic white balance by setting the <WHITE BAL> switch to the <B> position

  [AWB B GAIN OFFSET]: Sets whether to keep the values set for [R GAIN AWB B] and [B GAIN AWB B] or reset them.

Top of the page