- Top
- Network Connection
- Network settings
- Wired LAN settings

# Wired LAN settings

These are the settings when using a wired LAN.

Select the [NETWORK] menu → [DEVICE SEL] → [LAN].

In the [NETWORK] menu → [LAN PROPERTY], set each item as necessary.

- For details about the setting items, refer to “Setting items in [LAN PROPERTY] when set to [LAN]”.

Close the menu or return to the level of the [NETWORK] menu.

Configure the settings of the wired LAN on your device such as a computer.

For more information, refer to the operating instructions or help for the connection device.

#### Setting items in [LAN PROPERTY] when set to [LAN]

[MAC ADDRESS] | MAC address of the wired LAN (cannot be changed)
[IPv4 SETTING] | [DHCP] | Setting the DHCP function [OFF]: Does not use DHCP. [CLIENT]: Acquires automatically with DHCP. [SERVER]: Enables the DHCP server function of the camera. (Factory setting: [OFF])
[IP ADDRESS] | IP address of the camera (Factory setting: [192.168.0.1])
[SUBNET MASK] | Subnet mask (Factory setting: [255.255.255.0])
[DEFAULT GATEWAY] | Default gateway (Factory setting: [192.168.0.254])
[PRIMARY DNS] | Primary DNS server setting (Factory setting: [0.0.0.0])
[SECONDARY DNS] | Secondary DNS server setting (Factory setting: [0.0.0.0])
[IPv6 SETTING] | [ENABLE/DISABLE] | IPv6 setting [ENABLE]: Uses IPv6. [DISABLE]: Does not use IPv6. (Factory setting: [DISABLE])
| [DHCP] | Setting the DHCP function [OFF]: Does not use DHCP. [CLIENT]: Acquires automatically with DHCP. (Factory setting: [OFF])
[IP ADDRESS] | IP address of the camera (Factory setting: [::])
[PREFIX LENGTH] | Prefix length settings of the subnet (Factory setting: [64])
[DEFAULT GATEWAY] | Default gateway (Factory setting: [::])
[PRIMARY DNS] | Primary DNS server (Factory setting: [::])
[SECONDARY DNS] | Secondary DNS server (Factory setting: [::])

NOTE

- Some items cannot be selected depending on the settings such as [DHCP].

- The startup time after turning on the power may be longer due to starting of the network.

- When changing the settings of [DEVICE SEL], the changes will not be reflected until the camera is restarted. Also, the setting screen termination may take some time due to the restart of the network service after the setting is changed.

- All of the IP address, subnet mask, and default gateway must be correctly set.

  For details, contact the network administrator.

- Set [0.0.0.0] or [::] when not using the default gateway or DNS.

  However, DNS cannot be disabled when [DHCP] is set to [CLIENT].

- Depending on the network environment, even if [DHCP] is set to [CLIENT], entry of the DNS value manually may be required. When invalid DNS value is entered in any other cases, the automatic assignment by DHCP will not operate properly.

- DHCP and DNS may not function properly depending on the network environment.

- The IP address cannot be automatically acquired depending on the connection timing with network devices if [LAN PROPERTY] → [IPv6 SETTING] → [DHCP] → [CLIENT] is set.

  In this case, reconnect the LAN cable or contact your network administrator.

Top of the page