- Top
- Description of Parts
- Camera
- Rear side

# Rear side

Following terminals, card slots, and card access lamps are inside each cover.

- <USB3.0 DEVICE> terminal

- <AV OUT> terminal

- <REMOTE> terminal

- <LAN> terminal

- <HDMI> terminal

- <DC IN 12V> terminal

1. <USB3.0 DEVICE> terminal

   Connect to a computer with the USB type C cable to transfer data.

2. Card 1 access lamp

   Indicates the access status for recording and playback of the memory card inserted in card slot 1.

   Whether or not to illuminate the lamp can be set in the menu.

3. Card slot 1

   A slot for the memory card.

4. Card slot 2

   A slot for the memory card.

5. Card 2 access lamp

   Indicates the access status for recording and playback of the memory card inserted in card slot 2.

   Whether or not to illuminate the lamp can be set in the menu.

6. Fan inlet

   Fan inlet for cooling fan. Do not block this while the camera is being used.

7. <SDI OUT> terminal

   A terminal to output SDI signal by connecting a monitor, etc.

8. <AV OUT> terminal

   This is the output terminal for the video and audio of an external monitor.

9. <TC IN/OUT> terminal

   Connects to an external equipment and output/input a time code.

   Inputs the standard time code when locking the time code with an external equipment.

   Input and output are set in the [RECORDING] menu → [TC/UB] → [TC IN/OUT SEL].

10. <REMOTE> terminal

    Connects the remote control unit (optional) to control some functions remotely.

11. <LAN> terminal

    Connects the LAN cable.

12. Eye sensor

    Screen is displayed on the viewfinder when an eye is brought close.

13. Viewfinder

14. <AUDIO INPUT 1> terminal (XLR, 3-pin)

    Connects an audio equipment or an external microphone.

15. Rear tally lamp

    Illuminates when the recording is started. Flashes when the battery level becomes low.

    Whether or not to illuminate the lamp can be set in the menu.

16. <HDMI> terminal

    A terminal to output video signal by connecting a monitor, etc.

17. Battery mounting section

    Mounts a battery.

18. Battery release button

    Used when removing the battery from the camera.

19. <DC IN 12V> terminal

    Connects the supplied AC adaptor and supplies an external power.

20. <AUDIO INPUT 2> terminal (XLR, 3-pin)

    Connects an audio equipment or an external microphone.

Top of the page