- Top
- Network Connection
- Connecting to the remote camera controller (AW-RP150G)
- Camera settings

# Camera settings

For the firmware of the camera, use Ver.4.00 or above.

For details about the camera setting, refer to “Connecting to the iPhone/iPad or Android terminal”. According to the shooting environment, select [ENABLE] or [ENABLE(HOLD)] for the [NETWORK] menu → [IP REMOTE] → [ENABLE/DISABLE].

In addition, set the following:

- Switch to auto mode with the <AUTO/MANUAL> switch. (<AUTO/MANUAL> switch)

- When [SUPER GAIN] is assigned to any of the USER button, clear the assignment. (Super gain)

The following settings are also recommended.

- Select the [CAMERA] menu → [SW MODE] → [ATW] → [OFF]. ([ATW])

- Select the [CAMERA] menu → [AUTO SW] → [ATW] → [OFF]. ([ATW])

- Select the [CAMERA] menu → [AUTO SW] → [A.SHUTTER] → [OFF]. ([A.SHUTTER])

- Select the [CAMERA] menu → [AUTO SW] → [AGC] → [OFF]. ([AGC])

NOTE

- When the [NETWORK] menu → [IP REMOTE] → [ENABLE/DISABLE] → [ENABLE(HOLD)] is selected, connection will be preserved even if disconnecting from the remote controller. Restrictions during connection such as the <THUMBNAIL> button not operating will remain.

  To end the connection status, select the [NETWORK] menu → [IP REMOTE] → [ENABLE/DISABLE] → [DISABLE].

- Network setting and setting related to IP remote for the camera will be reflected immediately after operating the menu. This may cause the connection between the camera and remote controller to end when changing settings.

Top of the page