- Top
- Shooting
- Multi manual function
- Adjusting the width of the auto focus area

# Adjusting the width of the auto focus area

Adjusts the width of the area that auto focus is enabled according to the size of the subject.

Press the USER button assigned to [AF AREA] or touch the USER button icon while the camera image screen is displayed.

[ AF AREA] is displayed in the camera image screen.

Turn the multidial to adjust the auto focus area frame.

Press the multidial.

The setting changes to the width displayed and exits.

Press the <EXIT> button to exit without changing the setting.

To release the setting, press the USER button to which [AF AREA] is assigned or touch the USER button icon.

To adjust the setting again, press the multidial when [ AF AREA] is displayed in yellow and perform Steps 2 to 3.

NOTE

- The width of the auto focus area frame can be adjusted even if the [CAMERA] menu → [SW MODE] → [AF AREA WIDTH] → [ON] is set and the menu is closed.

Top of the page