- Top
- Description of Parts
- Shooting and recording/playback functions section
- Shooting and recording/playback functions section (Recording unit)

# Shooting and recording/playback functions section (Recording unit)

1. <REC> button

   Recording is started by pressing the <REC> button. Recording is stopped by pressing this button again.

   Performs the same operation as the <VTR> button of the lens to be attached.

2. Card access lamp 1/card access lamp 2/card access lamp 3

   Indicates the access status of recording and playback of the memory card.

3. Card slot 1

   This is a card slot only for expressP2 card.

4. <USB DEVICE> terminal

   In the USB device mode, the camera can be connected to the computer by the USB type C cable to transfer data. In this case, recording playback operations and camera shooting are not possible.

5. Card slot 2/card slot 3

   These are card slots for microP2 card and SD card.

6. <REV ()> button

   It will perform fast-reverse playback when this is pressed during playback.

   It will playback from the start of the clip when this is pressed while paused.

7. <STOP ()> button

   Press this button to stop playback.

8. <FWD ()> button

   It will perform fast playback when this is pressed during playback.

   It will play back from the start of the next clip when this is pressed while paused during a playback.

9. <PLAY/PAUSE (/)> button

   Plays back a clip.

   Playback is paused when this is pressed during the playback.

10. <SDI OUT 2 CHARACTER> switch

    Controls the superimposing of characters into the video output from the <SDI OUT2> terminal.

    Controls the superimposing of characters into the video output from the <HDMI> terminal when the [VIDEO OUT/LCD/VF] menu → [HDMI OUT] → [SIGNAL SEL] → [SDI OUT2] is set.

    <ON>: Superimposes the character.

    <OFF>: Does not superimpose the character.

11. <USB2.0 HOST> terminal

    Can connect via wireless LAN when the wireless module (optional) compatible to camera is mounted.

12. <HDMI> terminal

    This is the output terminal for videos.

    Output signal can be switched with the [VIDEO OUT/LCD/VF] menu → [HDMI OUT] → [SIGNAL SEL].

    [SDI OUT1(2160p)]: Follows the setting of the output signal from the <SDI OUT1> terminal.

    [SDI OUT2]: Follows the setting of the output signal from the <SDI OUT2> terminal.

    Setting for superimposing of characters can be switched in the [VIDEO OUT/LCD/VF] menu → [HDMI OUT] → [SIGNAL SEL].

13. <LAN> terminal

    Connects the 1000BASE-T/100BASE-TX/10BASE-T LAN cable.

    Use Category 7 LAN cable.

14. <SDI OUT1> terminal

    This is the output terminal only for SDI.

    Select an output signal in the [VIDEO OUT/LCD/VF] menu → [SDI OUT1] → [OUT FORMAT].

    Superimposing of characters is set in the [VIDEO OUT/LCD/VF] menu → [SDI OUT1] → [SDI OUT CHAR].

15. <SDI OUT2> terminal

    This is the video output terminal for the monitor.

    Select an output signal in the [VIDEO OUT/LCD/VF] menu → [SDI OUT2] → [OUT FORMAT].

    Superimposing of characters can be set with the <SDI OUT 2 CHARACTER> switch independently of the <SDI OUT1> terminal.

    NOTE

    - Use 5C-FB or higher cable to connect to the <SDI OUT1>/<SDI OUT2> terminals.

Top of the page