- Top
- Operation
- Menu settings
- [THUMBNAIL] menu

# [THUMBNAIL] menu

Performs confirmation or deleting of the recording clip.

This menu can be set when the thumbnail screen is displayed.

## [PLAYBACK]

Sets the playback of recorded clips.

### [CLIP SEL]

Selects a clip to be displayed on the thumbnail screen.

It is always displayed in [ALL SLOT] when switched from the camera image screen to the thumbnail screen.

[ALL SLOT] | Displays all the clips recorded on every memory card in each card slot.
[SLOT1] | Displays only the clips recorded on the memory card in card slot 1.
[SLOT2] | Displays only the clips recorded on the memory card in card slot 2.
[SLOT3] | Displays only the clips recorded on the memory card in card slot 3.
[SAME FORMAT] | Displays only the clips recorded in the same format as the system format. Clips recorded in the same format means that each item of the [SYSTEM] menu → [FREQUENCY]/[FILE FORMAT]/[REC FORMAT]/[AUDIO SAMPLE RES.] matches the current setting status.

(Factory setting: [ALL SLOT])

### [RESUME PLAY]

Select if the playback is to start from the position the playback has stopped or not.

[ON] | Plays back from the position where playback has stopped.
[OFF] | Always starts the playback from the beginning of the clip.

(Factory setting: [OFF])

## [CLIP]

The clip can be protected or copied to a different memory card.

[PROTECT] | [SELECT] | Protect the clip so it is not mistakenly deleted. Select the clip to protect, and set the protect.
[DELETE] | [ALL] | Deletes all the clips displayed in the thumbnail screen. The clip that is not displayed in the thumbnail screen is not deleted.
[SELECT] | Select the clip to delete, and delete it.
[COPY] | [ALL] | Copies all clips to a different memory card.
[SELECT] | Selects the clip to copy, and copies the clip to a different memory card. Select [SLOT2→SLOT1] or [SLOT3→SLOT1] to copy a clip recorded spanning over card slot 2 and card slot 3 to the expressP2 card in the card slot 1 while recording in P2 format. An error occurs at the start of the copy process if [SLOT2→SLOT3] or [SLOT3→SLOT2] is selected.
[REPAIR] | Repairs a clip displaying caused by the sudden power loss, etc., during recording in P2 format.
[RE-CONNECT] | [SELECT] | While recording in P2 format, a clip recorded over multiple microP2 cards may not be recognized as a continuous clip, and may display . Restores as a continuous clip by selecting the clips to re-connect.
[INFORMATION] | Displays the detailed information of the clip.

NOTE

- Clips in P2 format cannot be protected.

- Clips in MOV format cannot be copied.

## [DISPLAY]

Sets the display of the thumbnail screen.

### [DATA]

Selects the content to be displayed in the time code display area.

[START TC] | Displays the time code value at the start of the recording.
[CLIP NAME] | Displays clip names.

(Factory setting: [START TC])

Top of the page