- Top
- Operation
- Menu settings
- [NETWORK] menu

# [NETWORK] menu

Specifies the network function settings.

## [DEVICE SEL]

Select the device that connects external equipment (computer, etc.) to the camera.

The camera may restart when the setting is changed.

[LAN] | Connects via a wired LAN.
[WLAN] | Connects via a wireless LAN.
[OFF] | Does not connect.

(Factory setting: [OFF])

## [NETWORK FUNC]

Selects the network function of the camera.

[STREAMING] | Enables the streaming function.
[NDI|HX] | Enables the NDI|HX function.
[OFF] | Disables the network function.

(Factory setting: [OFF])

NOTE

- When [NDI|HX] is selected, recording and thumbnail display are not possible.

## [IP REMOTE]

Perform settings for the IP remote. (remote control by the CX ROP app)

### [ENABLE/DISABLE]

Sets whether to enable the IP remote function.

The items that can be set are as follows.

- [ENABLE], [DISABLE]

(Factory setting: [DISABLE])

### [USER ACCOUNT]

Registers a new user account to use for authentication in the network function of the camera. (Maximum of ten accounts)

The character limit of the user account name and password is as follows.

- User account name: Maximum of 31 characters

- Password: Between 8 to 15 characters

### [ACCOUNT LIST]

Displays a list of registered user accounts.

Also, confirmation screen for whether to delete the registered user is displayed when a user is selected.

## [STREAMING]

Performs the settings for the streaming function.

### [STREAMING FORMAT]

Specifies the streaming format.

The items that can be set are as follows.

- When [FILE FORMAT] is set to [P2] or [MOV], and [REC FORMAT] is set to 1080/50p

  - [1920×1080-50fps 24M], [1920×1080-50fps 20M], [1920×1080-50fps 16M], [1280×720-50fps 14M], [1280×720-50fps 8M], [1280×720-50fps 3M], [640×360-25fps 4M], [640×360-25fps 1.5M], [640×360-25fps 0.7M], [320×180-25fps 4M], [320×180-25fps 1.5M], [320×180-25fps 0.5M]

  (Factory setting: [640×360-25fps 0.7M])

- When [FILE FORMAT] is set to [P2] or [MOV], and [REC FORMAT] is set to 1080/59.94p

  - [1920×1080-60fps 24M], [1920×1080-60fps 20M], [1920×1080-60fps 16M], [1280×720-60fps 14M], [1280×720-60fps 8M], [1280×720-60fps 3M], [640×360-30fps 4M], [640×360-30fps 1.5M], [640×360-30fps 0.7M], [320×180-30fps 4M], [320×180-30fps 1.5M], [320×180-30fps 0.5M]

  (Factory setting: [640×360-30fps 0.7M])

- When [FILE FORMAT] is set to [P2] or [MOV], and [REC FORMAT] is set to 1080/50i or 1080/25p

  - [1920×1080-25fps 14M], [1920×1080-25fps 6M], [1920×1080-25fps 1M], [1280×720-25fps 8M], [1280×720-25fps 2M], [1280×720-25fps 1M], [640×360-25fps 4M], [640×360-25fps 1.5M], [640×360-25fps 0.7M], [320×180-25fps 4M], [320×180-25fps 1.5M], [320×180-25fps 0.5M]

  (Factory setting: [640×360-25fps 0.7M])

- When [FILE FORMAT] is set to [P2] or [MOV], and [REC FORMAT] is set to 1080/59.94i or 1080/29.97p

  - [1920×1080-30fps 14M], [1920×1080-30fps 6M], [1920×1080-30fps 1M], [1280×720-30fps 8M], [1280×720-30fps 2M], [1280×720-30fps 1M], [640×360-30fps 4M], [640×360-30fps 1.5M], [640×360-30fps 0.7M], [320×180-30fps 4M], [320×180-30fps 1.5M], [320×180-30fps 0.5M]

  (Factory setting: [640×360-30fps 0.7M])

- When [FILE FORMAT] is set to [P2] or [MOV], and [REC FORMAT] is set to 1080/23.98p

  - [1920×1080-24fps 14M], [1920×1080-24fps 6M], [1920×1080-24fps 1M]

  (Factory setting: [1920×1080-24fps 1M])

- When [FILE FORMAT] is set to [P2], and [REC FORMAT] is set to 720/50p

  - [1280×720-50fps 14M], [1280×720-50fps 8M], [1280×720-50fps 3M], [640×360-25fps 4M], [640×360-25fps 1.5M], [640×360-25fps 0.7M], [320×180-25fps 4M], [320×180-25fps 1.5M], [320×180-25fps 0.5M]

  (Factory setting: [640×360-25fps 0.7M])

- When [FILE FORMAT] is set to [P2], and [REC FORMAT] is set to 720/59.94p

  - [1280×720-60fps 14M], [1280×720-60fps 8M], [1280×720-60fps 3M], [640×360-30fps 4M], [640×360-30fps 1.5M], [640×360-30fps 0.7M], [320×180-30fps 4M], [320×180-30fps 1.5M], [320×180-30fps 0.5M]

  (Factory setting: [640×360-30fps 0.7M])

NOTE

- Cannot be set when [REC FORMAT] is set to UHD.

### [START TRIGGER]

Sets whether to start streaming with operation of the camera or operation of the application software.

The items that can be set are as follows.

- [CAMERA], [RECEIVER], [RECEIVER(MULTICAST)]

(Factory setting: [RECEIVER])

### [CONNECTION INFO.]

Selects reference location for the transfer destination when starting a streaming with the operation of the camera from the camera memory or the SD card.

The items that can be set are as follows.

- [MEMORY], [SD CARD]

(Factory setting: [MEMORY])

### [DATA TYPE]

Displays the type of the setting data. (Cannot be changed)

[GENERAL] | General streaming settings
[P2CAST] | P2 Cast setting

### [RECEIVER URL]

Enter the destination URL in following format.

- rtmp://(server URL):(port number)/(path)/(stream key)

- rtmps://(server URL):(port number)/(path)/(stream key)

### [MULTICAST ADDRESS]

Sets the address when using the streaming with the multicast.

(Factory setting: [239.192.0.20])

### [MULTICAST PORT]

Sets the port number when using the streaming with the multicast.

(Factory setting: [37004])

### [LOAD (SD CARD)]

Loads the settings file from the memory card and reflects in the menu when [CONNECTION INFO.] is set to [MEMORY].

The items that can be selected are as follows.

- [YES], [NO]

### [SAVE (SD CARD)]

Encrypts and saves the information of the destination URL to the memory card.

The items that can be selected are as follows.

- [YES], [NO]

### [CLEAR (MEMORY)]

Clears the contents of the streaming setting set in the menu item.

The URL information set in P2 Cast is also cleared.

The items that can be selected are as follows.

- [YES], [NO]

### [START]

Starts streaming.

The items that can be set are as follows.

- [ON], [OFF]

(Factory setting: [OFF])

## [NDI|HX]

Performs settings related to NDI|HX.

### [ACTIVATION]

Displays whether the NDI|HX function is enabled. (Cannot be changed)

[--] | Not active.
[NDI|HX] | Active.

### [STREAMING FORMAT]

Specifies the streaming format.

The items that can be set are as follows.

- When [FILE FORMAT] is set to [P2] or [MOV], and [REC FORMAT] is set to 1080/50p

  - [1920×1080-50fps 24M], [1920×1080-50fps 16M], [1920×1080-50fps 10M], [1920×1080-50fps 8M], [1280×720-50fps 14M], [1280×720-50fps 10M], [1280×720-50fps 6M]

  (Factory setting: [1920×1080-50fps 10M])

- When [FILE FORMAT] is set to [P2] or [MOV], and [REC FORMAT] is set to 1080/59.94p

  - [1920×1080-60fps 24M], [1920×1080-60fps 16M], [1920×1080-60fps 10M], [1920×1080-60fps 8M], [1280×720-60fps 14M], [1280×720-60fps 10M], [1280×720-60fps 6M]

  (Factory setting: [1920×1080-60fps 10M])

- When [FILE FORMAT] is set to [P2] or [MOV], and [REC FORMAT] is set to 1080/50i or 1080/25p

  - [1920×1080-25fps 14M], [1920×1080-25fps 10M], [1920×1080-25fps 6M], [1280×720-25fps 8M], [1280×720-25fps 4M], [1280×720-25fps 2M]

  (Factory setting: [1920×1080-25fps 10M])

- When [FILE FORMAT] is set to [P2] or [MOV], and [REC FORMAT] is set to 1080/59.94i or 1080/29.97p

  - [1920×1080-30fps 14M], [1920×1080-30fps 10M], [1920×1080-30fps 6M], [1280×720-30fps 8M], [1280×720-30fps 4M], [1280×720-30fps 2M]

  (Factory setting: [1920×1080-30fps 10M])

- When [FILE FORMAT] is set to [P2], and [REC FORMAT] is set to 720/50p

  - [1280×720-50fps 14M], [1280×720-50fps 10M], [1280×720-50fps 6M]

  (Factory setting: [1280×720-50fps 10M])

- When [FILE FORMAT] is set to [P2], and [REC FORMAT] is set to 720/59.94p

  - [1280×720-60fps 14M], [1280×720-60fps 10M], [1280×720-60fps 6M]

  (Factory setting: [1280×720-60fps 10M])

NOTE

- Cannot be set when [REC FORMAT] is set to UHD or 1080/23.98p.

### [MULTICAST]

Enables/disables the multicast function.

The items that can be set are as follows.

- [ENABLE], [DISABLE]

(Factory setting: [DISABLE])

### [MULTICAST ADDRESS]

Sets the address when using the streaming with the multicast.

(Factory setting: [239.192.0.20])

### [MULTICAST PORT]

Sets the port number when using the streaming with the multicast.

(Factory setting: [37004])

### [CLEAR ACTIVATION]

Clears the activation license information that is saved.

The items that can be selected are as follows.

- [YES], [NO]

## [LAN PROPERTY]

Sets the wired LAN setting.

### [MAC ADDRESS]

Displays the MAC address for the wired LAN of the camera. (Cannot be changed)

### [IPv4 SETTING]

[DHCP] | Sets whether to use the automatic acquisition through DHCP or to use the DHCP server function of the camera. [OFF]: Does not use DHCP. [CLIENT]: Acquires automatically with DHCP. The address from 192.168.0.10 through 192.168.0.255 is automatically assigned when the IP address cannot be acquired automatically within one minute. [SERVER]: Enables the DHCP server function of the camera. (Factory setting: [OFF])
[IP ADDRESS] | Sets the IP address. Cannot be set when [LAN PROPERTY] → [IPv4 SETTING] → [DHCP] → [CLIENT] is selected. (Factory setting: [192.168.0.1])
[SUBNET MASK] | Sets the subnet mask. Cannot be set when [LAN PROPERTY] → [IPv4 SETTING] → [DHCP] → [CLIENT] is selected. (Factory setting: [255.255.255.0])
[DEFAULT GATEWAY] | Sets the default gateway. Cannot be set when [LAN PROPERTY] → [IPv4 SETTING] → [DHCP] → [CLIENT] is selected. (Factory setting: [192.168.0.254])
[PRIMARY DNS] | Sets the primary DNS server. (Factory setting: [0.0.0.0])
[SECONDARY DNS] | Sets the secondary DNS server. (Factory setting: [0.0.0.0])

### [IPv6 SETTING]

[ENABLE/DISABLE] | Sets whether to use IPv6. [ENABLE]: Uses IPv6. [DISABLE]: Does not use IPv6. (Factory setting: [DISABLE])
[DHCP] | Sets whether to use automatic acquisition via DHCP. [OFF]: Does not use DHCP. [CLIENT]: Acquires automatically with DHCP. (Factory setting: [OFF])
[IP ADDRESS] | Sets the IP address. (Factory setting: [::])
[PREFIX LENGTH] | Sets the prefix length of the subnet. (Factory setting: [64])
[DEFAULT GATEWAY] | Sets the default gateway. (Factory setting: [::])
[PRIMARY DNS] | Sets the primary DNS server. (Factory setting: [::])
[SECONDARY DNS] | Sets the secondary DNS server. (Factory setting: [::])

## [WLAN PROPERTY]

Performs settings related to the wireless LAN.

### [MAC ADDRESS]

Displays the wireless LAN MAC address of the camera. (Cannot be changed)

### [TYPE]

Sets the connection method to the wireless LAN.

[DIRECT] | It can connect directly without using a wireless access point to a device equipped with wireless LAN such as a tablet terminal.
[INFRA(SELECT)] | Connects to the wireless access point. The access point is selected from the list.
[INFRA(MANUAL)] | Connects to the wireless access point. Wireless access point is entered manually.

(Factory setting: [DIRECT])

### [SSID]

Enters or displays the network name of the camera (SSID). (32 characters or less)

(Factory setting: [AJ-CX4000])

### [BAND]

Switches between two communication methods ([2.4GHz] or [5GHz]) when the [NETWORK] menu → [WLAN PROPERTY] → [TYPE] → [DIRECT] is selected.

The items that can be set are as follows.

- [2.4GHz], [5GHz]

(Factory setting: [2.4GHz])

### [CHANNEL(2.4GHz)]

Sets the channel to be used when connected to the wireless LAN with following items set.

- The [NETWORK] menu → [WLAN PROPERTY] → [TYPE] → [DIRECT]

- The [NETWORK] menu → [WLAN PROPERTY] → [BAND] → [2.4GHz]

The items that can be set are as follows.

- [AUTO], [CH1], [CH6], [CH11]

(Factory setting: [AUTO])

### [CHANNEL(5GHz)]

Sets the channel to be used when connected to the wireless LAN with following items set.

- The [NETWORK] menu → [WLAN PROPERTY] → [TYPE] → [DIRECT]

- The [NETWORK] menu → [WLAN PROPERTY] → [BAND] → [5GHz]

The items that can be set are as follows.

- [AUTO], [CH36], [CH40], [CH44], [CH48], [CH100], [CH104], [CH108], [CH112], [CH116], [CH132], [CH136], [CH140], [CH149], [CH153], [CH157], [CH161], [CH165]

(Factory setting: [AUTO])

NOTE

- Some items may not be able to select depending on the used wireless module.

### [ENCRYPTION]

Sets the encryption method when the [NETWORK] menu → [WLAN PROPERTY] → [TYPE] → [INFRA(SELECT)]/[INFRA(MANUAL)] is selected.

The items that can be set are as follows.

- [WPA-TKIP], [WPA-AES], [WPA2-TKIP], [WPA2-AES], [NONE]

(Factory setting: [WPA2-AES])

NOTE

- The setting is fixed to [WPA2-AES] when the [NETWORK] menu → [WLAN PROPERTY] → [TYPE] → [DIRECT] is set.

### [ENCRYPT KEY]

Sets the encryption key. Set the key using a string of 8 to 63 characters or a hexadecimal number with 64 digits.

(Factory setting: [01234567890123456789abcdef])

### [IPv4 SETTING]

[DHCP] | Sets whether to use the automatic acquisition through DHCP or to use the DHCP server function of the camera. [OFF]: Does not use DHCP. [CLIENT]: Automatically acquired with the DHCP when connected by setting [WLAN PROPERTY] → [TYPE] → [INFRA(SELECT)]/[INFRA(MANUAL)]. [SERVER]: Enables the DHCP server function of the camera when connecting by setting [WLAN PROPERTY] → [TYPE] → [DIRECT]. (Factory setting: [OFF])
[IP ADDRESS] | Sets the IP address. Cannot be set when [WLAN PROPERTY] → [IPv4 SETTING] → [DHCP] → [CLIENT] is selected. (Factory setting: [192.168.0.1])
[SUBNET MASK] | Sets the subnet mask. Cannot be set when [WLAN PROPERTY] → [IPv4 SETTING] → [DHCP] → [CLIENT] is selected. (Factory setting: [255.255.255.0])
[DEFAULT GATEWAY] | Sets the default gateway. If you do not use default gateway, set to [0.0.0.0]. Cannot be set when [WLAN PROPERTY] → [IPv4 SETTING] → [DHCP] → [CLIENT] is selected. Disables the setting for the default gateway when [WLAN PROPERTY] → [TYPE] → [DIRECT] is selected. (Factory setting: [192.168.0.254])
[PRIMARY DNS] | Sets the primary DNS server. Disables the setting for the primary DNS server when [WLAN PROPERTY] → [TYPE] → [DIRECT] is selected. (Factory setting: [0.0.0.0])
[SECONDARY DNS] | Sets the secondary DNS server. Disables the setting for the secondary DNS server when [WLAN PROPERTY] → [TYPE] → [DIRECT] is selected. (Factory setting: [0.0.0.0])

## [INFORMATION]

### [STATUS]

Displays the status of the network function.

## [UTILITY]

Performs the various operations related to the network function.

### [NETWORK INITIALIZE]

Restores the network setting status to the factory settings.

### [EASY IP SETTING]

Sets the time to accept EASY IP Setup Software.

The items that can be set are as follows.

- [DISABLE], [20 MIN.], [UNLIMITED]

(Factory setting: [DISABLE])

NOTE

- This is fixed to [UNLIMITED] when [NDI|HX] is selected in [NETWORK FUNC].

### [EASY IP CAMERA TITLE]

Configure the individual device names to display in EASY IP Setup Software. (15 characters or less)

The camera title set here is also displayed as the individual device name in the NDI|HX compatible switcher.

(Factory setting: [AJ-CX4000])

Top of the page