- Top
- Playback
- Thumbnail operation
- Thumbnail screen

# Thumbnail screen

Press the <THUMBNAIL> button to display the thumbnail screen while displaying the camera image screen.

Press the <THUMBNAIL> button again to display the camera image screen.

The clip in the recording file format (P2 or MOV) selected in the [SYSTEM] menu → [FILE FORMAT] is displayed in the thumbnail screen.

Also, menu in the thumbnail screen can be operated by pressing the <MENU> button while the thumbnail screen is displayed.

[ALL SLOT]

[PROTECT]

1. Clip status display

   [ALL SLOT]: Displays all the clips recorded on every memory card in each card slot.

   Displays in [ALL SLOT] when switched from the camera image screen to the thumbnail screen.

   [SLOT1]: Displays only the clips recorded on the memory card in card slot 1.

   [SLOT2]: Displays only the clips recorded on the memory card in card slot 2.

   [SLOT3]: Displays only the clips recorded on the memory card in card slot 3.

   [SAME FORMAT]: Displays only the clips recorded in the same format as the system format.

   Clips recorded in the same format means that each item of the [SYSTEM] menu → [FREQUENCY]/[FILE FORMAT]/[REC FORMAT]/[AUDIO SAMPLE RES.] matches the current setting status.

   Following items are also displayed when set to the [SYSTEM] menu → [FILE FORMAT] → [P2].

   [SLOT1→SLOT2]: Displayed when copying from the memory card in card slot 1 to the memory card in card slot 2.

   [SLOT1→SLOT3]: Displayed when copying from the memory card in card slot 1 to the memory card in card slot 3.

   [SLOT2→SLOT1]: Displayed when copying from the memory card in card slot 2 to the memory card in card slot 1.

   [SLOT2→SLOT3]: Displayed when copying from the memory card in card slot 2 to the memory card in card slot 3.

   [SLOT3→SLOT1]: Displayed when copying from the memory card in card slot 3 to the memory card in card slot 1.

   [SLOT3→SLOT2]: Displayed when copying from the memory card in card slot 3 to the memory card in card slot 2.

2. Function display

   This is displayed during the operation of copy, delete, protect, etc.

3. Recording mode

   : Displayed when P2 is selected as the recording file format.

   : Displayed when MOV is selected as the recording file format.

   : Displayed when MOV is selected as the recording file format, and there is at least one P2 clip on any of the memory cards.

   : Displayed when P2 is selected as the recording file format, and there is at least one MOV clip on any of the memory cards.

4. Defective clip status

   : Displayed when P2 is selected as the recording file format and there is at least one defective P2 clip that may be repaired in the thumbnail screen.

   : Displayed when P2 is selected as the recording file format and there is at least one defective P2 clip that cannot be repaired in the thumbnail screen.

   (No display): There is no defective P2 clip in the thumbnail screen.

5. Media status display

   The card slot number of the memory card where the clip in the cursor position is recorded is displayed in yellow.

6. Connection status of the wireless LAN/wired LAN

   Displays the connection status of the wireless LAN or wired LAN.

   (No display): It is not connected via wired LAN or wireless LAN. It is set to the [NETWORK] menu → [DEVICE SEL] → [OFF].

   : It is set to the wired LAN, and ROP is not connected.

   : It is set to the wired LAN, and ROP is connected.

   : It is set to the wireless LAN, and ROP is not connected.

   : It is set to the wireless LAN, and ROP is connected.

7. Battery status display

   Displays the battery remaining capacity.

   Display unit is “V” (voltage display) or “%” (percentage display).

8. Scroll bar

   Indicates which part of the whole thumbnail is currently being viewed.

9. Clip that cannot be played back

   Displays when the clip cannot be played back in the camera such as standard violation.

10. Cursor

11. Page switching button

    Switches the page of the thumbnail screen.

    []: Moves to previous page

    []: Moves to next page

NOTE

- When P2 is selected as the recording file format, a clip recorded over multiple memory cards is displayed as one clip.

- MOV clip and P2 clip cannot be displayed in the thumbnail screen simultaneously.

## Display of the clips in the thumbnail screen

1. Thumbnail number

   Displays the thumbnail number in [0001] to [9999].

   Normally, the number assigned to the clip in the order of recording is displayed.

2. Resume play status

3. Number of recording pixels, system frequency

4. Recording file format, recording codec

5. Protection status of the clip

   This is displayed when the clip is protected.

6. Standard time code/clip name

   The first eight digits for the time code when starting shooting of a clip or the file name of the clip are displayed in alphanumeric.

   The information to display is set in the [THUMBNAIL] menu → [DISPLAY] → [DATA].

7. Delete selection status

8. Clip that cannot be played back

   This is displayed when the clip cannot be played back with the camera because the system frequency is different, etc.

9. Copy selection status

   This is displayed when the clip is selected.

10. Re-connection selection status

    This is displayed when the clip to be re-connected is selected.

11. Incomplete clip

    : This is displayed for a P2 clip when the clip is recorded over multiple memory cards, and any of those memory cards are not inserted.

12. Defective clip/unknown clip

    : This is displayed for a defective P2 clip that may be repaired.

    : This is displayed for a defective P2 clip that cannot be repaired.

    : This is displayed for a P2 clip with a different format for P2 standard.

## Display of clip information

Displays the information of the clip where the cursor is positioned.

Move the yellow cursor to the clip to display the clip information.

Select the [THUMBNAIL] menu → [CLIP] → [INFORMATION].

The clip information is displayed.

#### Clip information

[CLIP INFORMATION]

[START TC]

[START UB]

[DATE]

[TIME]

[DURATION]

[PIXEL/FREQ]

[CODEC]

[FRAME RATE]

[GAMMA]

1. Clip that cannot be played back

   This is displayed when the clip cannot be played back with the camera because the system frequency is different, etc.

2. Thumbnail number

3. Protect status of the clip/defective clip/unknown clip/incomplete clip

   : This is displayed when the clip is protected.

   : This is displayed for a defective P2 clip that may be repaired.

   : This is displayed for a defective P2 clip that cannot be repaired.

   : This is displayed for a P2 clip with a different format for P2 standard.

   : This is displayed for a P2 clip when the clip is recorded over multiple memory cards, and any of those memory cards are not inserted.

4. Thumbnail image

5. Clip name

6. [START TC]

   Displays the time code value at the start of the recording.

7. [START UB]

   Displays the user bits value at the start of the recording.

8. [DATE]

   Displays the date of the recording.

9. [TIME]

   Displays the time at the start of recording.

10. [DURATION]

    Displays the time length of the clip.

11. [PIXEL/FREQ]

    Displays the recording format of the clip.

12. [CODEC]/[CODEC/AUDIO]

    Displays the recording file format and the recording codec of the clip.

    Displays the number of bits of the audio of the clip when recording format is AVC-Intra 100/AVC-Intra 50.

13. [FRAME RATE]

    Displays the recording frame rate of the clip.

    This camera does not support variable frame rate recording function and this item is not displayed in clips recorded by this camera.

14. [GAMMA]

    Displays the gamma of the clip.

Top of the page