- Top
- Maintenance
- Warning system
- Warning list

# Warning list

NOTE

- “Reduced wireless audio reception” is not displayed when set to the [AUDIO] menu → [INPUT SETTINGS] → [WIRELESS WARN] → [OFF].

- Card access lamp does not flash even a warning occurs when set to the [OTHERS] menu → [LED] → [ACCESS LED] → [OFF].

1. System error

   Status display | Does not display.
   Warning lamp | Flashes four times per second.
   Tally lamp | Flashes four times per second.
   Card access lamp | All card access lamps flash four times per second in orange.
   Viewfinder | [SYSTEM ERROR] is displayed.
   Alarm | Sounds continuously.
   Warning content | Reference signal error or communication error.
   Recording or playback operation | The current operation will stop.
   Action to take | Consult your dealer.

2. Card removal error

   Status display | Does not display.
   Warning lamp | Flashes four times per second.
   Tally lamp | Flashes four times per second.
   Card access lamp | All card access lamps flash four times per second in orange.
   Viewfinder | [TURN POWER OFF] is displayed.
   Alarm | Sounds continuously.
   Warning content | An error occurred in the camera because the expressP2 card being accessed was removed.
   Recording or playback operation | The current operation will stop.
   Action to take | Follow the message to turn the power off once and turn the power on again. Ensure that there is no error in the clips on the ejected card, and repair the clips as necessary.

3. Battery end (low voltage input)

   Status display | Seven battery charge level bars flash.
   Warning lamp | Lights.
   Tally lamp | Flashes four times per second.
   Card access lamp | All card access lamps flash four times per second in orange.
   Viewfinder | The [BATT] lamp is illuminated if the viewfinder has the [BATT] lamp. [EMP] flashes in the battery charge level display. ([%] flashes for batteries with information about its remaining capacity.)
   Alarm | Sounds continuously.
   Warning content | The battery has run out.
   Recording or playback operation | The current operation will stop. The power is turned off in approximately five seconds.
   Action to take | Change the batteries.

4. High temperature error

   Status display | Does not display.
   Warning lamp | Flashes four times per second.
   Tally lamp | Flashes four times per second.
   Card access lamp | All card access lamps flash four times per second in orange.
   Viewfinder | [HIGH TEMPERATURE] is displayed.
   Alarm | Sounds continuously.
   Warning content | The internal temperature of the camera has risen exceeding the expectation.
   Recording or playback operation | The current operation will stop. The power is turned off in approximately five seconds.
   Action to take | Turn on the power again and confirm the recording by playing it back. If the problem persists, consult the dealer.

5. Card end

   Status display | Seven remaining memory card capacity level bars flash.
   Warning lamp | Lights.
   Tally lamp | Flashes four times per second.
   Card access lamp | All card access lamps flash four times per second in orange.
   Viewfinder | [END] is displayed in the remaining memory card capacity display.
   Alarm | Sounds continuously.
   Warning content | There is no more remaining memory card capacity.
   Recording or playback operation | Recording will stop.
   Action to take | Delete clips in the memory card or insert a new memory card.

6. Recording error

   Status display | Does not display.
   Warning lamp | Flashes four times per second.
   Tally lamp | Flashes four times per second.
   Card access lamp | All card access lamps flash four times per second in orange.
   Viewfinder | [REC WARNING] is displayed. [REC WARNING]/[<OVER MAX NUM. OF CLIPS>] is displayed when you try to record exceeding the limit for number of clips. [TEMPORARY PAUSE]/[IRREGULAR SIG] is displayed when the genlock reference signal is not correctly received.
   Alarm | Sounds four times per second.
   Warning content | This is a recording or recording circuit setting error.
   Recording or playback operation | Recording will stop. When the reference signal for genlock is not correctly received, pause the recording, and resume the recording when the signal returns to normal.
   Action to take | Start recording again. Or, turn the power off once and then start recording again. To record exceeding the maximum numbers of the clips, replace the memory card or delete unnecessary clips.

7. Card error

   Status display | Does not display.
   Warning lamp | Flashes four times per second when occurring during recording. It does not illuminate when it occurs during playback.
   Tally lamp | Flashes four times per second when occurring during recording. It does not illuminate when it occurs during playback.
   Card access lamp | All card access lamps flash four times per second in orange when occurring during recording.
   Viewfinder | Displays [CARD ERROR <SLOT 1>] (corresponding card slot number is displayed).
   Alarm | Sounds four times per second when occurring during recording. It does not sound when it occurs during playback.
   Warning content | A memory card error occurred during recording or playback.
   Recording or playback operation | The current operation will stop. The memory card with the error is write-protected after it is stopped.
   Action to take | Replace the memory card.

8. Reduced wireless audio reception

   Status display | Does not display.
   Warning lamp | Flashes four times per second. (When idle or during recording)
   Tally lamp | Flashes four times per second while recording is continued.
   Viewfinder | [WIRELESS RF] is displayed.
   Alarm | Sounds four times per second while recording is continued.
   Warning content | The error indicates poor wireless audio reception conditions.
   Recording or playback operation | The current operation will continue.
   Action to take | Check the microphone power supply and the reception status of the receiver.

9. Battery near end

   Status display | One battery charge level bar flashes.
   Warning lamp | Flashes once per second.
   Tally lamp | Flashes once per second.
   Viewfinder | The [BATT] lamp flashes once per second if the viewfinder has the [BATT] lamp. ([%] indication flashes if the battery has information of remaining capacity.)
   Alarm | Sounds four times per second.
   Warning content | The battery is about to run out.
   Recording or playback operation | The current operation will continue.
   Action to take | Change the batteries as needed.

10. Memory card recording near end

    Status display | One remaining memory card capacity level bar flashes.
    Warning lamp | Flashes once per second while recording is continued.
    Tally lamp | Flashes once per second while recording is continued.
    Viewfinder | The remaining memory card capacity indicator flashes.
    Alarm | Sounds once per second while recording is continued.
    Warning content | The remaining memory card capacity totals 2 minutes or less.
    Recording or playback operation | The current operation will continue.
    Action to take | Change the memory card or insert an additional card as needed.

Top of the page