- Top
- Maintenance
- Recording function that cannot be used simultaneously

# Recording function that cannot be used simultaneously

Depending on the recording function that is set, there are recording functions that cannot be used simultaneously.

- Meaning of the symbols used in the table are as follows.

  - ✓: Can be used simultaneously.

  - —: Cannot be used simultaneously.

| Recording function that is set
--- | ---
Recording function to additionally set | Pre-recording*1*2 | Relay recording | Simultaneous recording | Interval recording*3*4*5*6
Pre-recording*1*2 |  | ✓ | ✓ | —
Relay recording | ✓ |  | — | —
Simultaneous recording | ✓ | — |  | ✓
Interval recording*3*4*5*6 | — | — | ✓ |

Time code is fixed to free run.

The pre-recording is canceled once when three hours has passed without starting the recording.

Time code is fixed to recording run.

The time code is fixed to [NDF].

The [VIDEO OUT/LCD/VF] menu → [SDI OUT1]/[SDI OUT2]/[HDMI OUT] → [HDMI REC REMOTE] will not operate.

Cannot set simultaneously when recording format is set to AVC-Intra 200/AVC-Intra 100/AVC-Intra 50.

Top of the page