- Top
- Operation
- Menu settings
- [VIDEO OUT/LCD/VF] menu

# [VIDEO OUT/LCD/VF] menu

Configures the settings for the external output, the information to display in the LCD monitor or viewfinder and the output format.

## [SDI OUT1]

### [OUTPUT SW]

Enables/disables the output from the <SDI OUT1> terminal.

[ON] | Outputs the video.
[OFF] | Does not output the video.

(Factory setting: [ON])

### [OUT FORMAT]

Selects the signal to output from the <SDI OUT1> terminal. The item that can be selected varies depending on the setting of the [SYSTEM] menu → [FREQUENCY]/[FILE FORMAT]/[REC FORMAT].

[3840×2160p] | Outputs in 3840×2160p.
[1920×1080p] | Outputs in 1920×1080p.
[1920×1080i] | Outputs in 1920×1080i.
[1920×1080PsF] | Outputs in 1920×1080PsF.
[1280×720p] | Outputs in 1280×720p.

(Factory setting: [1920×1080i])

NOTE

- For the combinations that can be set, refer to “Format that can be output from the <SDI OUT1> terminal”.

### [3G-SDI OUT]

Sets the format of the 3G-SDI signal output from the <SDI OUT1> terminal.

Can be set when the 3G-SDI signal is output.

[LEVEL-A] | Selects the LEVEL-A method.
[LEVEL-B] | Selects the LEVEL-B DL method.

(Factory setting: [LEVEL-B])

### [SDI REC REMOTE]

Sets if the recording operation against the external equipment connected to the <SDI OUT1> terminal (such as recorder) is to be controlled or not.

[ON] | Controls the recording operation of the external equipment.
[OFF] | Does not control the recording operation of the external equipment.

(Factory setting: [OFF])

NOTE

- This cannot be set when set to the [RECORDING] menu → [REC FUNCTION] → [REC MODE] → [INTERVAL].

### [SDI OUT CHAR]

Sets whether to superimpose the character to the output from the <SDI OUT1> terminal.

[ON] | Superimposes.
[OFF] | Does not superimpose.

(Factory setting: [OFF])

### [SDI OUT ZEBRA]

Sets whether to superimpose the zebra signal to the output from the <SDI OUT1> terminal.

The setting of the zebra signal is in accordance with the following setting in the [VIDEO OUT/LCD/VF] menu → [EI ASSIST].

- [ZEBRA1 DETECT], [ZEBRA2 DETECT], [ZEBRA2]

[ON] | Superimposes.
[OFF] | Does not superimpose.

(Factory setting: [OFF])

### [SDI OUT HDR]

Sets the signal to output from the <SDI OUT1> terminal.

[SDR] | Outputs in the standard dynamic range.
[HDR] | Outputs in the high dynamic range.

(Factory setting: [HDR])

NOTE

- When the [SCENE FILE] menu → [GAMMA MODE SEL] is set to anything other than [HLG], the camera image is output in the standard dynamic range.

### [MARKER SW]

Marker is displayed in the output from the <SDI OUT1> terminal.

The items that can be set are as follows.

- [ON], [OFF]

(Factory setting: [OFF])

## [SDI OUT2]

### [OUTPUT SW]

Enables/disables the output from the <SDI OUT2> terminal.

[ON] | Outputs the video.
[OFF] | Does not output the video.

(Factory setting: [ON])

### [OUT FORMAT]

Sets the signal to output from the <SDI OUT2> terminal. The item that can be selected varies depending on the [SYSTEM] menu → [FREQUENCY]/[FILE FORMAT]/[REC FORMAT] setting.

[1920×1080p] | Outputs in 1920×1080p.
[1920×1080i] | Outputs in 1920×1080i.
[1920×1080PsF] | Outputs in 1920×1080PsF.
[1280×720p] | Outputs in 1280×720p.
[720×480i] | Outputs in 720×480i.
[720×576i] | Outputs in 720×576i.

(Factory setting: [1920×1080i])

NOTE

- For the combinations that can be set, refer to “Format that can be output from the <SDI OUT2> terminal”.

### [3G-SDI OUT]

Sets the format of the 3G-SDI signal output from the <SDI OUT2> terminal.

Can be set when the 3G-SDI signal is output.

[LEVEL-A] | Selects the LEVEL-A method.
[LEVEL-B] | Selects the LEVEL-B DL method.

(Factory setting: [LEVEL-B])

### [SD-SDI EDH]

Sets whether to superimpose EDH when output from the <SDI OUT2> terminal is the SD signal (480i and 576i).

[ON] | Superimposes.
[OFF] | Does not superimpose.

(Factory setting: [ON])

### [SDI REC REMOTE]

Sets if the recording operation against the external equipment connected to the <SDI OUT2> terminal (such as recorder) is to be controlled or not.

[ON] | Controls the recording operation of the external equipment.
[OFF] | Does not control the recording operation of the external equipment.

(Factory setting: [OFF])

NOTE

- This cannot be set when set to the [RECORDING] menu → [REC FUNCTION] → [REC MODE] → [INTERVAL].

### [SDI OUT ZEBRA]

Sets whether to superimpose the zebra signal to the output from the <SDI OUT2> terminal.

The setting of the zebra signal is in accordance with the following setting in the [VIDEO OUT/LCD/VF] menu → [EI ASSIST].

- [ZEBRA1 DETECT], [ZEBRA2 DETECT], [ZEBRA2]

[ON] | Superimposes.
[OFF] | Does not superimpose.

(Factory setting: [OFF])

### [SDI OUT HDR]

Sets the signal to output from the <SDI OUT2> terminal.

[SDR] | Outputs in the standard dynamic range.
[HDR] | Outputs in the high dynamic range.

(Factory setting: [HDR])

NOTE

- The setting is fixed to [SDR] when set to the following menu.

  - [VIDEO OUT/LCD/VF] menu → [SDI OUT2] → [OUT FORMAT] → [720×480i]

  - [VIDEO OUT/LCD/VF] menu → [SDI OUT2] → [OUT FORMAT] → [720×576i]

- The camera image is output in the standard dynamic range when the [SCENE FILE] menu → [GAMMA MODE SEL] is set to anything other than [HLG].

### [MARKER SW]

Marker is displayed in the output from the <SDI OUT2> terminal.

The items that can be set are as follows.

- [ON], [OFF]

(Factory setting: [OFF])

## [SDI OUTPUT ITEM]

Sets the character content to superimpose on the output signal of the <SDI OUT1>/<SDI OUT2>/<HDMI> terminals.

[MENU ONLY] | Superimposes only the menu when displaying the menu. Normally, nothing is superimposed.
[TC] | Superimposes the time code. Superimposes only the menu when displaying the menu.
[STATUS] | Displays the same contents as all the characters displayed in the viewfinder and the LCD monitor. Superimposes only the menu when displaying the menu.

(Factory setting: [MENU ONLY])

## [HDMI OUT]

### [SIGNAL SEL]

Sets the signal to output from the <HDMI> terminal.

The items that can be set are as follows.

- [SDI OUT1(2160p)], [SDI OUT2]

(Factory setting: [SDI OUT2])

NOTE

- [SDI OUT1(2160p)] can be selected only when [OUT FORMAT] of [SDI OUT1] is set to [3840×2160p].

  This is fixed to [SDI OUT2] when [OUT FORMAT] of [SDI OUT1] is set to anything other than [3840×2160p].

### [HDMI TC OUT]

Sets if the time code information is output or not in the output from the <HDMI> terminal.

The items that can be set are as follows.

- [ON], [OFF]

(Factory setting: [OFF])

### [HDMI REC REMOTE]

Sets if the recording operation against the external equipment connected to the <HDMI> terminal (such as recorder) is to be controlled or not. This can be set when [HDMI TC OUT] in [HDMI OUT] is enabled.

[ON] | Controls the recording operation of the external equipment.
[OFF] | Does not control the recording operation of the external equipment.

(Factory setting: [OFF])

NOTE

- This cannot be set when set to the [RECORDING] menu → [REC FUNCTION] → [REC MODE] → [INTERVAL].

## [SD DOWNCON MODE]

Sets the mode of the SD down converter output signal from the <SDI OUT2>/<HDMI OUT> terminal.

[SIDE CROP] | Outputs an equal top and bottom width.
[LETTER BOX] | Outputs an equal right and left width.
[SQUEEZE] | Outputs by compressing in the horizontal direction to fit the screen.

(Factory setting: [LETTER BOX])

## [VF COLOR]

Selects whether to display viewfinder images in color or in black and white.

[ON] | Displays in color.
[OFF] | Displays in black and white. The playback image, thumbnail screen, and menu display will be kept in color.

(Factory setting: [ON])

## [LCD]

### [BRIGHTNESS]

Adjusts the brightness of the LCD monitor.

The items that can be set are as follows.

- [−15]…[15]

(Factory setting: [0])

### [COLOR LEVEL]

Adjusts the color level of the LCD monitor.

The items that can be set are as follows.

- [−15]…[15]

(Factory setting: [0])

### [CONTRAST]

Adjusts the contrast of the LCD monitor.

The items that can be set are as follows.

- [−30]…[30]

(Factory setting: [0])

### [BACK LIGHT]

Adjusts the brightness of the LCD monitor backlight. [0] is the standard brightness.

The items that can be set are as follows.

- [−1], [0], [1], [2]

(Factory setting: [0])

### [SELF SHOOT]

Sets the display of the LCD monitor when mirror shooting is performed.

[NORMAL] | Does not invert the left and right sides.
[MIRROR] | Inverts the left and right sides.

(Factory setting: [MIRROR])

## [LCD/VF HDR]

Sets the output image from the LCD monitor and viewfinder.

[SDR] | Outputs in the standard dynamic range.
[HDR] | Outputs in the high dynamic range.

(Factory setting: [HDR])

NOTE

- When the [SCENE FILE] menu → [GAMMA MODE SEL] is set to anything other than [HLG], the camera image is output in the standard dynamic range.

## [INDICATOR]

Selects the indicator to display in the output image.

### [INDICATOR SW]

Selects the status display method.

[ON] | Status is displayed constantly.
[OFF] | Normally, status is not displayed. This is displayed when the mode check screen is displayed by pressing the <MARKER SEL>/<MODE CHECK> switch toward the <MCK> side.

(Factory setting: [ON])

### [TC]

Displays/hides the time code, user bits, and counter.

The items that can be set are as follows.

- [ON], [OFF]

(Factory setting: [OFF])

### [TC ON COLOR BAR]

Selects whether to display the time code, user bits, and counter when color bar is output.

The items that can be set are as follows.

- [ON], [OFF]

(Factory setting: [OFF])

### [REC STATUS]

Sets whether to display [REC] during recording.

[ON] | [REC] is displayed.
[OFF] | [REC] is not displayed. However, [REC] is displayed when set to the [OTHERS] menu → [LED] → [REC TALLY] → [CHAR].

(Factory setting: [OFF])

### [REC MEDIA]

Displays/hides the setting status of the memory card format to record.

The items that can be set are as follows.

- [ON], [OFF]

(Factory setting: [ON])

### [SLOT STATUS]

Displays/hides the status of the card slot and remaining memory card capacity.

The items that can be set are as follows.

- [ON], [OFF]

(Factory setting: [ON])

### [2 SLOTS FUNC.]

Displays/hides the setting in the [RECORDING] menu → [2 SLOTS FUNC.].

The items that can be set are as follows.

- [ON], [OFF]

(Factory setting: [ON])

### [STREAMING]

Displays/hides the streaming status.

The items that can be set are as follows.

- [ON], [OFF]

(Factory setting: [ON])

### [NETWORK]

Displays/hides the wireless LAN and wired LAN connection status.

The items that can be set are as follows.

- [ON], [OFF]

(Factory setting: [ON])

### [BATTERY REMAIN]

Displays/hides the remaining battery level.

The items that can be set are as follows.

- [ON], [OFF]

(Factory setting: [ON])

### [REC FORMAT]

Displays/hides the recording format settings.

The items that can be set are as follows.

- [ON], [OFF]

(Factory setting: [ON])

### [CLIP NAME]

Displays/hides the clip file name to be recorded. Up to eight characters from the beginning of the file name are displayed.

The items that can be set are as follows.

- [ON], [OFF]

(Factory setting: [ON])

### [BONDING DEVICE]

Displays/hides the status of the device acquired from the bonding device.

This is not displayed when the device status cannot be acquired from the bonding device even if [ON] is selected.

The items that can be set are as follows.

- [ON], [OFF]

(Factory setting: [ON])

### [REC REMOTE]

Displays/hides the remote control status of the external equipment connected to the <SDI OUT1>/<SDI OUT2>/<HDMI> terminals.

The items that can be set are as follows.

- [ON], [OFF]

(Factory setting: [ON])

### [REC MODE]

Displays/hides the status of the interval recording.

The items that can be set are as follows.

- [ON], [OFF]

(Factory setting: [ON])

### [FBC]

Displays/hides the operation status of the flash band compensation function.

The items that can be set are as follows.

- [ON], [OFF]

(Factory setting: [ON])

### [HDR/DRS]

Displays/hides the operation status of the high dynamic range recording function or the dynamic range stretcher function.

The items that can be set are as follows.

- [ON], [OFF]

(Factory setting: [ON])

### [CAC]

Displays/hides the operation status of the chromatic aberration compensation function.

The items that can be set are as follows.

- [ON], [OFF]

(Factory setting: [ON])

### [GAMMA MODE]

Displays/hides the gamma mode.

The items that can be set are as follows.

- [ON], [OFF]

(Factory setting: [ON])

### [SCENE FILE]

Displays/hides scene file name.

The items that can be set are as follows.

- [ON], [OFF]

(Factory setting: [ON])

### [AUDIO LEVEL METER]

Displays/hides the audio level meter.

The items that can be set are as follows.

- [ON], [OFF]

(Factory setting: [ON])

### [GAIN]

Displays/hides the gain value and the digital super gain value.

The items that can be set are as follows.

- [ON], [OFF]

(Factory setting: [ON])

### [SHUTTER]

Displays/hides the shutter speed.

The items that can be set are as follows.

- [ON], [OFF]

(Factory setting: [ON])

### [IRIS]

Displays/hides the F value, operation status of the super iris, and the operation status of the super black.

[IRIS] | Displays only the F value.
[S+IRIS] | Displays all.
[S] | Displays only the operation status of the super iris and operation status of the super black.
[OFF] | Does not display.

(Factory setting: [S+IRIS])

NOTE

- The display of the F value and the display of the iris override are linked. The F value is displayed while changing the iris override even when set to [S] or [OFF].

### [ZOOM/FOCUS]

Switches the unit of zoom and focus values.

[NUMBER] | Displays the zoom and focus in the position value between [000]/[00] and [999]/[99].
[mm/feet] | Displays the zoom in units of millimeters and the focus in units of feet.
[mm/m] | Displays the zoom in units of millimeters and the focus in units of meters.
[OFF] | Does not display either the zoom or focus.

(Factory setting: [NUMBER])

### [FILTER]

Displays/hides the positions of the ND filter and the CC filter.

The items that can be set are as follows.

- [ON], [OFF]

(Factory setting: [ON])

### [WHITE BALANCE]

Displays/hides the color temperature.

The items that can be set are as follows.

- [ON], [OFF]

(Factory setting: [ON])

### [DATE/TIME]

Displays/hides the date and time.

Display order of the year, month, and date follows the setting in the [OTHERS] menu → [CLOCK] → [DATE FORMAT].

[OFF] | Does not display the date and time.
[DATE] | Displays only the date.
[TIME] | Displays only the time.
[DATE&TIME] | Displays the date and time.

(Factory setting: [OFF])

### [SHOOTING MODE]

Displays/hides high-sensitivity mode.

The items that can be set are as follows.

- [ON], [OFF]

(Factory setting: [ON])

### [EXTENDER]

Displays/hides the display whether lens extender function is active.

The items that can be set are as follows.

- [ON], [OFF]

(Factory setting: [ON])

### [D.ZOOM]

Displays/hides the digital zoom ratio.

The items that can be set are as follows.

- [ON], [OFF]

(Factory setting: [ON])

### [PLAYBACK STATUS]

Displays/hides the playback status.

The items that can be set are as follows.

- [ON], [OFF]

(Factory setting: [ON])

## [MODE CHECK INDICATOR]

### [STATUS]

Sets whether to display the STATUS screen when the <MARKER SEL>/<MODE CHECK> switch is pushed to the <MCK> side.

The items that can be set are as follows.

- [ON], [OFF]

(Factory setting: [ON])

### [!LED]

Sets whether to display the !LED screen when the <MARKER SEL>/<MODE CHECK> switch is pushed to the <MCK> side.

The cause for the viewfinder lamp is illuminated is displayed by [!] with black and white inverted.

The items that can be set are as follows.

- [ON], [OFF]

(Factory setting: [ON])

### [FUNCTION]

Sets whether to display the FUNCTION screen when the <MARKER SEL>/<MODE CHECK> switch is pushed to the <MCK> side.

The items that can be set are as follows.

- [ON], [OFF]

(Factory setting: [ON])

### [AUDIO]

Sets whether to display the AUDIO screen when the <MARKER SEL>/<MODE CHECK> switch is pushed to the <MCK> side.

The items that can be set are as follows.

- [ON], [OFF]

(Factory setting: [ON])

### [CAC]

Sets whether to display the CAC screen when the <MARKER SEL>/<MODE CHECK> switch is pushed to the <MCK> side.

The items that can be set are as follows.

- [ON], [OFF]

(Factory setting: [ON])

### [USER SW STATUS]

Selects whether to display the SWITCH screen when the <MARKER SEL>/<MODE CHECK> switch is pushed to the <MCK> side.

The items that can be set are as follows.

- [ON], [OFF]

(Factory setting: [ON])

### [NETWORK]

Selects whether to display the NETWORK screen when the <MARKER SEL>/<MODE CHECK> switch is pushed to the <MCK> side.

The items that can be set are as follows.

- [ON], [OFF]

(Factory setting: [ON])

## [SDI OUT1 MARKER]

### [CENTER MARKER]

Switch the type of the center marker.

[1] | + (large)
[2] | Open center (large)
[3] | + (small)
[4] | Open center (small)
[OFF] | Does not display.

(Factory setting: [1])

### [SAFETY MARKER]

Selects the type of frame for the safety zone marker.

[1] | Box
[2] | Corners
[OFF] | Does not display.

(Factory setting: [2])

### [SAFETY AREA]

Sets the size of the safety zone marker.

It can be set in 1% steps with the ratio of length to width constant.

The items that can be set are as follows.

- [80%]…[100%]

(Factory setting: [90%])

### [FRAME MARKER]

Sets the aspect ratio of the frame marker. The frame marker is not displayed when [OFF] is selected.

The items that can be set are as follows.

- [4:3], [13:9], [14:9], [1.85:1], [2.35:1], [OFF]

(Factory setting: [OFF])

### [FRAME COLOR]

Sets the color of the frame marker.

The items that can be set are as follows.

- [WHITE], [BLACK], [RED], [GREEN], [BLUE], [YELLOW]

(Factory setting: [WHITE])

## [SDI OUT2 MARKER]

### [CENTER MARKER]

Switch the type of the center marker.

[1] | + (large)
[2] | Open center (large)
[3] | + (small)
[4] | Open center (small)
[OFF] | Does not display.

(Factory setting: [1])

### [SAFETY MARKER]

Selects the type of frame for the safety zone marker.

[1] | Box
[2] | Corners
[OFF] | Does not display.

(Factory setting: [2])

### [SAFETY AREA]

Sets the size of the safety zone marker.

It can be set in 1% steps with the ratio of length to width constant.

The items that can be set are as follows.

- [80%]…[100%]

(Factory setting: [90%])

### [FRAME MARKER]

Sets the aspect ratio of the frame marker. The frame marker is not displayed when [OFF] is selected.

The items that can be set are as follows.

- [4:3], [13:9], [14:9], [1.85:1], [2.35:1], [OFF]

(Factory setting: [OFF])

### [FRAME COLOR]

Sets the color of the frame marker.

The items that can be set are as follows.

- [WHITE], [BLACK], [RED], [GREEN], [BLUE], [YELLOW]

(Factory setting: [WHITE])

## [LCD/VF MARKER]

### [TABLE]

Selects the setting table of the marker select function. Check or set the details of [A]/[B] at subsequent settings.

The items that can be set are as follows.

- [A], [B]

(Factory setting: [A])

### [CENTER MARKER]

Switch the type of the center marker.

[1] | + (large)
[2] | Open center (large)
[3] | + (small)
[4] | Open center (small)
[OFF] | Does not display.

(Factory setting: [1])

### [SAFETY MARKER]

Selects the type of frame for the safety zone marker.

[1] | Box
[2] | Corners
[OFF] | Does not display.

(Factory setting: [2])

### [SAFETY AREA]

Sets the size of the safety zone marker.

It can be set in 1% steps with the ratio of length to width constant.

The items that can be set are as follows.

- [80%]…[100%]

(Factory setting: [90%])

### [FRAME MARKER]

Sets the aspect ratio of the frame marker. The frame marker is not displayed when [OFF] is selected.

The items that can be set are as follows.

- [4:3], [13:9], [14:9], [1.85:1], [2.35:1], [OFF]

(Factory setting: [OFF])

### [FRAME LEVEL]

Sets the level for outside of the frame marker.

[0] | Equivalent to when signal is off (blanking status).
[1]…[14] | Becomes brighter as the number becomes higher.
[15] | Becomes same brightness as the center area.

(Factory setting: [15])

### [FRAME COLOR]

Sets the color of the frame marker.

The items that can be set are as follows.

- [WHITE], [BLACK], [RED], [GREEN], [BLUE], [YELLOW]

(Factory setting: [WHITE])

## [FOCUS ASSIST]

### [FOCUS ASSIST SELECT]

Sets the focus assist method when the USER button assigned with [FOCUS ASSIST] is operated.

[EXPAND] | Sets the enlarged display.
[PEAKING] | Sets the peaking display.
[SQUARES] | Sets the focus square display.
[EXPAND+PEAKING] | Displays in the combination of [EXPAND] and [PEAKING].
[EXPAND+SQUARES] | Displays in the combination of [EXPAND] and [SQUARES].

(Factory setting: [EXPAND])

### [EXPAND MODE]

Sets the enlargement display function mode.

[10SEC] | Disables the enlarged display function after ten seconds have elapsed.
[HOLD] | Enables the enlarged display function until the <FOCUS ASSIST> button or the USER button assigned with [EXPAND] is pressed.
[UNTIL REC] | Enables the enlarged display function until recording starts.

(Factory setting: [10SEC])

### [EXPAND VALUE]

Adjusts the enlargement factor of the enlarged display function.

The items that can be set are as follows.

- [×2], [×3], [×4]

(Factory setting: [×2])

### [PEAKING LEVEL]

Sets the intensity of the peaking display.

The items that can be set are as follows.

- [LOW], [MID], [HIGH]

(Factory setting: [MID])

### [PEAKING COLOR]

Sets the color of the peaking display.

The items that can be set are as follows.

- [RED], [GREEN], [WHITE]

(Factory setting: [RED])

### [BLACK & WHITE]

Enables/disables the monochrome display.

[ON] | Enables the monochrome display.
[OFF] | Disables the monochrome display.
[DURING PEAKING] | Enables the monochrome display while the peaking display is enabled.

(Factory setting: [OFF])

### [DETAIL]

Sets the intensity of the contour for the video to make it easier to focus.

The items that can be set are as follows.

- [ON], [OFF]

(Factory setting: [ON])

### [DETAIL LEVEL]

Sets the intensity of the contours.

The items that can be set are as follows.

- [−3]…[3]

(Factory setting: [0])

### [DETAIL FREQ.]

Adjusts the frequency of the contour highlights.

The items that can be set are as follows.

- [HIGH], [LOW]

(Factory setting: [LOW])

## [EI ASSIST]

### [ZEBRA1 DETECT]

Sets the detection level of zebra pattern 1.

The items that can be set are as follows.

- [0%]…[109%]

(Factory setting: [80%])

### [ZEBRA2 DETECT]

Sets the detection level of zebra pattern 2.

The items that can be set are as follows.

- [0%]…[109%]

(Factory setting: [100%])

### [ZEBRA2]

Enables/disables zebra pattern 2 and selects [SPOT].

The items that can be set are as follows.

- [ON], [SPOT], [OFF]

(Factory setting: [OFF])

### [LOW LIGHT LEVEL]

Sets the amount of the light entering the camera to be the reference to display [LOW LIGHT].

The items that can be set are as follows.

- [OFF], [10%], [15%], [20%], [25%], [30%], [35%]

(Factory setting: [35%])

### [WFM MODE]

Sets the display of the waveform monitor. Displaying of the waveform and the vector can be switched.

[WAVE] | Displays the waveform.
[VECTOR] | Displays the vector.
[WAVE/VECTOR] | Displays the waveform and the vector. The display switches in the order of waveform, vector, and no display every time the USER button assigned with [WFM] is pressed.

(Factory setting: [WAVE])

### [WFM TRANSPARENCE]

Sets the transmittance of the waveform monitor.

The items that can be set are as follows.

- [0%], [25%], [50%]

(Factory setting: [25%])

## [!LED]

### [GAIN(0dB)]

Sets whether to illuminate the [!] lamp on the viewfinder when the gain is anything other than 0 dB.

The items that can be set are as follows.

- [ON], [OFF]

(Factory setting: [ON])

### [DS.GAIN]

Sets whether to illuminate the [!] lamp on the viewfinder when [DS.GAIN] (incremental gain) is working.

The items that can be set are as follows.

- [ON], [OFF]

(Factory setting: [OFF])

### [SHUTTER]

Sets whether to illuminate the [!] lamp on the viewfinder when the electronic shutter is working.

The items that can be set are as follows.

- [ON], [OFF]

(Factory setting: [ON])

### [WHITE PRESET]

Sets whether to illuminate the [!] lamp on the viewfinder when the <WHITE BAL> switch is set to <PRST>.

The items that can be set are as follows.

- [ON], [OFF]

(Factory setting: [OFF])

### [EXTENDER]

Sets whether to illuminate the [!] lamp on the viewfinder when the lens extender is working.

The items that can be set are as follows.

- [ON], [OFF]

(Factory setting: [ON])

### [B.GAMMA]

Sets whether to illuminate the [!] lamp on the viewfinder when the black gamma is working.

The items that can be set are as follows.

- [ON], [OFF]

(Factory setting: [OFF])

### [MATRIX]

Sets whether to illuminate the [!] lamp on the viewfinder when the color correction table for linear matrix is selected.

The items that can be set are as follows.

- [ON], [OFF]

(Factory setting: [OFF])

### [COLOR CORRECTION]

Sets whether to illuminate the [!] lamp on the viewfinder when the <GAIN> switch matches the setting in the [SCENE FILE] menu → [COLOR CORRECTION], and the 16-axis independent color correction is set.

The items that can be set are as follows.

- [ON], [OFF]

(Factory setting: [OFF])

### [FILTER]

Sets whether to illuminate the [!] lamp on the viewfinder for any setting combination other than the <CC FILTER> dial set to<A> (<3200 K>) and the <ND FILTER> dial set to <1> (<CLEAR>).

The items that can be set are as follows.

- [ON], [OFF]

(Factory setting: [OFF])

### [ATW]

Sets whether to illuminate the [!] lamp on the viewfinder when the automatic tracking white balance function is working.

The items that can be set are as follows.

- [ON], [OFF]

(Factory setting: [OFF])

Top of the page