- Top
- Shooting
- Assigning function to the USER buttons
- Selectable functions

# Selectable functions

Item name | Description
--- | ---
[INHIBIT] | Disables assignment of functions.
[DRS] | Assigns the dynamic range stretcher function. This function expands the dynamic range by compressing the image level in high-luminosity areas and stretching the image level in low-luminosity areas. The compression level can be varied in the [SCENE FILE] menu → [DRS EFFECT DEPTH]. A slight difference in coloring might occur by enabling/disabling the dynamic range stretcher function. When the dynamic range stretcher function is enabled, the knee function or the black gamma function are not activated.
[FBC]* | Enables/disables the flash band compensation function.
[S.GAIN]* | Assigns the super gain function. Automatic white balance does not function while the super gain function is enabled.
[ATW]* | Assigns the auto tracking white balance function.
[ATW LOCK]* | Fixes the white balance value when pressing this item while the auto tracking white balance function is activated. Resumes the auto tracking white balance function when pressing again.
[Y GET]* | Assigns the function for displaying the luminance level of the image at the position indicated by the square marker displayed near the center.
[D.ZOOM]* | Assigns the digital zoom function. Zooms in on the field angle by 2x, 3x and 4x vertically and horizontally.
[DS.GAIN]* | Assigns the digital super gain function. The digital super gain function is activated only during shooting in 59.94p, 59.94i, 50p, and 50i. While the function is activated, the shutter becomes [OFF]. Video at the instant that the digital super gain function is enabled/disabled, becomes discontinuous.
[S.IRIS]* | Assigns the super iris function. This is enabled when performing backlight compensation.
[I.OVR]* | Assigns the iris override function. To change the target value in auto iris mode, set to this mode and press the jog dial button. Turn the jog dial button to the left or right to change the target value. [+]/[++]/[−]/[−−] is displayed on the iris override display area on the viewfinder screen. Stop turning the jog dial button at the position to change the target value and press the jog dial button to apply the new target value setting. The reference value is returned when this mode is canceled or the power is turned off. [+]: Opens aperture by about 0.5. [++]: Opens aperture by about 1. [−]: Closes aperture by about 0.5. [−−]: Closes aperture by about 1. No display: Reference value.
[S.BLK]* | Assigns the super black function. This is the function for lowering the black level to the pedestal level or below.
[B.GAMMA]* | Assigns the black gamma function. This function enhances the black tones. Regardless of the value set by selecting the [SCENE FILE] menu → [LOW SETTING]/[MID SETTING]/[HIGH SETTING] → [BLACK GAMMA], [BLACK GAMMA]: [6] and [B.GAMMA RANGE]: [3] are set.
[FOCUS ASSIST]* | Displays/hides the focus assist display. Select the type of display in the [VIDEO OUT/LCD/VF] menu → [FOCUS ASSIST] → [FOCUS ASSIST SELECT].
[C.TEMP]* | Assigns the function for switching to the mode for changing the color temperature by the jog dial button. This is effective for intentionally varying the color temperature after white balance has been performed. To change the color temperature, press the USER button assigned with this function, and then press the jog dial button. The color temperature indicator in the viewfinder screen flashes in reverse to indicate that the mode is entered for changing the color temperature. While the indicator is flashing, turn the jog dial button to change the color temperature. At this time, the setting value of the position (<PRST>/<A>/<B>) where the <WHITE BAL> switch is currently set is also changed.
[ADAPTIVE MATRIX] | Enables/disables the function to control the linear matrix in accordance with the shooting condition.
[PRE REC] | Assigns the function for enabling/disabling the pre-recording.
[REC CHECK] | Assigns the function to automatically play back the last approximately three seconds of the previously shot clip.
[DEL LAST CLIP] | Assigns the function to delete the clip last shot.
[SLOT SEL] | Assigns the function for switching the card slot to record to when memory cards are inserted to card slot 2 and card slot 3.
[REC SW] | Assigns the function of the <REC> button.
[WFM]* | Assigns the function for displaying the waveform or vector in the viewfinder and LCD monitor. Select the waveform display in the [VIDEO OUT/LCD/VF] menu → [EI ASSIST] → [WFM MODE].
[LCD/VF HDR] | Assigns the function that switches output of the viewfinder and LCD monitor to high dynamic range/standard dynamic range. Enabled only when set to the [SCENE FILE] menu → [GAMMA MODE SEL] → [HLG].
[LCD/VF DETAIL] | Assigns function to adjust the intensity for the contour of the video in the viewfinder or LCD monitor to make it easier to focus.
[VF COLOR] | Assigns the function for switching the viewfinder screen to color display/monochrome display. This is interlocked with the setting value in the [VIDEO OUT/LCD/VF] menu → [VF COLOR].
[INDICATOR SW] | Assigns the function for enabling/disabling the status display.
[LOAD SETUP FILE] | Assigns the function to display the list of setup files saved in the SD card. This does not function in the thumbnail screen.
[LCD BACKLIGHT] | Assigns the function for switching the brightness of the LCD monitor. Every time the USER button is pressed, it is toggled in the order of [−1], [0], [1], and [2].
[CARD READER MODE]* | Assigns the function for enabling/disabling the card reader mode function (USB mass storage function).
[STREAMING START]* | Assigns the function for starting or stopping streaming from the camera. This is interlocked with the setting value in the [NETWORK] menu → [STREAMING] → [START].

The function also turns off when the camera is turned off.

Note, however, that the [C.TEMP] color temperature is held after it is altered.

Top of the page