- Top
- Specification
- Specifications
- Streaming

# Streaming

Video compression format | H.264/MPEG-4 AVC Main Profile H.264/MPEG-4 AVC High Profile
Video resolution | 1920×1080 (FHD), 1280×720 (HD), 640×360, 320×180
Streaming method | Unicast, Multicast
Frame rate | When the [SYSTEM] menu → [FREQUENCY] → [59.94Hz] is set 24 fps, 30 fps, 60 fps When the [SYSTEM] menu → [FREQUENCY] → [50.00Hz] is set 25 fps, 50 fps
Bit rate | 24 Mbps, 20 Mbps, 16 Mbps, 14 Mbps, 8 Mbps, 6 Mbps, 4 Mbps, 3 Mbps, 2 Mbps, 1.5 Mbps, 1 Mbps, 0.7 Mbps
Audio compression format | AAC-LC: 48 kHz/16 bit 2ch
Supported protocol | RTSP/RTP/RTMP/RTMPS

Top of the page