- Top
- Maintenance
- Warning system
- Alert

# Alert

Screen display | Description | Behavior and cause
--- | --- | ---
Camera image screen
[SIMUL REC WARNING <SLOT 2>]/[SIMUL REC WARNING <SLOT 3>] | An error has occurred in one of the memory cards during simultaneous recording. | A message is displayed for approximately five seconds. Recording to the other memory card will continue.
[SIMUL REC WARNING <SLOT 2>]/[SIMUL REC WARNING <SLOT 3>] | Recording has been attempted while the number of clips has exceeded the limit on one of the memory cards during simultaneous recording. | A message is displayed for approximately five seconds. Recording to the other memory card will continue. [SIMUL REC WARNING <SLOT 2>] [<OVER MAX NUM. OF CLIPS>]/[SIMUL REC WARNING <SLOT 3>] [<OVER MAX NUM. OF CLIPS>] is displayed in the message display area of the STATUS screen for the mode check. Replace the memory card or delete unnecessary clips.
[FAN STOPPED] | The fan has stopped. | A message is displayed. The current operation will continue. Stop the use immediately when the fan has stopped and alert is displayed, and consult the dealer. If the fan has stopped, temperature of the camera will rise. Therefore, do not use the camera for a long period of time. Use the tripod, etc., and do not touch the camera directly.
[Non-supported card. <SLOT 1>] [Insert expressP2 card.] | Card other than expressP2 card is inserted in the card slot 1. | A message is displayed for approximately five seconds. Insert an expressP2 card.
[ENCRYPTED CARD <SLOT 1>]/[ENCRYPTED CARD <SLOT 2>]/ [ENCRYPTED CARD <SLOT 3>] | P2 card formatted with encryption with CPS (Content Protection System) password is inserted. | A message is displayed for approximately five seconds. The camera does not support the CPS function of the P2 card. Insert a P2 card that is not formatted with encryption with CPS password. Formatting P2 card, which was formatted with encryption with CPS password, in the camera will enable P2 card to be used as unencrypted card.
[REINSERT OR CHECK CARD <SLOT 1>]/[REINSERT OR CHECK CARD <SLOT 2>]/[REINSERT OR CHECK CARD <SLOT 3>] | The memory card cannot be recognized properly because a recording medium which is not supported has been inserted or there is dirt on the terminal of the memory card. | A message is displayed for approximately five seconds. Check the memory card that is inserted. Insert the memory card again if displayed when inserting a memory card.
[FORMAT ERROR CARD <SLOT 1>]/[FORMAT ERROR CARD <SLOT 2>]/[FORMAT ERROR CARD <SLOT 3>] | A memory card with management information out of specifications has been inserted. | A message is displayed for approximately five seconds. Insert a memory card that can record.
[NOT SDXC CARD <SLOT 2>]/[NOT SDXC CARD <SLOT 3>] | A SDHC memory card that cannot record the MOV format data or a 32 GB microP2 card is inserted when [FILE FORMAT] is set to MOV format. | A message is displayed for approximately five seconds. Insert a SDXC memory card or 64 GB microP2 card.
[INCOMPATIBLE CARD <SLOT 2>]/[INCOMPATIBLE CARD <SLOT 3>] | A memory card that may not be able to record due to slow writing speed has been inserted. | A message is displayed for approximately five seconds. The current operation will continue. Use a memory card with sufficient writing speed.
[DIR NG CARD <SLOT 1>]/[DIR NG CARD <SLOT 2>]/[DIR NG CARD <SLOT 3>] | A P2 card with inappropriate directory placement is inserted when [FILE FORMAT] is set to P2 format. | A message is displayed for approximately five seconds. The current operation will continue. Take a backup of the memory card immediately, and use it again after formatting.
[RUN DOWN CARD <SLOT 1>]/[RUN DOWN CARD <SLOT 2>]/[RUN DOWN CARD <SLOT 3>] | A P2 card exceeding the specified number of overwrites is inserted. | A message is displayed for approximately five seconds. The current operation will continue. Replace the P2 card.
[SD CARD <SLOT 2>]/[SD CARD <SLOT 3>] | SD card is inserted when [FILE FORMAT] is set to P2 format. | A message is displayed for approximately five seconds. The current operation will continue. Recording to a P2 card is recommended.
[SLOT1 CANNOT REC] [microP2/SD SELECTED] | A memory card is inserted in card slot 1 when the [RECORDING] menu → [REC MEDIA] → [microP2/SD] is set. | A message is displayed for approximately five seconds. Set to the [RECORDING] menu → [REC MEDIA] → [expressP2] when recording on the memory card inserted in card slot 1.
[SLOT2/3 CANNOT REC] [expressP2 SELECTED] | A memory card is inserted in card slot 2 or card slot 3 when the [RECORDING] menu → [REC MEDIA] → [expressP2] is set. | A message is displayed for approximately five seconds. Set to the [RECORDING] menu → [REC MEDIA] → [microP2/SD] when recording on the memory card inserted in card slot 2 or card slot 3.
[BACKUP BATT EMPTY] | Voltage lowering of the backup battery for internal clock was detected when the power is set to < > (ON). | A message is displayed for approximately five seconds. The current operation will continue. Set the date/time again after charging the built-in battery.

Top of the page