- Top
- Preparation
- Power supply
- Attaching and setting the battery

# Attaching and setting the battery

## Using Anton/Bauer batteries

Release lever

Anton/Bauer battery

Mount the Anton/Bauer battery.

Insert the battery terminal and slide in the direction of the arrow.

Set the battery type.

Select the type of the battery in the [OTHERS] menu → [BATTERY] → [ONBOARD BATTERY] → [BATTERY SEL].

NOTE

- When removing the battery, keep the release lever of the battery holder completely down, slide the battery in the opposite direction of when you mounted it.

## Using V-mount type batteries

Mount the V-mount type battery plate. As shown in the figure, insert and slide in the direction of the arrow.

Release lever

Mount the V-mount type battery plate.

Slide in the direction of the arrow.

Set the battery type.

- Set the type of the battery in the [OTHERS] menu → [BATTERY] → [ONBOARD BATTERY] → [BATTERY SEL].

NOTE

- Contact your dealer for information about the V-mount type battery plate.

- When the V-mount type battery plate is used, % (percent) is not displayed even if batteries with a battery level indicator function are used.

- When removing the plate, keep the release lever of the battery holder completely down, slide the plate in the opposite direction of when you mounted it.

- When using a battery that is not in the [BATTERY SEL], set to [other], and set [FULL VOLT]/[NEAR END VOLT]/[END VOLT] according to the characteristics of the battery.

Top of the page